Table of Contents

Program Version:EnergyPlus, Version 25.1.0-68a4a7c774, YMD=2025.05.15 15:06

Tabular Output Report in Format: HTML

Building: US+SF+CZ6A+oilfurnace+crawlspace+IECC_2024_gahp

Environment: ANNUAL ** Rochester International Arpt MN USA TMY3 WMO#=726440

Simulation Timestamp: 2025-05-15 15:06:31

Table of Contents

Report: Annual Building Utility Performance Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Values gathered over 8760.00 hours
Site and Source Energy

| Total Energy [kBtu] | Energy Per Total Building Area [kBtu/ft2] | Energy Per Conditioned Building Area [kBtu/ft2]
Total Site Energy | 78456.25 | 15.22 | 33.01
Net Site Energy | 78456.25 | 15.22 | 33.01
Total Source Energy | 170933.62 | 33.16 | 71.91
Net Source Energy | 170933.62 | 33.16 | 71.91

Site to Source Energy Conversion Factors

| Site=>Source Conversion Factor
Electricity | 3.167
Natural Gas | 1.084
District Cooling | 1.056
District Heating Water | 3.613
District Heating Steam | 1.200
Gasoline | 1.050
Diesel | 1.050
Coal | 1.050
Fuel Oil No 1 | 1.050
Fuel Oil No 2 | 1.050
Propane | 1.050
Other Fuel 1 | 1.000
Other Fuel 2 | 1.000

Building Area

| Area [ft2]
Total Building Area | 5154.23
Net Conditioned Building Area | 2377.10
Unconditioned Building Area | 2777.13

End Uses

| Electricity [kBtu] | Natural Gas [kBtu] | Gasoline [kBtu] | Diesel [kBtu] | Coal [kBtu] | Fuel Oil No 1 [kBtu] | Fuel Oil No 2 [kBtu] | Propane [kBtu] | Other Fuel 1 [kBtu] | Other Fuel 2 [kBtu] | District Cooling [kBtu] | District Heating Water [kBtu] | District Heating Steam [kBtu] | Water [gal]
Heating | 0.00 | 23051.97 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | 5319.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | 3542.90 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 721.78 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 26605.68 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 5100.70 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 169.41 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 13944.29 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14862.19
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total End Uses | 41459.99 | 23051.97 | 0.00 | 0.00 | 0.00 | 0.00 | 13944.29 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14862.19

Note: Natural gas appears to be the principal heating source based on energy usage.
End Uses By Subcategory

| Subcategory | Electricity [kBtu] | Natural Gas [kBtu] | Gasoline [kBtu] | Diesel [kBtu] | Coal [kBtu] | Fuel Oil No 1 [kBtu] | Fuel Oil No 2 [kBtu] | Propane [kBtu] | Other Fuel 1 [kBtu] | Other Fuel 2 [kBtu] | District Cooling [kBtu] | District Heating Water [kBtu] | District Heating Steam [kBtu] | Water [gal]
Heating | General | 0.00 | 23051.97 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Boiler Parasitic | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | General | 5319.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | General | 3542.90 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | Exterior-Lights | 646.70 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Garage-Lights | 75.08 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | dishwasher | 703.03 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| refrigerator | 2283.13 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| clotheswasher | 359.04 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_dryer | 2845.15 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_range | 2062.62 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| television | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_mels | 11465.79 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| IECC_adj | 6886.92 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Ventilation | 2991.03 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| General | 2109.67 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | General | 169.41 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Domestic Hot Water | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14862.19
| Water Heater | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 13944.29 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

End Uses By Space Type

| Space Type | Electricity [kBtu] | Natural Gas [kBtu] | Gasoline [kBtu] | Diesel [kBtu] | Coal [kBtu] | Fuel Oil No 1 [kBtu] | Fuel Oil No 2 [kBtu] | Propane [kBtu] | Other Fuel 1 [kBtu] | Other Fuel 2 [kBtu] | District Cooling [kBtu] | District Heating Water [kBtu] | District Heating Steam [kBtu] | Water [gal]
Heating | Unassigned | 0.00 | 23051.97 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | Unassigned | 5319.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | GENERAL | 3542.90 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | Unassigned | 721.78 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | GENERAL | 26605.68 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Unassigned | 5100.70 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | Unassigned | 169.41 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 13944.29 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14862.19
Refrigeration | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | Unassigned | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Normalized Metrics
Utility Use Per Conditioned Floor Area

| Electricity Intensity [kBtu/ft2] | Natural Gas Intensity [kBtu/ft2] | Gasoline Intensity [kBtu/ft2] | Diesel Intensity [kBtu/ft2] | Coal Intensity [kBtu/ft2] | Fuel Oil No 1 Intensity [kBtu/ft2] | Fuel Oil No 2 Intensity [kBtu/ft2] | Propane Intensity [kBtu/ft2] | Other Fuel 1 Intensity [kBtu/ft2] | Other Fuel 2 Intensity [kBtu/ft2] | District Cooling Intensity [kBtu/ft2] | District Heating Water Intensity [kBtu/ft2] | District Heating Steam Intensity [kBtu/ft2] | Water Intensity [gal/ft2]
Lighting | 1.79 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
HVAC | 4.45 | 9.70 | 0.00 | 0.00 | 0.00 | 0.00 | 5.87 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 6.25
Other | 11.19 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total | 17.44 | 9.70 | 0.00 | 0.00 | 0.00 | 0.00 | 5.87 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 6.25

Utility Use Per Total Floor Area

| Electricity Intensity [kBtu/ft2] | Natural Gas Intensity [kBtu/ft2] | Gasoline Intensity [kBtu/ft2] | Diesel Intensity [kBtu/ft2] | Coal Intensity [kBtu/ft2] | Fuel Oil No 1 Intensity [kBtu/ft2] | Fuel Oil No 2 Intensity [kBtu/ft2] | Propane Intensity [kBtu/ft2] | Other Fuel 1 Intensity [kBtu/ft2] | Other Fuel 2 Intensity [kBtu/ft2] | District Cooling Intensity [kBtu/ft2] | District Heating Water Intensity [kBtu/ft2] | District Heating Steam Intensity [kBtu/ft2] | Water Intensity [gal/ft2]
Lighting | 0.83 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |
HVAC | 2.05 | 4.47 | 0.00 | 0.00 | 0.00 | 0.00 | 2.71 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |
Other | 5.16 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |
Total | 8.04 | 4.47 | 0.00 | 0.00 | 0.00 | 0.00 | 2.71 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 |

Electric Loads Satisfied

| Electricity [kBtu] | Percent Electricity [%]
Fuel-Fired Power Generation | 0.000 | 0.00
High Temperature Geothermal* | 0.000 | 0.00
Photovoltaic Power | 0.000 | 0.00
Wind Power | 0.000 | 0.00
Power Conversion | 0.000 | 0.00
Net Decrease in On-Site Storage | 0.000 | 0.00
Total On-Site Electric Sources | 0.000 | 0.00
Electricity Coming From Utility | 41459.987 | 100.00
Surplus Electricity Going To Utility | 0.000 | 0.00
Net Electricity From Utility | 41459.987 | 100.00
Total On-Site and Utility Electric Sources | 41459.987 | 100.00
Total Electricity End Uses | 41459.987 | 100.00

On-Site Thermal Sources

| Heat [kBtu] | Percent Heat [%]
Water-Side Heat Recovery | 0.00 | 0.00
Air to Air Heat Recovery for Cooling | 142.92 | 1.20
Air to Air Heat Recovery for Heating | 11721.71 | 98.80
High-Temperature Geothermal* | 0.00 | 0.00
Solar Water Thermal | 0.00 | 0.00
Solar Air Thermal | 0.00 | 0.00
Total On-Site Thermal Sources | 11864.63 | 100.00

Water Source Summary

| Water [gal] | Percent Water [%]
Rainwater Collection | 0.00 | 0.00
Condensate Collection | 0.00 | 0.00
Groundwater Well | 0.00 | 0.00
Total On Site Water Sources | 0.00 | 0.00
- | - | -
Initial Storage | 0.00 | 0.00
Final Storage | 0.00 | 0.00
Change in Storage | 0.00 | 0.00
- | - | -
Water Supplied by Utility | 14862.19 | 100.00
- | - | -
Total On Site, Change in Storage, and Utility Water Sources | 14862.19 | 100.00
Total Water End Uses | 14862.19 | 100.00

Setpoint Not Met Criteria

| Degrees [deltaF]
Tolerance for Zone Heating Setpoint Not Met Time | 0.36
Tolerance for Zone Cooling Setpoint Not Met Time | 0.36

Comfort and Setpoint Not Met Summary

| Facility [Hours]
Time Setpoint Not Met During Occupied Heating | 0.00
Time Setpoint Not Met During Occupied Cooling | 0.00
Time Not Comfortable Based on Simple ASHRAE 55-2004 | 1416.17

Note 1: An asterisk (*) indicates that the feature is not yet implemented.

Table of Contents

Top
Annual Building Utility Performance Summary
Input Verification and Results Summary
Demand End Use Components Summary
Source Energy End Use Components Summary
Component Sizing Summary
Surface Shadowing Summary
Adaptive Comfort Summary
Initialization Summary
Annual Heat Emissions Summary
Annual Thermal Resilience Summary
Climatic Data Summary
Envelope Summary
Shading Summary
Lighting Summary
Equipment Summary
HVAC Sizing Summary
Coil Sizing Details
System Summary
HVAC Topology
Outdoor Air Summary
Outdoor Air Details
Object Count Summary
Energy Meters
Sensible Heat Gain Summary
Standard 62.1 Summary
LEED Summary
Annual CO2 Resilience Summary
Annual Visual Resilience Summary

FANSPLIT

| CENTRAL SYSTEM_UNIT1 |

COILLOADS

| MAIN DX HEATING COIL_UNIT1 | SUPP HEATING COIL_UNIT1 | DX COOLING COIL_UNIT1 |

HEATING AND COOLING LOADS

| LIVING_UNIT1 | GARAGE1 | ATTIC_UNIT1 | CRAWLSPACE_UNIT1 |

WATER HEATER: LOADS

| WATER HEATER_UNIT1 |

Table of Contents

Report: Input Verification and Results Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

General

| Value
Program Version and Build | EnergyPlus, Version 25.1.0-68a4a7c774, YMD=2025.05.15 15:06
RunPeriod | ANNUAL
Weather File | Rochester International Arpt MN USA TMY3 WMO#=726440
Latitude [deg] | 43.90
Longitude [deg] | -92.5
Elevation [ft] | 1305.84
Time Zone | -6.0
North Axis Angle [deg] | 0.00
Rotation for Appendix G [deg] | 0.00
Hours Simulated [hrs] | 8760.00

ENVELOPE
Window-Wall Ratio

| Total | North (315 to 45 deg) | East (45 to 135 deg) | South (135 to 225 deg) | West (225 to 315 deg)
Gross Wall Area [ft2] | 3178.51 | 756.60 | 832.66 | 756.60 | 832.66
Above Ground Wall Area [ft2] | 2969.45 | 696.86 | 787.86 | 696.86 | 787.86
Window Opening Area [ft2] | 355.40 | 88.85 | 88.85 | 88.85 | 88.85
Gross Window-Wall Ratio [%] | 11.18 | 11.74 | 10.67 | 11.74 | 10.67
Above Ground Window-Wall Ratio [%] | 11.97 | 12.75 | 11.28 | 12.75 | 11.28

Conditioned Window-Wall Ratio

| Total | North (315 to 45 deg) | East (45 to 135 deg) | South (135 to 225 deg) | West (225 to 315 deg)
Gross Wall Area [ft2] | 2199.28 | 676.95 | 507.72 | 506.89 | 507.72
Above Ground Wall Area [ft2] | 2199.28 | 676.95 | 507.72 | 506.89 | 507.72
Window Opening Area [ft2] | 355.40 | 88.85 | 88.85 | 88.85 | 88.85
Gross Window-Wall Ratio [%] | 16.16 | 13.12 | 17.50 | 17.53 | 17.50
Above Ground Window-Wall Ratio [%] | 16.16 | 13.12 | 17.50 | 17.53 | 17.50

Skylight-Roof Ratio

| Total
Gross Roof Area [ft2] | 1656.61
Skylight Area [ft2] | 0.00
Skylight-Roof Ratio [%] | 0.00

PERFORMANCE
Zone Summary

| Area [ft2] | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Volume [ft3] | Multipliers | Above Ground Gross Wall Area [ft2] | Underground Gross Wall Area [ft2] | Window Glass Area [ft2] | Opening Area [ft2] | Lighting [Btu/h-ft2] | People [ft2 per person] | Plug and Process [Btu/h-ft2]
LIVING_UNIT1 | 2377.10 | Yes | Yes | 17050.56 | 1.00 | 2199.28 | 0.00 | 355.40 | 355.40 | 0.4851 | 792.37 | 2.2317
GARAGE1 | 400.04 | No | Yes | 3968.09 | 1.00 | 566.85 | 0.00 | 0.00 | 0.00 | 0.0000 |  | 0.0000
ATTIC_UNIT1 | 1188.55 | No | Yes | 2659.93 | 1.00 | 133.64 | 0.00 | 0.00 | 0.00 | 0.0000 |  | 0.0000
CRAWLSPACE_UNIT1 | 1188.55 | No | Yes | 2377.82 | 1.00 | 69.69 | 209.06 | 0.00 | 0.00 | 0.0000 |  | 0.0000
Total | 5154.23 |  |  | 26056.40 |  | 2969.45 | 209.06 | 355.40 | 355.40 | 0.2237 | 1718.08 | 1.0292
Conditioned Total | 2377.10 |  |  | 17050.56 |  | 2199.28 | 0.00 | 355.40 | 355.40 | 0.4851 | 792.37 | 2.2317
Unconditioned Total | 2777.13 |  |  | 9005.84 |  | 770.17 | 209.06 | 0.00 | 0.00 | 0.0000 |  | 0.0000
Not Part of Total | 0.00 |  |  | 0.00 |  | 0.00 | 0.00 | 0.00 | 0.00 |  |  |

Space Summary

| Area [ft2] | Conditioned (Y/N) | Part of Total Floor Area (Y/N) | Multipliers | Zone Name | Space Type | Radiant/Solar Enclosure Name | Lighting [Btu/h-ft2] | People [ft2 per person] | Plug and Process [Btu/h-ft2] | Tags
LIVING_UNIT1 | 2377.10 | Yes | Yes | 1.00 | LIVING_UNIT1 | GENERAL | LIVING_UNIT1 | 0.4851 | 792.37 | 2.2317 |
GARAGE1 | 400.04 | No | Yes | 1.00 | GARAGE1 | GENERAL | GARAGE1 | 0.0000 | 0.00 | 0.0000 |
ATTIC_UNIT1 | 1188.55 | No | Yes | 1.00 | ATTIC_UNIT1 | GENERAL | ATTIC_UNIT1 | 0.0000 | 0.00 | 0.0000 |
CRAWLSPACE_UNIT1 | 1188.55 | No | Yes | 1.00 | CRAWLSPACE_UNIT1 | GENERAL | CRAWLSPACE_UNIT1 | 0.0000 | 0.00 | 0.0000 |
Total | 5154.23 |  |  |  |  |  |  | 0.2237 | 1718.08 | 1.0292 |
Conditioned Total | 2377.10 |  |  |  |  |  |  | 0.4851 | 792.37 | 2.2317 |
Unconditioned Total | 2777.13 |  |  |  |  |  |  | 0.0000 | 0.00 | 0.0000 |
Not Part of Total | 0.00 |  |  |  |  |  |  | 0.0000 | 0.00 | 0.0000 |

Space Type Summary

| Total Area [ft2] | Conditioned Area [ft2] | Unconditioned Area [ft2] | Not Part of Total Area [ft2] | Lighting [Btu/h-ft2] | People [ft2 per person] | Plug and Process [Btu/h-ft2]
GENERAL | 5154.23 | 2377.10 | 2777.13 | 0.00 | 0.2237 | 1718.08 | 1.0292
Total | 5154.23 | 2377.10 | 2777.13 | 0.00 |  |  |

Table of Contents

Report: Demand End Use Components Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

End Uses

| Electricity [kBtuh] | Natural Gas [kBtuh] | Gasoline [kBtuh] | Diesel [kBtuh] | Coal [kBtuh] | Fuel Oil No 1 [kBtuh] | Fuel Oil No 2 [kBtuh] | Propane [kBtuh] | Other Fuel 1 [kBtuh] | Other Fuel 2 [kBtuh] | District Cooling [kBtuh] | District Heating Water [kBtuh] | District Heating Steam [kBtuh] | Water [gal/min]
Time of Peak | 25-JUN-18:20 | 02-FEB-07:40 | - | - | - | - | 26-FEB-08:19 | - | - | - | - | - | - | 07-JAN-08:49
Heating | 0.00 | 18.08 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | 4.53 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | 1.04 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.17 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 4.57 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 1.12 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 12.37 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.05
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total End Uses | 11.42 | 18.08 | 0.00 | 0.00 | 0.00 | 0.00 | 12.37 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.05

End Uses By Subcategory

| Subcategory | Electricity [kBtuh] | Natural Gas [kBtuh] | Gasoline [kBtuh] | Diesel [kBtuh] | Coal [kBtuh] | Fuel Oil No 1 [kBtuh] | Fuel Oil No 2 [kBtuh] | Propane [kBtuh] | Other Fuel 1 [kBtuh] | Other Fuel 2 [kBtuh] | District Cooling [kBtuh] | District Heating Water [kBtuh] | District Heating Steam [kBtuh] | Water [gal/min]
Heating | General | 0.00 | 18.08 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Boiler Parasitic | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | General | 4.53 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | General | 1.04 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | Exterior-Lights | 0.15 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Garage-Lights | 0.02 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | dishwasher | 0.18 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| refrigerator | 0.31 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| clotheswasher | 0.05 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_dryer | 0.46 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_range | 0.66 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| television | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| electric_mels | 1.81 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| IECC_adj | 1.09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Ventilation | 0.34 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| General | 0.78 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
| Domestic Hot Water | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.05
| Water Heater | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 12.37 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Source Energy End Use Components Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Values gathered over 8760.00 hours
Source Energy End Use Components Summary

| Source Electricity [kBtu] | Source Natural Gas [kBtu] | Source Gasoline [kBtu] | Source Diesel [kBtu] | Source Coal [kBtu] | Source Fuel Oil No 1 [kBtu] | Source Fuel Oil No 2 [kBtu] | Source Propane [kBtu] | Source Other Fuel 1 [kBtu] | Source Other Fuel 2 [kBtu] | Source District Cooling [kBtu] | Source District Heating Water [kBtu] | Source District Heating Steam [kBtu]
Heating | 0.00 | 24988.33 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | 16846.91 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | 11220.36 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 2285.88 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 84260.19 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 16153.93 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 536.52 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 14641.51 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 131303.78 | 24988.33 | 0.00 | 0.00 | 0.00 | 0.00 | 14641.51 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Normalized Metrics
Source Energy End Use Components Per Conditioned Floor Area

| Source Electricity [kBtu/ft2] | Source Natural Gas [kBtu/ft2] | Source Gasoline [kBtu/ft2] | Source Diesel [kBtu/ft2] | Source Coal [kBtu/ft2] | Source Fuel Oil No 1 [kBtu/ft2] | Source Fuel Oil No 2 [kBtu/ft2] | Source Propane [kBtu/ft2] | Source Other Fuel 1 [kBtu/ft2] | Source Other Fuel 2 [kBtu/ft2] | Source District Cooling [kBtu/ft2] | Source District Heating Water [kBtu/ft2] | Source District Heating Steam [kBtu/ft2]
Heating | 0.00 | 10.51 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | 7.09 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | 4.72 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.96 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 35.45 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 6.80 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.23 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 6.16 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 55.24 | 10.51 | 0.00 | 0.00 | 0.00 | 0.00 | 6.16 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Source Energy End Use Components Per Total Floor Area

| Source Electricity [kBtu/ft2] | Source Natural Gas [kBtu/ft2] | Source Gasoline [kBtu/ft2] | Source Diesel [kBtu/ft2] | Source Coal [kBtu/ft2] | Source Fuel Oil No 1 [kBtu/ft2] | Source Fuel Oil No 2 [kBtu/ft2] | Source Propane [kBtu/ft2] | Source Other Fuel 1 [kBtu/ft2] | Source Other Fuel 2 [kBtu/ft2] | Source District Cooling [kBtu/ft2] | Source District Heating Water [kBtu/ft2] | Source District Heating Steam [kBtu/ft2]
Heating | 0.00 | 4.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling | 3.27 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting | 2.18 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting | 0.44 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment | 16.35 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans | 3.13 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps | 0.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 2.84 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Source Energy End Use Components | 25.47 | 4.85 | 0.00 | 0.00 | 0.00 | 0.00 | 2.84 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Component Sizing Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

ZoneHVAC:EnergyRecoveryVentilator

| User-Specified Supply Air Flow Rate [ft3/min] | User-Specified Exhaust Air Flow Rate [ft3/min]
ERV_UNIT1 | 59.99 | 59.99

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Fan:OnOff

| User-Specified Maximum Flow Rate [ft3/min] | Design Electric Power Consumption [W]
OASUPPLYFAN_UNIT1 | 59.99 | 50.00
OAEXHAUSTFAN_UNIT1 | 59.99 | 50.00

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
HeatExchanger:AirToAir:SensibleAndLatent

| User-Specified Nominal Supply Air Flow Rate [ft3/min]
OA_HEAT_RECOVERY_UNIT1 | 59.99

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
AirTerminal:SingleDuct:ConstantVolume:NoReheat

| Design Size Maximum Air Flow Rate [ft3/min]
ZONEDIRECTAIR_UNIT1 | 692.47

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
AirLoopHVAC

| Sum of Air Terminal Maximum Heating Flow Rates [ft3/min] | Sum of Air Terminal Minimum Heating Flow Rates [ft3/min] | Sum of Air Terminal Maximum Flow Rates [ft3/min] | Adjusted Heating Design Air Flow Rate [ft3/min] | Adjusted Cooling Design Air Flow Rate [ft3/min] | Adjusted Main Design Air Flow Rate [ft3/min] | User Heating Air Flow Ratio [] | Calculated Heating Air Flow Ratio [] | Design Supply Air Flow Rate [ft3/min]
CENTRAL SYSTEM_UNIT1 | 692.47 | 692.47 | 692.47 | 692.47 | 692.47 | 692.47 | 1.00 | 1.00 | 692.47

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Fan:SystemModel

| Design Size Design Maximum Air Flow Rate [ft3/min] | Design Electric Power Consumption [W]
SUPPLY FAN_UNIT1 | 692.47 | 263.17

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
AirLoopHVAC:UnitarySystem

| Design Size Supply Air Flow Rate [ft3/min] | Design Size Heating Supply Air Flow Rate [ft3/min] | Design Size Cooling Supply Air Flow Rate [ft3/min] | User-Specified No Load Supply Air Flow Rate [ft3/min] | Design Size Nominal Cooling Capacity [ton] | Design Size Nominal Heating Capacity [Btu/h] | Design Size Maximum Supply Air Temperature [F] | User-Specified Maximum Supply Air Temperature [F] | User-Specified Supplemental Heating Coil Nominal Capacity [Btu/h] | Fraction of Supply Air Flow That Goes Through the Controlling Zone
GAHP_AHU_UNIT1 | 692.47 | 692.47 | 692.47 | 0.000000 | 1.93 | 35350.81 | 104.00 | 122.00 | 44188.51 | 1.00

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Coil:Heating:Water

| Design Size Rated Capacity [Btu/h] | Design Size Maximum Water Flow Rate [gal/min] | Design Size U-Factor Times Area Value [Btu/h-F]
MAIN DX HEATING COIL_UNIT1 | 44188.51 | 2.56 | 2159.71

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Coil:Cooling:DX:SingleSpeed

| Design Size Rated Air Flow Rate [ft3/min] | Design Size Gross Rated Total Cooling Capacity [ton] | Design Size Gross Rated Sensible Heat Ratio
DX COOLING COIL_UNIT1 | 692.47 | 1.93 | 0.761847

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Coil:Heating:Fuel

| Design Size Nominal Capacity [Btu/h]
SUPP HEATING COIL_UNIT1 | 44188.51

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
PlantLoop

| Maximum Loop Flow Rate [ft3/min] | Plant Loop Volume [ft3] | Design Supply Temperature [F] | Design Return Temperature [F] | Sizing option (Coincident/NonCoincident) | Minimum Loop Flow Rate [ft3/min] | Design Capacity [Btu/h]
GAHP_LOOP | 0.341969 | 0.684114 | 125.06 | 89.96 | 1.00 | 0.000000 | 45077.82
DHW LOOP_UNIT1 | 1.05 | 2.09 | 120.00 | 110.00 | 1.00 | 0.000000 | 39290.29

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Pump:VariableSpeed

| Design Flow Rate [ft3/min] | Design Power Consumption [Btu/h] | Design Minimum Flow Rate [ft3/min]
GAHP_PUMP | 0.341969 | 140.70 | 0.000000
MAINS PRESSURE_UNIT1 | 1.05 |  |

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
Boiler:HotWater

| Design Size Nominal Capacity [Btu/h] | Design Size Design Water Flow Rate [gal/min]
GAHP | 44188.51 | 2.56

User-Specified values were used. Design Size values were used if no User-Specified values were provided.
WaterHeater:Mixed

| Maximum Heater Capacity [Btu/h] | Use Side Design Flow Rate [ft3/min]
WATER HEATER_UNIT1 | 38002.17 | 1.05

User-Specified values were used. Design Size values were used if no User-Specified values were provided.

Table of Contents

Report: Surface Shadowing Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Surfaces (Walls, Roofs, etc) that may be Shadowed by Other Surfaces

| Possible Shadow Receivers
OVERHANG_SDR_1.UNIT1 | WALL_SDR_1.UNIT1 | WALL_SDR_1.GARAGE1 |
Mir-OVERHANG_SDR_1.UNIT1 | OVERHANG_SDR_2.UNIT1 | WALL_SDR_1.UNIT1 | WALL_SDR_2.UNIT1 | WALL_SDR_1.GARAGE1 | ROOF_RIGHT_GARAGE1 | ROOF_BACK_GARAGE1 | ROOF_RIGHT_UNIT1 |
OVERHANG_SDR_2.UNIT1 | WALL_SDR_2.UNIT1 |
Mir-OVERHANG_SDR_2.UNIT1 | WALL_SDR_2.UNIT1 | ROOF_RIGHT_UNIT1 |
WALL_LDF_1.UNIT1 | WALL_SDL_1.GARAGE1 | ROOF_LEFT_GARAGE1 |
WALL_SDR_1.UNIT1 | OVERHANG_SDR_1.UNIT1 | OVERHANG_SDR_2.UNIT1 |
WALL_LDF_2.UNIT1 | ROOF_LEFT_GARAGE1 | ROOF_FRONT_GARAGE1 | ROOF_BACK_GARAGE1 |
WALL_SDR_2.UNIT1 | OVERHANG_SDR_2.UNIT1 |
WALL_SDR_1.GARAGE1 | OVERHANG_SDR_1.UNIT1 | OVERHANG_SDR_2.UNIT1 |
WALL_SDL_1.GARAGE1 | WALL_LDF_1.UNIT1 | WALL_LDF_2.UNIT1 |
ROOF_RIGHT_GARAGE1 | OVERHANG_SDR_2.UNIT1 |
ROOF_LEFT_GARAGE1 | WALL_LDF_2.UNIT1 |
ROOF_FRONT_GARAGE1 | OVERHANG_SDR_2.UNIT1 | WALL_LDF_2.UNIT1 |
ROOF_BACK_GARAGE1 | OVERHANG_SDR_2.UNIT1 | WALL_LDF_2.UNIT1 |
BGWALL_UPPER_LDF | WALL_SDL_1.GARAGE1 | ROOF_LEFT_GARAGE1 |
BGWALL_UPPER_SDR | OVERHANG_SDR_1.UNIT1 | OVERHANG_SDR_2.UNIT1 |

Subsurfaces (Windows and Doors) that may be Shadowed by Surfaces

| Possible Shadow Receivers
WALL_LDF_1.UNIT1 | WINDOW_LDF_1.UNIT1 |
WALL_SDR_1.UNIT1 | WINDOW_SDR_1.UNIT1 |
WALL_LDB_1.UNIT1 | DOOR_LDB_UNIT1 | WINDOW_LDB_1.UNIT1 |
WALL_SDL_1.UNIT1 | WINDOW_SDL_1.UNIT1 |
WALL_LDF_2.UNIT1 | WINDOW_LDF_2.UNIT1 |
WALL_SDR_2.UNIT1 | WINDOW_SDR_2.UNIT1 |
WALL_LDB_2.UNIT1 | WINDOW_LDB_2.UNIT1 |
WALL_SDL_2.UNIT1 | WINDOW_SDL_2.UNIT1 |
WALL_LDF_1.GARAGE1 | DOOR_GARAGE1 |

Table of Contents

Report: Adaptive Comfort Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Time Not Meeting the Adaptive Comfort Models during Occupied Hours

| ASHRAE55 90% Acceptability Limits [Hours] | ASHRAE55 80% Acceptability Limits [Hours] | CEN15251 Category I Acceptability Limits [Hours] | CEN15251 Category II Acceptability Limits [Hours] | CEN15251 Category III Acceptability Limits [Hours]

Table of Contents

Report: Initialization Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Version

| Version ID
1 | 25.1

Timesteps per Hour

| #TimeSteps | Minutes per TimeStep {minutes}
1 | 6 | 10

System Convergence Limits

| Minimum System TimeStep {minutes} | Max HVAC Iterations | Minimum Plant Iterations | Maximum Plant Iterations
1 | 1 | 20 | 2 | 8

Simulation Control

| Do Zone Sizing | Do System Sizing | Do Plant Sizing | Do Design Days | Do Weather Simulation | Do HVAC Sizing Simulation
1 | Yes | Yes | No | Yes | Yes | No

Performance Precision Tradeoffs

| Use Coil Direct Simulation | Zone Radiant Exchange Algorithm | Override Mode | Number of Timestep In Hour | Force Euler Method | Minimum Number of Warmup Days | Force Suppress All Begin Environment Resets | Minimum System Timestep | MaxZoneTempDiff | MaxAllowedDelTemp
1 | No | ScriptF | Normal | 6 | No | 1 | No | 1.0 | 0.300 | 2.0000E-003

Output Reporting Tolerances

| Tolerance for Time Heating Setpoint Not Met | Tolerance for Zone Cooling Setpoint Not Met Time
1 | 0.200 | 0.200

Site:GroundTemperature:BuildingSurface

| Jan{F} | Feb{F} | Mar{F} | Apr{F} | May{F} | Jun{F} | Jul{F} | Aug{F} | Sep{F} | Oct{F} | Nov{F} | Dec{F}
1 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40 | 64.40

Site:GroundTemperature:FCfactorMethod

| Jan{F} | Feb{F} | Mar{F} | Apr{F} | May{F} | Jun{F} | Jul{F} | Aug{F} | Sep{F} | Oct{F} | Nov{F} | Dec{F}
1 | 28.06 | 18.73 | 16.21 | 18.41 | 30.99 | 45.09 | 58.35 | 67.95 | 70.75 | 66.24 | 55.38 | 41.68

Site:GroundTemperature:Shallow

| Jan{F} | Feb{F} | Mar{F} | Apr{F} | May{F} | Jun{F} | Jul{F} | Aug{F} | Sep{F} | Oct{F} | Nov{F} | Dec{F}
1 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40 | 55.40

Site:GroundTemperature:Deep

| Jan{F} | Feb{F} | Mar{F} | Apr{F} | May{F} | Jun{F} | Jul{F} | Aug{F} | Sep{F} | Oct{F} | Nov{F} | Dec{F}
1 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80 | 60.80

Site:GroundReflectance

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Site:GroundReflectance:SnowModifier

| Normal | Daylighting {dimensionless}
1 | 1.000 | 1.000

Site:GroundReflectance:Snow

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Site:GroundReflectance:Snow:Daylighting

| Jan{dimensionless} | Feb{dimensionless} | Mar{dimensionless} | Apr{dimensionless} | May{dimensionless} | Jun{dimensionless} | Jul{dimensionless} | Aug{dimensionless} | Sep{dimensionless} | Oct{dimensionless} | Nov{dimensionless} | Dec{dimensionless}
1 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20 | 0.20

Environment:Weather Station

| Wind Sensor Height Above Ground {ft} | Wind Speed Profile Exponent {} | Wind Speed Profile Boundary Layer Thickness {ft} | Air Temperature Sensor Height Above Ground {ft} | Wind Speed Modifier Coefficient-Internal | Temperature Modifier Coefficient-Internal
1 | 32.810 | 0.140 | 885.870 | 4.921 | 1.586 | 9.750E-003

Site:Location

| Location Name | Latitude {N+/S- Deg} | Longitude {E+/W- Deg} | Time Zone Number {GMT+/-} | Elevation {ft} | Standard Pressure at Elevation {psi} | Standard RhoAir at Elevation
1 | Rochester International Arpt MN USA TMY3 WMO#=726440 | 43.90 | -92.50 | -6.00 | 1305.84 | 14. | 1.1486

Site Water Mains Temperature Information

| Calculation Method{} | Water Mains Temperature Schedule Name{} | Annual Average Outdoor Air Temperature{F} | Maximum Difference In Monthly Average Outdoor Air Temperatures{deltaF} | Fixed Default Water Mains Temperature{F}
1 | Correlation | NA | 43.48 | 60.30 | NA

Building Information

| Building Name | North Axis {deg} | Terrain | Loads Convergence Tolerance Value | Temperature Convergence Tolerance Value | Solar Distribution | Maximum Number of Warmup Days | Minimum Number of Warmup Days
1 | US+SF+CZ6A+oilfurnace+crawlspace+IECC_2024_gahp | 0.000 | Suburbs | 4.00000E-002 | 0.40000 | FullExterior | 25 | 6

Inside Convection Algorithm

| Algorithm {Simple TARP CeilingDiffuser AdaptiveConvectionAlgorithm}
1 | TARP

Outside Convection Algorithm

| Algorithm {SimpleCombined TARP MoWitt DOE-2 AdaptiveConvectionAlgorithm}
1 | DOE-2

Sky Radiance Distribution

| Value {Anisotropic}
1 | Anisotropic

Zone Air Solution Algorithm

| Algorithm {ThirdOrderBackwardDifference AnalyticalSolution EulerMethod} | Space Heat Balance Sizing | Space Heat Balance Simulation
1 | ThirdOrderBackwardDifference | No | No

Zone Air Carbon Dioxide Balance Simulation

| Simulation {Yes/No} | Carbon Dioxide Concentration
1 | No | N/A

Zone Air Generic Contaminant Balance Simulation

| Simulation {Yes/No} | Generic Contaminant Concentration
1 | No | N/A

Zone Air Mass Flow Balance Simulation

| Enforce Mass Balance | Adjust Zone Mixing and Return {AdjustMixingOnly AdjustReturnOnly AdjustMixingThenReturn AdjustReturnThenMixing None} | Adjust Zone Infiltration {AddInfiltration AdjustInfiltration None} | Infiltration Zones {MixingSourceZonesOnly AllZones}
1 | No | N/A | N/A | N/A

HVACSystemRootFindingAlgorithm

| Value {RegulaFalsi Bisection BisectionThenRegulaFalsi RegulaFalsiThenBisection}
1 | RegulaFalsi

Environment:Site Atmospheric Variation

| Wind Speed Profile Exponent {} | Wind Speed Profile Boundary Layer Thickness {ft} | Air Temperature Gradient Coefficient {F/ft}
1 | 0.220 | 1213.970 | 0.003566

Material Details

| Material Name | ThermalResistance {m2-K/w} | Roughness | Thickness {ft} | Conductivity {w/m-K} | Density {lb/ft3} | Specific Heat {Btu/lbm-R} | Absorptance:Thermal | Absorptance:Solar | Absorptance:Visible
1 | sheathing_consol_layer | 0.8807 | Rough | 0.1021 | 3.533E-002 | 1.255 | 0.350 | 0.9000 | 0.7000 | 0.7000
2 | ceil_consol_layer | 6.4845 | Rough | 1.3131 | 6.172E-002 | 2.618 | 0.185 | 0.9000 | 0.7000 | 0.7000
3 | floor_consol_layer | 4.5576 | Rough | 0.7710 | 5.155E-002 | 3.438 | 0.219 | 0.9000 | 0.7000 | 0.7000
4 | bsmtwall_consol_layer | 2.3423E-005 | Rough | 0.0008 | 10.844 | 7.541 | 0.248 | 0.9000 | 0.7000 | 0.7000
5 | crawlwall_consol_layer | 2.3423E-005 | Rough | 0.0008 | 10.844 | 7.541 | 0.248 | 0.9000 | 0.7000 | 0.7000
6 | wall_consol_layer | 2.4438 | Rough | 0.4584 | 5.717E-002 | 7.541 | 0.248 | 0.9000 | 0.7000 | 0.7000
7 | Very High Reflectivity Surface | 2.1097E-006 | Smooth | 0.0016 | 237.000 | 168.680 | 0.216 | 0.9000 | 5.0000E-002 | 5.0000E-002
8 | GypsumBoard-5/16in | 5.0054E-002 | Rough | 0.0260 | 0.159 | 39.954 | 0.270 | 0.9000 | 0.4000 | 0.1000
9 | CopperPipe | 4.7506E-005 | MediumRough | 0.0625 | 401.000 | 140.026 | 0.200 | 0.9000 | 0.6500 | 0.6500
10 | F08 Metal surface | 1.7668E-005 | Smooth | 0.0026 | 45.280 | 488.437 | 0.119 | 0.9000 | 0.7000 | 0.7000
11 | Concrete_4in | 7.7356E-002 | Rough | 0.3330 | 1.312 | 140.014 | 0.111 | 0.9000 | 0.7000 | 0.7000
12 | Asphalt_shingle | 7.7448E-002 | MediumRough | 0.0208 | 8.186E-002 | 70.000 | 0.300 | 0.9000 | 0.7500 | 0.7000
13 | Wood_shingle | 0.1115 | MediumSmooth | 0.0417 | 0.114 | 26.600 | 0.390 | 0.9000 | 0.7000 | 0.7000
14 | Slate_shingle | 8.8061E-003 | MediumSmooth | 0.0417 | 1.442 | 100.000 | 0.300 | 0.9000 | 0.7000 | 0.7000
15 | cement_stucco | 2.6422E-002 | MediumSmooth | 0.0625 | 0.721 | 116.464 | 0.210 | 0.9000 | 0.7000 | 0.7000
16 | syn_stucco | 3.5237E-002 | MediumSmooth | 0.0100 | 8.650E-002 | 24.971 | 0.210 | 0.7000 | 0.7000 | 0.7000
17 | Drywall_1/2in | 7.9331E-002 | MediumSmooth | 0.0417 | 0.160 | 50.000 | 0.260 | 0.9000 | 0.7000 | 0.7000
18 | OSB_5/8in | 0.1365 | MediumSmooth | 0.0521 | 0.116 | 34.000 | 0.290 | 0.9000 | 0.7000 | 0.7000
19 | OSB_7/16in | 9.5550E-002 | MediumSmooth | 0.0365 | 0.116 | 34.000 | 0.290 | 0.9000 | 0.7000 | 0.7000
20 | Blown_R30 | 5.1614 | MediumRough | 0.6975 | 4.119E-002 | 0.600 | 0.200 | 0.9000 | 0.7000 | 0.7000
21 | Blown_R30_top | 2.8489 | MediumRough | 0.3849 | 4.119E-002 | 0.600 | 0.200 | 0.9000 | 0.7000 | 0.7000
22 | Plywood_3/4in | 0.1650 | Rough | 0.0625 | 0.115 | 34.003 | 0.161 | 0.9000 | 0.7000 | 0.7000
23 | Batt_R19 | 7.3089 | MediumRough | 0.0833 | 3.475E-003 | 0.600 | 0.200 | 0.9000 | 0.7000 | 0.7000
24 | Lumber_2x4 | 0.7709 | Rough | 0.2920 | 0.115 | 32.003 | 0.183 | 0.9000 | 0.7000 | 0.7000
25 | Carpet_n_pad | 0.4224 | MediumSmooth | 0.0833 | 6.013E-002 | 2.000 | 0.200 | 0.9000 | 0.7000 | 0.7000
26 | Batt_R13 | 2.2936 | MediumRough | 0.2917 | 3.876E-002 | 0.600 | 0.200 | 0.9000 | 0.7000 | 0.7000
27 | OSB_1/2in | 0.1092 | MediumSmooth | 0.0417 | 0.116 | 34.000 | 0.290 | 0.9000 | 0.7000 | 0.7000
28 | soil_12in | 0.1761 | Rough | 1.0000 | 1.731 | 115.011 | 0.056 | 0.9000 | 0.7000 | 0.7000
29 | door_const | 0.6289 | Smooth | 0.1486 | 7.201E-002 | 32.003 | 0.183 | 0.9000 | 0.7000 | 0.7000
30 | Gyp_board_1/2in | 8.0130E-002 | Rough | 0.0417 | 0.159 | 39.954 | 0.270 | 0.9000 | 0.4000 | 0.1000
31 | Std Wood 6inch | 1.2500 | MediumSmooth | 0.4921 | 0.120 | 33.711 | 0.289 | 0.9000 | 0.7000 | 0.7000
32 | Pipe Insulation | 1.2255 | VeryRough | 0.1334 | 3.317E-002 | 5.681 | 0.200 | 0.9000 | 0.5000 | 0.5000
33 | MANF_WALL_AIRGAP | 0.1200 | Smooth | 0.0000 | 0.000 | 0.000 | 0.000 | 0.9000 | 0.7000 | 0.7000
34 | BLDG_PAPER_FELT | 1.0567E-002 | Smooth | 0.0000 | 0.000 | 0.000 | 0.000 | 0.9000 | 0.7000 | 0.7000
35 | R_HIGH | 177.0000 | MediumRough | 0.0000 | 0.000 | 0.000 | 0.000 | 0.9000 | 0.7000 | 0.7000
36 | CLEAR ACRYLIC PLASTIC | 3.3333E-003 | VerySmooth | 0.0098 | 0.900 | 0.000 | 0.000 | 0.9000 | 0.0000 | 0.0000
37 | DIFFUSING ACRYLIC PLASTIC | 2.4444E-003 | VerySmooth | 0.0072 | 0.900 | 0.000 | 0.000 | 0.9000 | 0.0000 | 0.0000
38 | INT_BLIND | 0.0000 | Rough | 0.0000 | 0.000 | 0.000 | 0.000 | 0.0000 | 0.0000 | 0.0000
39 | GLASS | 0.4542 | VerySmooth | 0.1425 | 9.560E-002 | 0.000 | 0.000 | 0.8400 | 0.0000 | 0.0000

Material:Air

| Material Name | ThermalResistance {m2-K/w}
1 | AIR_4_IN_VERT | 0.1585
2 | 3/4IN_AIR_SPACE | 8.5130E-002
3 | 3/4IN_REFLECTIVE_AIR_SPACE | 0.2466
4 | AIR_4_IN_VERT | 0.1585

Shadowing/Sun Position Calculations Annual Simulations

| Shading Calculation Method | Shading Calculation Update Frequency Method | Shading Calculation Update Frequency {days} | Maximum Figures in Shadow Overlap Calculations {} | Polygon Clipping Algorithm | Pixel Counting Resolution | Sky Diffuse Modeling Algorithm | Output External Shading Calculation Results | Disable Self-Shading Within Shading Zone Groups | Disable Self-Shading From Shading Zone Groups to Other Zones
1 | PolygonClipping | Periodic | 20 | 15000. | SutherlandHodgman | 512 | SimpleSkyDiffuseModeling | No | No | No

Surface Geometry

| Starting Corner | Vertex Input Direction | Coordinate System | Daylight Reference Point Coordinate System | Rectangular (Simple) Surface Coordinate System
1 | LowerLeftCorner | Counterclockwise | RelativeCoordinateSystem | RelativeCoordinateSystem | RelativeToZoneOrigin

Other Side Coefficients

| Name | Combined convective/radiative film coefficient {Btu/h-ft2-F} | User selected Constant Temperature {F} | Coefficient modifying the constant temperature term | Coefficient modifying the external dry bulb temperature term | Coefficient modifying the ground temperature term | Coefficient modifying the wind speed term {s/m} | Coefficient modifying the zone air temperature term | Constant Temperature Schedule Name | Sinusoidal Variation | Period of Sinusoidal Variation | Previous Other Side Temperature Coefficient | Minimum Other Side Temperature {F} | Maximum Other Side Temperature {F}
1 | SURFPROPOTHSDCOEFSLABAVERAGE | N/A | N/A | 1.000 | 0.000 | 0.000 | 0.000 | 0.000 | SCHEDULEOSCSLABAVERAGESURFACETEMP | NO | 24.000 | 0.000 | N/A | N/A
2 | SURFPROPOTHSDCOEFSLABPERIMETER | N/A | N/A | 1.000 | 0.000 | 0.000 | 0.000 | 0.000 | SCHEDULEOSCSLABPERIMETERTEMP | NO | 24.000 | 0.000 | N/A | N/A
3 | SURFPROPOTHSDCOEFSLABCORE | N/A | N/A | 1.000 | 0.000 | 0.000 | 0.000 | 0.000 | SCHEDULEOSCSLABCORETEMP | NO | 24.000 | 0.000 | N/A | N/A

Surface Heat Transfer Algorithm

| Value {CTF - ConductionTransferFunction EMPD - MoisturePenetrationDepthConductionTransferFunction CondFD - ConductionFiniteDifference HAMT - CombinedHeatAndMoistureFiniteElement} - Description | Inside Surface Max Temperature Limit{F} | Surface Convection Coefficient Lower Limit {Btu/h-ft2-F} | Surface Convection Coefficient Upper Limit {Btu/h-ft2-F}
1 | CTF - ConductionTransferFunction | 392. | 0.02 | 176.1

Shading Summary

| Number of Fixed Detached Shades | Number of Building Detached Shades | Number of Attached Shades
1 | 0 | 0 | 4

Zone Summary

| Number of Zones | Number of Zone Surfaces | Number of SubSurfaces
1 | 4 | 49 | 12

Zone Information

| Zone Name | North Axis {deg} | Origin X-Coordinate {ft} | Origin Y-Coordinate {ft} | Origin Z-Coordinate {ft} | Centroid X-Coordinate {ft} | Centroid Y-Coordinate {ft} | Centroid Z-Coordinate {ft} | Type | Zone Multiplier | Zone List Multiplier | Minimum X {ft} | Maximum X {ft} | Minimum Y {ft} | Maximum Y {ft} | Minimum Z {ft} | Maximum Z {ft} | Ceiling Height {ft} | Volume {ft3} | Zone Inside Convection Algorithm {Simple-Detailed-CeilingDiffuser-TrombeWall} | Zone Outside Convection Algorithm {Simple-Detailed-Tarp-MoWitt-DOE-2-BLAST} | Floor Area {ft2} | Exterior Gross Wall Area {ft2} | Exterior Net Wall Area {ft2} | Exterior Window Area {ft2} | Number of Surfaces | Number of SubSurfaces | Number of Shading SubSurfaces | Part of Total Building Area
1 | LIVING_UNIT1 | 0.0 | 0.00 | 0.00 | 0.00 | 19.92 | 14.93 | 8.99 | 1 | 1 | 1 | 0.00 | 39.80 | 0.00 | 29.86 | 0.49 | 17.52 | 12.76 | 17050.65 | TARP | DOE-2 | 2377.12 | 2199.28 | 1803.88 | 355.35 | 12 | 10 | 4 | Yes
2 | GARAGE1 | 0.0 | 19.82 | -20.0 | 0.00 | 29.82 | -10.0 | 5.35 | 1 | 1 | 1 | 19.82 | 39.80 | -20.0 | 0.00 | 0.49 | 11.84 | 9.91 | 3968.18 | TARP | DOE-2 | 400.03 | 566.88 | 454.82 | 0.00 | 9 | 2 | 0 | Yes
3 | ATTIC_UNIT1 | 0.0 | 0.00 | 0.00 | 0.00 | 19.92 | 14.93 | 18.67 | 1 | 1 | 1 | 0.00 | 39.80 | 0.00 | 29.86 | 17.52 | 21.98 | 2.23 | 2659.94 | TARP | DOE-2 | 1188.56 | 133.59 | 133.59 | 0.00 | 5 | 0 | 0 | Yes
4 | CRAWLSPACE_UNIT1 | 0.0 | 0.00 | 0.00 | 0.00 | 19.92 | 14.93 | -0.5 | 1 | 1 | 1 | 0.00 | 39.80 | 0.00 | 29.86 | -1.5 | 0.49 | 2.00 | 2377.73 | TARP | DOE-2 | 1188.56 | 69.65 | 69.65 | 0.00 | 10 | 0 | 0 | Yes

Zone Internal Gains Nominal

| Zone Name | Floor Area {ft2} | # Occupants | Area per Occupant {ft2/person} | Occupant per Area {person/ft2} | Interior Lighting {Btu/h-ft2} | Electric Load {Btu/h-ft2} | Gas Load {Btu/h-ft2} | Other Load {Btu/h-ft2} | Hot Water Eq {Btu/h-ft2} | Steam Equipment {Btu/h-ft2} | Sum Loads per Area {Btu/h-ft2} | Outdoor Controlled Baseboard Heat
1 | LIVING_UNIT1 | 2377.12 | 3.0 | 792.366 | 0.001 | 0.485 | 2.232 | 0.000 | 0.000 | 0.000 | 0.000 | 2.717 | No
2 | GARAGE1 | 400.03 | 0.0 | N/A | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | No
3 | ATTIC_UNIT1 | 1188.56 | 0.0 | N/A | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | No
4 | CRAWLSPACE_UNIT1 | 1188.56 | 0.0 | N/A | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | No

People Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {ft2} | # Zone Occupants | Number of People {} | People/Floor Area {person/ft2} | Floor Area per person {ft2/person} | Fraction Radiant | Fraction Convected | Sensible Fraction Calculation | Activity level | ASHRAE 55 Warnings | Carbon Dioxide Generation Rate | Minimum Number of People for All Day Types | Maximum Number of People for All Day Types | Minimum Number of People for Weekdays | Maximum Number of People for Weekdays | Minimum Number of People for Weekends/Holidays | Maximum Number of People for Weekends /Holidays | Minimum Number of People for Summer Design Days | Maximum Number of People for Summer Design Days | Minimum Number of People for Winter Design Days | Maximum Number of People for Winter Design Days
1 | PEOPLE_UNIT1 | OCCUPANCY | LIVING_UNIT1 | 2377.12 | 3.0 | 3.0 | 0.001 | 792.366 | 0.000 | 1.000 | AutoCalculate | ACTIVITY_SCH | No | 3.8200E-008 | 0.7 | 3.0 | 0.7 | 3.0 | 0.7 | 3.0 | 0.7 | 3.0 | 0.7 | 3.0

Lights Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {ft2} | # Zone Occupants | Lighting Level {Btu/h} | Lights/Floor Area {Btu/h-ft2} | Lights per person {W/person} | Fraction Return Air | Fraction Radiant | Fraction Short Wave | Fraction Convected | Fraction Replaceable | End-Use | Minimum Lighting Level for All Day Types {Btu/h} | Maximum Lighting Level for All Day Types {Btu/h} | Minimum Lighting Level for Weekdays {Btu/h} | Maximum Lighting Level for Weekdays {Btu/h} | Minimum Lighting Level for Weekends/Holidays {Btu/h} | Maximum Lighting Level for Weekends /Holidays {Btu/h} | Minimum Lighting Level for Summer Design Days {Btu/h} | Maximum Lighting Level for Summer Design Days {Btu/h} | Minimum Lighting Level for Winter Design Days {Btu/h} | Maximum Lighting Level for Winter Design Days {Btu/h}
1 | LIVING HARDWIRED LIGHTING1 | INTERIORLIGHTINGHE | LIVING_UNIT1 | 2377.12 | 3.0 | 792.730 | 0.333 | 77.445 | 0.000 | 0.600 | 0.200 | 0.200 | 0.000 | General | 54.500 | 792.730 | 54.500 | 792.6 | 54.500 | 792.730 | 54.500 | 792.730 | 54.500 | 792.730
2 | LIVING PLUG-IN LIGHTING1 | INTERIORLIGHTINGHE | LIVING_UNIT1 | 2377.12 | 3.0 | 360.491 | 0.152 | 35.218 | 0.000 | 0.600 | 0.200 | 0.200 | 0.000 | General | 24.785 | 360.491 | 24.785 | 360.6 | 24.785 | 360.491 | 24.785 | 360.491 | 24.785 | 360.491

ElectricEquipment Internal Gains Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {ft2} | # Zone Occupants | Equipment Level {Btu/h} | Equipment/Floor Area {Btu/h-ft2} | Equipment per person {W/person} | Fraction Latent | Fraction Radiant | Fraction Lost | Fraction Convected | End-Use SubCategory | Minimum Equipment Level for All Day Types {Btu/h} | Maximum Equipment Level for All Day Types {Btu/h} | Minimum Equipment Level for Weekdays {Btu/h} | Maximum Equipment Level for Weekdays {Btu/h} | Minimum Equipment Level for Weekends/Holidays {Btu/h} | Maximum Equipment Level for Weekends /Holidays {Btu/h} | Minimum Equipment Level for Summer Design Days {Btu/h} | Maximum Equipment Level for Summer Design Days {Btu/h} | Minimum Equipment Level for Winter Design Days {Btu/h} | Maximum Equipment Level for Winter Design Days {Btu/h}
1 | DISHWASHER1 | DISHWASHER_EQUIP_SCH | LIVING_UNIT1 | 2377.12 | 3.0 | 224.165 | 0.094 | 21.900 | 0.150 | 0.600 | 0.250 | 0.000 | dishwasher | 0.000 | 224.165 | 6.432 | 209.220 | 6.892 | 224.165 | 6.892 | 224.165 | 6.892 | 224.165
2 | REFRIGERATOR1 | REFRIGERATOR | LIVING_UNIT1 | 2377.12 | 3.0 | 310.690 | 0.131 | 30.353 | 0.000 | 1.000 | 0.000 | 0.000 | refrigerator | 227.232 | 310.690 | 227.232 | 310.690 | 227.232 | 310.690 | 227.232 | 310.690 | 227.232 | 310.690
3 | CLOTHESWASHER1 | CLOTHESWASHER_EQUIP_SCH | LIVING_UNIT1 | 2377.12 | 3.0 | 97.167 | 0.041 | 9.493 | 0.000 | 0.800 | 0.200 | 0.000 | clotheswasher | 0.000 | 97.167 | 3.446 | 79.425 | 4.214 | 97.167 | 4.214 | 97.167 | 4.214 | 97.167
4 | ELECTRIC_DRYER1 | CLOTHESDRYER | LIVING_UNIT1 | 2377.12 | 3.0 | 726.978 | 0.306 | 71.022 | 5.000E-002 | 0.150 | 0.800 | 0.000 | electric_dryer | 0.000 | 726.978 | 14.494 | 594.224 | 17.732 | 726.978 | 17.732 | 726.978 | 17.732 | 726.978
5 | ELECTRIC_RANGE1 | COOKINGRANGE | LIVING_UNIT1 | 2377.12 | 3.0 | 846.701 | 0.356 | 82.718 | 0.300 | 0.400 | 0.300 | 0.000 | electric_range | 19.936 | 846.701 | 19.936 | 846.701 | 19.936 | 846.701 | 19.936 | 846.701 | 19.936 | 846.701
6 | TELEVISION1 | INTERIORLIGHTING | LIVING_UNIT1 | 2377.12 | 3.0 | 0.000 | 0.000 | 0.000 | 0.000 | 1.000 | 0.000 | 0.000 | television | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000
7 | ELECTRIC_MELS1 | MISCPLUGLOAD | LIVING_UNIT1 | 2377.12 | 3.0 | 1936.187 | 0.815 | 189.155 | 6.000E-002 | 0.690 | 0.250 | 0.000 | electric_mels | 1001.054 | 1936.187 | 1001.054 | 1936.187 | 1001.054 | 1936.187 | 1001.054 | 1936.187 | 1001.054 | 1936.187
8 | IECC_ADJ1 | MISCPLUGLOAD | LIVING_UNIT1 | 2377.12 | 3.0 | 1162.970 | 0.489 | 113.616 | 6.244E-002 | 0.412 | 0.251 | 0.275 | IECC_adj | 601.283 | 1162.970 | 601.283 | 1162.970 | 601.283 | 1162.970 | 601.283 | 1162.970 | 601.283 | 1162.970

Construction CTF

| Construction Name | Index | #Layers | #CTFs | Time Step {Hours} | ThermalConductance {Btu/h-ft2-F} | OuterThermalAbsorptance | InnerThermalAbsorptance | OuterSolarAbsorptance | InnerSolarAbsorptance | Roughness
1 | EXTERIOR WALL | 1 | 5 | 10 | 0.167 | 0.0498 | 0.700 | 0.900 | 0.700 | 0.700 | MediumSmooth
2 | INTERIORFURNISHINGS | 2 | 1 | 9 | 0.167 | 0.1409 | 0.900 | 0.900 | 0.700 | 0.700 | MediumSmooth
3 | EXTERIOR FLOOR | 4 | 3 | 9 | 0.167 | 0.0342 | 0.900 | 0.900 | 0.700 | 0.700 | Rough
4 | INTERIOR FLOOR | 5 | 2 | 4 | 0.167 | 0.300 | 0.900 | 0.900 | 0.700 | 0.700 | Rough
5 | INTERIOR CEILING | 6 | 2 | 10 | 0.167 | 0.0268 | 0.900 | 0.900 | 0.700 | 0.700 | Rough
6 | ATTIC FLOOR | 7 | 2 | 10 | 0.167 | 0.0268 | 0.900 | 0.900 | 0.700 | 0.700 | MediumSmooth
7 | EXTERIOR ROOF | 11 | 2 | 4 | 0.167 | 0.943 | 0.900 | 0.900 | 0.750 | 0.700 | MediumRough
8 | EXTERIOR DOOR | 14 | 1 | 5 | 0.167 | 0.280 | 0.900 | 0.900 | 0.700 | 0.700 | Smooth
9 | GABLE_END | 16 | 5 | 6 | 0.167 | 0.428 | 0.900 | 0.900 | 0.700 | 0.700 | MediumSmooth
10 | CRAWL WALL | 24 | 1 | 5 | 0.167 | 2.28 | 0.900 | 0.900 | 0.700 | 0.700 | Rough
11 | iz-EXTERIOR WALL | 25 | 5 | 10 | 0.167 | 0.0498 | 0.900 | 0.700 | 0.700 | 0.700 | MediumSmooth
12 | iz-EXTERIOR FLOOR | 26 | 3 | 9 | 0.167 | 0.0342 | 0.900 | 0.900 | 0.700 | 0.700 | MediumSmooth

Material CTF Summary

| Material Name | Thickness {ft} | Conductivity {w/m-K} | Density {lb/ft3} | Specific Heat {Btu/lbm-R} | ThermalResistance {m2-K/w}
1 | syn_stucco | 0.0098 | 0.086 | 24.971 | 0.210 | 0.3524E-01
2 | sheathing_consol_layer | 0.1020 | 0.035 | 1.255 | 0.350 | 0.8807
3 | OSB_7/16in | 0.0364 | 0.116 | 34.000 | 0.290 | 0.9555E-01
4 | wall_consol_layer | 0.4584 | 0.057 | 7.541 | 0.248 | 2.444
5 | Drywall_1/2in | 0.0417 | 0.160 | 50.000 | 0.260 | 0.7933E-01
6 | Std Wood 6inch | 0.4921 | 0.120 | 33.711 | 0.289 | 1.250
7 | floor_consol_layer | 0.7707 | 0.052 | 3.438 | 0.219 | 4.558
8 | Plywood_3/4in | 0.0627 | 0.115 | 34.003 | 0.161 | 0.1650
9 | Carpet_n_pad | 0.0833 | 0.060 | 2.000 | 0.200 | 0.4224
10 | Plywood_3/4in | 0.0627 | 0.115 | 34.003 | 0.161 | 0.1650
11 | Carpet_n_pad | 0.0833 | 0.060 | 2.000 | 0.200 | 0.4224
12 | ceil_consol_layer | 1.3131 | 0.062 | 2.618 | 0.185 | 6.484
13 | Drywall_1/2in | 0.0417 | 0.160 | 50.000 | 0.260 | 0.7933E-01
14 | Drywall_1/2in | 0.0417 | 0.160 | 50.000 | 0.260 | 0.7933E-01
15 | ceil_consol_layer | 1.3131 | 0.062 | 2.618 | 0.185 | 6.484
16 | Asphalt_shingle | 0.0207 | 0.082 | 70.000 | 0.300 | 0.7745E-01
17 | OSB_1/2in | 0.0417 | 0.116 | 34.000 | 0.290 | 0.1092
18 | door_const | 0.1486 | 0.072 | 32.003 | 0.183 | 0.6289
19 | cement_stucco | 0.0627 | 0.721 | 116.464 | 0.210 | 0.2642E-01
20 | BLDG_PAPER_FELT | 0.0000 | 0.000 | 0.000 | 0.000 | 0.1057E-01
21 | OSB_5/8in | 0.0522 | 0.116 | 34.000 | 0.290 | 0.1365
22 | Drywall_1/2in | 0.0417 | 0.160 | 50.000 | 0.260 | 0.7933E-01
23 | Concrete_4in | 0.3330 | 1.312 | 140.014 | 0.111 | 0.7736E-01
24 | Drywall_1/2in | 0.0417 | 0.160 | 50.000 | 0.260 | 0.7933E-01
25 | wall_consol_layer | 0.4584 | 0.057 | 7.541 | 0.248 | 2.444
26 | OSB_7/16in | 0.0364 | 0.116 | 34.000 | 0.290 | 0.9555E-01
27 | sheathing_consol_layer | 0.1020 | 0.035 | 1.255 | 0.350 | 0.8807
28 | syn_stucco | 0.0098 | 0.086 | 24.971 | 0.210 | 0.3524E-01
29 | Carpet_n_pad | 0.0833 | 0.060 | 2.000 | 0.200 | 0.4224
30 | Plywood_3/4in | 0.0627 | 0.115 | 34.003 | 0.161 | 0.1650
31 | floor_consol_layer | 0.7707 | 0.052 | 3.438 | 0.219 | 4.558

Material:Air

| Material Name | ThermalResistance {m2-K/w}
1 | AIR_4_IN_VERT | 0.1585
2 | 3/4IN_AIR_SPACE | 8.5130E-002
3 | 3/4IN_REFLECTIVE_AIR_SPACE | 0.2466
4 | AIR_4_IN_VERT | 0.1585

CTF

| Time | Outside | Cross | Inside | Flux (except final one)
1 | 10 | 0.51360630E-08 | -0.22035233E-13 | 0.91774209E-08 | -0.50676220E-13
2 | 9 | -0.14060012E-04 | 0.39159197E-12 | -0.22958088E-04 | 0.29728831E-08
3 | 8 | 0.28980689E-02 | 0.65531654E-09 | 0.46215968E-02 | -0.71708779E-05
4 | 7 | -0.65978682E-01 | 0.13350779E-06 | -0.16306378 | 0.13238707E-02
5 | 6 | 0.64596177 | 0.50193482E-05 | 2.1320981 | -0.28125917E-01
6 | 5 | -3.4215999 | 0.48298777E-04 | -13.652056 | 0.25148823
7 | 4 | 10.645660 | 0.13839053E-03 | 47.881148 | -1.1749737
8 | 3 | -19.924231 | 0.11919231E-03 | -96.040791 | 3.0621859
9 | 2 | 21.976583 | 0.26462555E-04 | 109.48934 | -4.4404618
10 | 1 | -13.118296 | 0.91387708E-06 | -65.855375 | 3.3273744
11 | 0 | 3.2593552 | 0.33613880E-09 | 16.204438 |
12 | 9 | -0.27580628E-02 | 0.97439125E-12 | -0.27580628E-02 | 0.28516790E-03
13 | 8 | 0.73590997E-01 | 0.21837543E-08 | 0.73590997E-01 | -0.77836043E-02
14 | 7 | -0.82599318 | 0.23162835E-06 | -0.82599318 | 0.89703933E-01
15 | 6 | 5.1113916 | 0.48671053E-05 | 5.1113916 | -0.57224845
16 | 5 | -19.214933 | 0.30163627E-04 | -19.214933 | 2.2266322
17 | 4 | 45.557404 | 0.63181060E-04 | 45.557404 | -5.4853312
18 | 3 | -68.275533 | 0.44785456E-04 | -68.275533 | 8.5710568
19 | 2 | 62.555368 | 0.93952058E-05 | 62.555368 | -8.2111738
20 | 1 | -31.904423 | 0.39200004E-06 | -31.904423 | 4.3886678
21 | 0 | 6.9260389 | 0.77047546E-09 | 6.9260389 |
22 | 9 | -0.61797381E-16 | 0.10275554E-15 | -0.94176193E-10 | 0.70550100E-16
23 | 8 | 0.55018702E-09 | 0.40996745E-13 | 0.10446581E-03 | -0.35964092E-09
24 | 7 | -0.45325743E-03 | 0.10183730E-08 | -0.10651944E-01 | 0.29628111E-03
25 | 6 | 0.35000963E-01 | 0.28248981E-06 | 0.18262466 | -0.23007581E-01
26 | 5 | -0.40204458 | 0.87190144E-05 | -1.3453660 | 0.27251248
27 | 4 | 1.9371679 | 0.56641591E-04 | 5.2219591 | -1.3641479
28 | 3 | -4.7809977 | 0.95620201E-04 | -11.428910 | 3.5178846
29 | 2 | 6.3416706 | 0.40914426E-04 | 14.116582 | -4.8962826
30 | 1 | -4.2976303 | 0.32019284E-05 | -9.1505965 | 3.4916880
31 | 0 | 1.1674918 | 0.10995666E-07 | 2.4144591 |
32 | 4 | 0.50405178E-13 | 0.16668152E-13 | 0.29402090E-13 | -0.58636069E-16
33 | 3 | -0.78967347E-05 | 0.18486376E-05 | -0.51544008E-05 | 0.20741056E-12
34 | 2 | 0.37655193 | 0.34407043E-01 | 0.80677627E-01 | -0.16328896E-04
35 | 1 | -8.0349315 | 0.81344511 | -1.1624309 | 0.21506451
36 | 0 | 8.9946927 | 0.48845120 | 2.4180636 |
37 | 10 | -0.96769015E-17 | -0.20747839E-14 | 0.29297638E-08 | 0.78932515E-17
38 | 9 | -0.56587496E-08 | -0.24945017E-14 | -0.14784763E-02 | 0.38539146E-08
39 | 8 | 0.72238700E-03 | 0.96019310E-10 | 0.66422612E-01 | -0.49198669E-03
40 | 7 | -0.17427411E-01 | 0.40956981E-07 | -1.0050332 | 0.12133364E-01
41 | 6 | 0.17512309 | 0.18498148E-05 | 7.5797971 | -0.12514619
42 | 5 | -0.95338624 | 0.19370257E-04 | -32.757448 | 0.70262168
43 | 4 | 3.0653739 | 0.60507497E-04 | 85.929347 | -2.3420755
44 | 3 | -5.9495223 | 0.59223871E-04 | -138.69581 | 4.7385057
45 | 2 | 6.8074199 | 0.16249306E-04 | 134.19793 | -5.6812110
46 | 1 | -4.2061463 | 0.84447462E-06 | -71.229973 | 3.6946262
47 | 0 | 1.0780011 | 0.18118629E-08 | 15.916399 |
48 | 10 | 0.29297638E-08 | -0.20747839E-14 | -0.96769015E-17 | 0.78932515E-17
49 | 9 | -0.14784763E-02 | -0.24945017E-14 | -0.56587496E-08 | 0.38539146E-08
50 | 8 | 0.66422612E-01 | 0.96019310E-10 | 0.72238700E-03 | -0.49198669E-03
51 | 7 | -1.0050332 | 0.40956981E-07 | -0.17427411E-01 | 0.12133364E-01
52 | 6 | 7.5797971 | 0.18498148E-05 | 0.17512309 | -0.12514619
53 | 5 | -32.757448 | 0.19370257E-04 | -0.95338624 | 0.70262168
54 | 4 | 85.929347 | 0.60507497E-04 | 3.0653739 | -2.3420755
55 | 3 | -138.69581 | 0.59223871E-04 | -5.9495223 | 4.7385057
56 | 2 | 134.19793 | 0.16249306E-04 | 6.8074199 | -5.6812110
57 | 1 | -71.229973 | 0.84447462E-06 | -4.2061463 | 3.6946262
58 | 0 | 15.916399 | 0.18118629E-08 | 1.0780011 |
59 | 4 | 0.75441920E-10 | 0.23883683E-10 | 0.47514224E-10 | -0.69373194E-20
60 | 3 | -0.33730907E-03 | 0.89366797E-04 | -0.22574866E-03 | 0.77828620E-10
61 | 2 | 0.58624422 | 0.18542418 | 0.49024360 | -0.17301269E-03
62 | 1 | -11.299243 | 2.8799011 | -8.6239668 | 0.15905732
63 | 0 | 15.219762 | 1.4410112 | 12.640375 |
64 | 5 | -0.22386379E-05 | 0.14507658E-06 | -0.22386379E-05 | 0.55751404E-07
65 | 4 | 0.19828726E-02 | 0.23087232E-03 | 0.19828726E-02 | -0.63287341E-04
66 | 3 | -0.19189141 | 0.19999256E-01 | -0.19189141 | 0.89189542E-02
67 | 2 | 2.6725246 | 0.18376164 | 2.6725246 | -0.18999148
68 | 1 | -8.2383273 | 0.21538727 | -8.2383273 | 0.90472632
69 | 0 | 6.1952067 | 0.20114026E-01 | 6.1952067 |
70 | 6 | 0.97988530E-11 | 0.43917118E-12 | 0.24496810E-11 | -0.34892153E-15
71 | 5 | -0.75005310E-05 | 0.16499726E-06 | -0.28271466E-05 | 0.19166609E-11
72 | 4 | 0.32354224E-01 | 0.66949565E-03 | 0.10283773E-01 | -0.11111676E-05
73 | 3 | -1.8201547 | 0.67148336E-01 | -0.62076152 | 0.38788549E-02
74 | 2 | 21.173821 | 0.53241617 | 7.5279938 | -0.97325542E-01
75 | 1 | -64.420211 | 0.46601667 | -21.697519 | 0.64629334
76 | 0 | 46.121323 | 0.20873329E-01 | 15.867130 |
77 | 5 | -0.15664505E-06 | 0.43005807E-07 | -0.15664505E-06 | 0.11899247E-09
78 | 4 | 0.10791049E-02 | 0.34140917E-03 | 0.10791049E-02 | -0.15677434E-05
79 | 3 | -0.39592122 | 0.90314630E-01 | -0.39592122 | 0.13116776E-02
80 | 2 | 11.651569 | 1.6702487 | 11.651569 | -0.78737360E-01
81 | 1 | -51.506798 | 3.1050242 | -51.506798 | 0.66829999
82 | 0 | 45.538973 | 0.42297268 | 45.538973 |
83 | 10 | 0.91774209E-08 | -0.22035233E-13 | 0.51360630E-08 | -0.50676220E-13
84 | 9 | -0.22958088E-04 | 0.39159197E-12 | -0.14060012E-04 | 0.29728831E-08
85 | 8 | 0.46215968E-02 | 0.65531654E-09 | 0.28980689E-02 | -0.71708779E-05
86 | 7 | -0.16306378 | 0.13350779E-06 | -0.65978682E-01 | 0.13238707E-02
87 | 6 | 2.1320981 | 0.50193482E-05 | 0.64596177 | -0.28125917E-01
88 | 5 | -13.652056 | 0.48298777E-04 | -3.4215999 | 0.25148823
89 | 4 | 47.881148 | 0.13839053E-03 | 10.645660 | -1.1749737
90 | 3 | -96.040791 | 0.11919231E-03 | -19.924231 | 3.0621859
91 | 2 | 109.48934 | 0.26462555E-04 | 21.976583 | -4.4404618
92 | 1 | -65.855375 | 0.91387708E-06 | -13.118296 | 3.3273744
93 | 0 | 16.204438 | 0.33613880E-09 | 3.2593552 |
94 | 9 | -0.94176193E-10 | 0.10275554E-15 | -0.61797381E-16 | 0.70550100E-16
95 | 8 | 0.10446581E-03 | 0.40996745E-13 | 0.55018702E-09 | -0.35964092E-09
96 | 7 | -0.10651944E-01 | 0.10183730E-08 | -0.45325743E-03 | 0.29628111E-03
97 | 6 | 0.18262466 | 0.28248981E-06 | 0.35000963E-01 | -0.23007581E-01
98 | 5 | -1.3453660 | 0.87190144E-05 | -0.40204458 | 0.27251248
99 | 4 | 5.2219591 | 0.56641591E-04 | 1.9371679 | -1.3641479
100 | 3 | -11.428910 | 0.95620201E-04 | -4.7809977 | 3.5178846
101 | 2 | 14.116582 | 0.40914426E-04 | 6.3416706 | -4.8962826
102 | 1 | -9.1505965 | 0.32019284E-05 | -4.2976303 | 3.4916880
103 | 0 | 2.4144591 | 0.10995666E-07 | 1.1674918 |

WindowConstruction

| Construction Name | Index | #Layers | Roughness | Conductance {Btu/h-ft2-F} | Conductance (Before Adjusted) {Btu/h-ft2-F} | Convection Coefficient Adjustment Ratio | SHGC | Solar Transmittance at Normal Incidence | Visible Transmittance at Normal Incidence
1 | EXTERIOR WINDOW | 12 | 1 | VerySmooth | 0.280 | 0.280 | 1.000 | 0.335 | 0.248 | 0.882
2 | INTERIOR WINDOW | 13 | 1 | VerySmooth | 0.280 | 0.280 | 1.000 | 0.335 | 0.248 | 0.882
3 | WINDOW_W_BLINDS | 18 | 2 | VerySmooth | 0.280 | 0.280 | 1.000 | 0.309 | 4.642E-002 | 0.133
4 | TDD DOME | 22 | 1 | VerySmooth | 1.071 | 1.071 | 1.000 | 0.929 | 0.920 | 0.920
5 | TDD DIFFUSER | 23 | 1 | VerySmooth | 1.077 | 1.077 | 1.000 | 0.906 | 0.900 | 0.900

WindowMaterial:Glazing

| Material Name | Optical Data Type | Spectral Data Set Name | Thickness {ft} | Solar Transmittance | Front Solar Reflectance | Back Solar Reflectance | Visible Transmittance | Front Visible Reflectance | Back Visible Reflectance | Infrared Transmittance | Front Thermal Emissivity | Back Thermal Emissivity | Conductivity {W/m-K} | Dirt Factor | Solar Diffusing
1 | GLASS | SpectralAverage |  | 0.14246 | 0.24698 | 0.55318 | 0.55318 | 0.88000 | 0.11900 | 0.11900 | 0.00000 | 0.84000 | 0.84000 | 9.56013E-002 | 1.00000 | No
2 | GLASS | SpectralAverage |  | 0.14246 | 0.24698 | 0.55318 | 0.55318 | 0.88000 | 0.11900 | 0.11900 | 0.00000 | 0.84000 | 0.84000 | 9.56013E-002 | 1.00000 | No
3 | GLASS | SpectralAverage |  | 0.14246 | 0.24698 | 0.55318 | 0.55318 | 0.88000 | 0.11900 | 0.11900 | 0.00000 | 0.84000 | 0.84000 | 9.56013E-002 | 1.00000 | No
4 | CLEAR ACRYLIC PLASTIC | SpectralAverage |  | 0.00984 | 0.92000 | 5.00000E-002 | 5.00000E-002 | 0.92000 | 5.00000E-002 | 5.00000E-002 | 0.00000 | 0.90000 | 0.90000 | 0.90000 | 1.00000 | No
5 | DIFFUSING ACRYLIC PLASTIC | SpectralAverage |  | 0.00722 | 0.90000 | 8.00000E-002 | 8.00000E-002 | 0.90000 | 8.00000E-002 | 8.00000E-002 | 0.00000 | 0.90000 | 0.90000 | 0.90000 | 1.00000 | No

WindowMaterial:Blind

| Material Name | Slat Width {ft} | Slat Separation {ft} | Slat Thickness {ft} | Slat Angle {deg} | Slat Beam Solar Transmittance | Slat Beam Solar Front Reflectance | Blind To Glass Distance {ft}
1 | INT_BLIND | 0.0820 | 0.0615 | 0.0033 | 45.000 | 0.000 | 0.500 | 0.164

Water Heater Information

| Type | Name | Volume {ft3} | Maximum Capacity {Btu/h} | Standard Rated Recovery Efficiency | Standard Rated Energy Factor
1 | WaterHeater:Mixed | WATER HEATER_UNIT1 | 6.9509 | 38002.2 | 0.821 | 0.6023

ZoneVentilation Airflow Stats Nominal

| Name | Schedule Name | Zone Name | Zone Floor Area {ft2} | # Zone Occupants | Design Volume Flow Rate {ft3/min} | Volume Flow Rate/Floor Area {ft3/min-ft2} | Volume Flow Rate/person Area {ft3/min-person} | ACH - Air Changes per Hour | Fan Type {Exhaust;Intake;Natural} | Fan Pressure Rise {psi} | Fan Efficiency {} | Equation A - Constant Term Coefficient {} | Equation B - Temperature Term Coefficient {1/C} | Equation C - Velocity Term Coefficient {s/m} | Equation D - Velocity Squared Term Coefficient {s2/m2} | Minimum Indoor Temperature{F}/Schedule | Maximum Indoor Temperature{F}/Schedule | Delta Temperature{F}/Schedule | Minimum Outdoor Temperature{F}/Schedule | Maximum Outdoor Temperature{F}/Schedule | Maximum WindSpeed{ft/min}
1 | VENTILATION_UNIT1 | ALWAYS_AVAIL | LIVING_UNIT1 | 2377.12 | 3.0 | 0.000 | 0.000 | 0.000 | 0.000 | Exhaust | 0.000 | 0.6 | 1.000 | 0.000 | 0.000 | 0.000 | -148.0 | 212.00 | -148.0 | -148.0 | 212.00 | 7874.40

AirFlow Model

| Simple
1 | Simple

RoomAir Model

| Zone Name | Mixing/Mundt/UCSDDV/UCSDCV/UCSDUFI/UCSDUFE/User Defined
1 | LIVING_UNIT1 | Mixing/Well-Stirred
2 | GARAGE1 | Mixing/Well-Stirred
3 | ATTIC_UNIT1 | Mixing/Well-Stirred
4 | CRAWLSPACE_UNIT1 | Mixing/Well-Stirred

AirflowNetwork Model:Control

| No Multizone or Distribution/Multizone with Distribution/Multizone without Distribution/Multizone with Distribution only during Fan Operation
1 | NoMultizoneOrDistribution

Zone Volume Capacitance Multiplier

| Sensible Heat Capacity Multiplier | Moisture Capacity Multiplier | Carbon Dioxide Capacity Multiplier | Generic Contaminant Capacity Multiplier
1 | 1.000 | 1.000 | 1.000 | 1.000

Load Timesteps in Zone Design Calculation Averaging Window

| Value
1 | 6

Heating Sizing Factor Information

| Sizing Factor ID | Value
1 | Global | 1.0000

Cooling Sizing Factor Information

| Sizing Factor ID | Value
1 | Global | 1.0000

Zone Sizing Information

| Zone Name | Load Type | Calc Des Load {Btu/h} | User Des Load {Btu/h} | Calc Des Air Flow Rate {ft3/min} | User Des Air Flow Rate {ft3/min} | Design Day Name | Date/Time of Peak | Temperature at Peak {F} | Humidity Ratio at Peak {lbWater/lbDryAir} | Floor Area {ft2} | # Occupants | Calc Outdoor Air Flow Rate {ft3/min} | Calc DOAS Heat Addition Rate {Btu/h}
1 | LIVING_UNIT1 | Cooling | 15513.87799 | 15513.87799 | 692.47873 | 692.47873 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | 83.58080 | 0.01536 | 2377.09544 | 3.00000 | 59.99321 | 0.00000
2 | LIVING_UNIT1 | Heating | 16579.66499 | 16579.66499 | 494.44909 | 494.44909 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | -15.1600 | 0.00036 | 2377.09544 | 3.00000 | 59.99321 | 0.00000

System Sizing Information

| System Name | Load Type | Peak Load Kind | User Design Capacity [Btu/h] | Calc Des Air Flow Rate [ft3/min] | User Des Air Flow Rate [ft3/min] | Design Day Name | Date/Time of Peak
1 | CENTRAL SYSTEM_UNIT1 | Cooling | Sensible | 15833.45 | 692.47873 | 692.47873 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00
2 | CENTRAL SYSTEM_UNIT1 | Heating | Sensible | 21737.75 | 494.44909 | 494.44909 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00

Component Sizing Information

| Component Type | Component Name | Input Field Description | Value
1 | ZoneHVAC:EnergyRecoveryVentilator | ERV_UNIT1 | User-Specified Supply Air Flow Rate [ft3/min] | 59.99321
2 | ZoneHVAC:EnergyRecoveryVentilator | ERV_UNIT1 | User-Specified Exhaust Air Flow Rate [ft3/min] | 59.99321
3 | Fan:OnOff | OASUPPLYFAN_UNIT1 | User-Specified Maximum Flow Rate [ft3/min] | 59.99321
4 | Fan:OnOff | OASUPPLYFAN_UNIT1 | Design Electric Power Consumption [W] | 50.00000
5 | Fan:OnOff | OAEXHAUSTFAN_UNIT1 | User-Specified Maximum Flow Rate [ft3/min] | 59.99321
6 | Fan:OnOff | OAEXHAUSTFAN_UNIT1 | Design Electric Power Consumption [W] | 50.00000
7 | HeatExchanger:AirToAir:SensibleAndLatent | OA_HEAT_RECOVERY_UNIT1 | User-Specified Nominal Supply Air Flow Rate [ft3/min] | 59.99321
8 | AirTerminal:SingleDuct:ConstantVolume:NoReheat | ZONEDIRECTAIR_UNIT1 | Design Size Maximum Air Flow Rate [ft3/min] | 692.47873
9 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Sum of Air Terminal Maximum Heating Flow Rates [ft3/min] | 692.47873
10 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Sum of Air Terminal Minimum Heating Flow Rates [ft3/min] | 692.47873
11 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Sum of Air Terminal Maximum Flow Rates [ft3/min] | 692.47873
12 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Adjusted Heating Design Air Flow Rate [ft3/min] | 692.47873
13 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Adjusted Cooling Design Air Flow Rate [ft3/min] | 692.47873
14 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Adjusted Main Design Air Flow Rate [ft3/min] | 692.47873
15 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | User Heating Air Flow Ratio [] | 1.00000
16 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Calculated Heating Air Flow Ratio [] | 1.00000
17 | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | Design Supply Air Flow Rate [ft3/min] | 692.47873
18 | Fan:SystemModel | SUPPLY FAN_UNIT1 | Design Size Design Maximum Air Flow Rate [ft3/min] | 692.47873
19 | Fan:SystemModel | SUPPLY FAN_UNIT1 | Design Electric Power Consumption [W] | 263.16859
20 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Supply Air Flow Rate [ft3/min] | 692.47873
21 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Heating Supply Air Flow Rate [ft3/min] | 692.47873
22 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Cooling Supply Air Flow Rate [ft3/min] | 692.47873
23 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | User-Specified No Load Supply Air Flow Rate [ft3/min] | 0.00000
24 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Nominal Cooling Capacity [ton] | 1.93136
25 | Coil:Heating:Water | MAIN DX HEATING COIL_UNIT1 | Design Size Rated Capacity [Btu/h] | 44188.50830
26 | Coil:Heating:Water | MAIN DX HEATING COIL_UNIT1 | Design Size Maximum Water Flow Rate [gal/min] | 2.55866
27 | Coil:Heating:Water | MAIN DX HEATING COIL_UNIT1 | Design Size U-Factor Times Area Value [Btu/h-F] | 2159.71178
28 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Nominal Heating Capacity [Btu/h] | 35350.80663
29 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Design Size Maximum Supply Air Temperature [F] | 104.00000
30 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | User-Specified Maximum Supply Air Temperature [F] | 122.00000
31 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | User-Specified Supplemental Heating Coil Nominal Capacity [Btu/h] | 44188.50830
32 | AirLoopHVAC:UnitarySystem | GAHP_AHU_UNIT1 | Fraction of Supply Air Flow That Goes Through the Controlling Zone | 1.00000
33 | Coil:Cooling:DX:SingleSpeed | DX COOLING COIL_UNIT1 | Design Size Rated Air Flow Rate [ft3/min] | 692.47873
34 | Coil:Cooling:DX:SingleSpeed | DX COOLING COIL_UNIT1 | Design Size Gross Rated Total Cooling Capacity [ton] | 1.93136
35 | Coil:Cooling:DX:SingleSpeed | DX COOLING COIL_UNIT1 | Design Size Gross Rated Sensible Heat Ratio | 0.76185
36 | Coil:Heating:Fuel | SUPP HEATING COIL_UNIT1 | Design Size Nominal Capacity [Btu/h] | 44188.50830
37 | PlantLoop | GAHP_LOOP | Maximum Loop Flow Rate [ft3/min] | 0.34197
38 | PlantLoop | GAHP_LOOP | Plant Loop Volume [ft3] | 0.68411
39 | PlantLoop | GAHP_LOOP | Design Supply Temperature [F] | 125.06000
40 | PlantLoop | GAHP_LOOP | Design Return Temperature [F] | 89.96000
41 | PlantLoop | GAHP_LOOP | Sizing option (Coincident/NonCoincident) | 1.00000
42 | PlantLoop | GAHP_LOOP | Minimum Loop Flow Rate [ft3/min] | 0.00000
43 | PlantLoop | GAHP_LOOP | Design Capacity [Btu/h] | 45077.81959
44 | Pump:VariableSpeed | GAHP_PUMP | Design Flow Rate [ft3/min] | 0.34197
45 | Pump:VariableSpeed | GAHP_PUMP | Design Power Consumption [Btu/h] | 140.70402
46 | Pump:VariableSpeed | GAHP_PUMP | Design Minimum Flow Rate [ft3/min] | 0.00000
47 | Boiler:HotWater | GAHP | Design Size Nominal Capacity [Btu/h] | 44188.50830
48 | Boiler:HotWater | GAHP | Design Size Design Water Flow Rate [gal/min] | 2.55866
49 | PlantLoop | DHW LOOP_UNIT1 | Maximum Loop Flow Rate [ft3/min] | 1.04620
50 | PlantLoop | DHW LOOP_UNIT1 | Plant Loop Volume [ft3] | 2.09294
51 | PlantLoop | DHW LOOP_UNIT1 | Design Supply Temperature [F] | 120.00000
52 | PlantLoop | DHW LOOP_UNIT1 | Design Return Temperature [F] | 109.99999
53 | PlantLoop | DHW LOOP_UNIT1 | Sizing option (Coincident/NonCoincident) | 1.00000
54 | PlantLoop | DHW LOOP_UNIT1 | Minimum Loop Flow Rate [ft3/min] | 0.00000
55 | PlantLoop | DHW LOOP_UNIT1 | Design Capacity [Btu/h] | 39290.28535
56 | Pump:VariableSpeed | MAINS PRESSURE_UNIT1 | Design Flow Rate [ft3/min] | 1.04620
57 | WaterHeater:Mixed | WATER HEATER_UNIT1 | Maximum Heater Capacity [Btu/h] | 38002.17360
58 | WaterHeater:Mixed | WATER HEATER_UNIT1 | Use Side Design Flow Rate [ft3/min] | 1.04620

Water Heating Coil Capacity Information

| Component Type | Name | Nominal Total Capacity {Btu/h}
1 | Coil:Heating:Water | MAIN DX HEATING COIL_UNIT1 | 69088.19

DX Cooling Coil Standard Rating Information

| Component Type | Component Name | Standard Rating (Net) Cooling Capacity {ton} | Standard Rating Net COP {Btuh/Btuh} | EER {Btu/W-h} | SEER User {Btu/W-h} | SEER Standard {Btu/W-h} | IEER {Btu/W-h}
1 | Coil:Cooling:DX:SingleSpeed | DX COOLING COIL_UNIT1 | 1.9 | 3.42 | 11.67 | 12.37 | 11.89 | 12.1

DX Cooling Coil AHRI 2023 Standard Rating Information

| Component Type | Component Name | Standard Rating (Net) Cooling Capacity {ton} | Standard Rating Net COP2 {Btuh/Btuh} | EER2 {Btu/W-h} | SEER2 User {Btu/W-h} | SEER2 Standard {Btu/W-h} | IEER 2022 {Btu/W-h}
1 | Coil:Cooling:DX:SingleSpeed | DX COOLING COIL_UNIT1 | 1.8 | 3.30 | 11.26 | 11.93 | 11.79 | 11.5

Environment

| Environment Name | Environment Type | Start Date | End Date | Start DayOfWeek | Duration {#days} | Source:Start DayOfWeek | Use Daylight Saving | Use Holidays | Apply Weekend Holiday Rule | Use Rain Values | Use Snow Values | Sky Temperature Model
1 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | SizingPeriod:DesignDay | 01/21 | 01/21 | WinterDesignDay | 1 | N/A | N/A | N/A | N/A | N/A | N/A | Clark and Allen
2 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | SizingPeriod:DesignDay | 07/21 | 07/21 | SummerDesignDay | 1 | N/A | N/A | N/A | N/A | N/A | N/A | Clark and Allen
3 | ANNUAL | WeatherFileRunPeriod | 01/01/2017 | 12/31/2017 | Sunday | 365 | Use RunPeriod Specified Day | Yes | Yes | No | Yes | Yes | Clark and Allen

Environment:Daylight Saving

| Daylight Saving Indicator | Source | Start Date | End Date
1 | No | SizingPeriod:DesignDay |  |
2 | No | SizingPeriod:DesignDay |  |
3 | No |  |  |

Environment:WarmupDays

| NumberofWarmupDays
1 | 6
2 | 6
3 | 6

Environment:Design Day Data

| Max Dry-Bulb Temp {F} | Temp Range {dC} | Temp Range Ind Type | Hum Ind Type | Hum Ind Value at Max Temp | Hum Ind Units | Pressure {psi} | Wind Direction {deg CW from N} | Wind Speed {ft/min} | Clearness | Rain | Snow
1 | -15.2 | 0.00 | DefaultMultipliers | Wetbulb | -26.20 | {C} | 14. | 310 | 1122.1 | 0.00 | No | No
2 | 88.16 | 10.60 | DefaultMultipliers | Wetbulb | 23.10 | {C} | 14. | 200 | 1319.0 | 0.00 | No | No

Environment:Design Day Misc

| DayOfYear | ASHRAE A Coeff | ASHRAE B Coeff | ASHRAE C Coeff | Solar Constant-Annual Variation | Eq of Time {minutes} | Solar Declination Angle {deg} | Solar Model
1 | 21 | 1229.0 | 0.1415 | 5.7310E-002 | 1.0 | -11.15 | -20. | ASHRAEClearSky
2 | 202 | 1084.4 | 0.2082 | 0.1365 | 1.0 | -6.23 | 20.6 | ASHRAETau

Tabular Report

| Style | Unit Conversion
1 | Commaandhtml | commaandhtml

Warmup Convergence Information

| Zone Name | Environment Type/Name | Average Warmup Temperature Difference {deltaF} | Std Dev Warmup Temperature Difference {deltaF} | Max Temperature Pass/Fail Convergence | Min Temperature Pass/Fail Convergence | Average Warmup Load Difference {Btu/h} | Std Dev Warmup Load Difference {Btu/h} | Heating Load Pass/Fail Convergence | Cooling Load Pass/Fail Convergence
1 | LIVING_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 0.000014712 | 0.000070146 | Pass | Pass | 0.009273042 | 0.016186961 | Pass | Pass
2 | GARAGE1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 0.000103424 | 0.000084625 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
3 | ATTIC_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 0.000247284 | 0.000211191 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
4 | CRAWLSPACE_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 0.000351400 | 0.000305122 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
5 | LIVING_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 0.000041275 | 0.000203114 | Pass | Pass | 0.095215824 | 0.080630953 | Pass | Pass
6 | GARAGE1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 0.619008273 | 0.487526695 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
7 | ATTIC_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 0.896375457 | 0.683341617 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
8 | CRAWLSPACE_UNIT1 | SizingPeriod: ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 0.060810460 | 0.035886895 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
9 | LIVING_UNIT1 | RunPeriod: ANNUAL | 0.000022084 | 0.000067082 | Pass | Pass | 0.043409708 | 0.066021738 | Pass | Pass
10 | GARAGE1 | RunPeriod: ANNUAL | 0.176553867 | 0.200401135 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
11 | ATTIC_UNIT1 | RunPeriod: ANNUAL | 0.283892765 | 0.339484198 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass
12 | CRAWLSPACE_UNIT1 | RunPeriod: ANNUAL | 0.016858210 | 0.016375579 | Pass | Pass | 0.000000000 | 0.000000000 | Pass | Pass

Table of Contents

Report: Annual Heat Emissions Report

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Annual Heat Emissions Summary

| Envelope Convection | Zone Exfiltration | Zone Exhaust Air | HVAC Relief Air | HVAC Reject Heat | Total
Heat Emissions [kBtu] | 524828.38 | 0.00 | 0.00 | 0.00 | 29668.58 | 554497.61

Table of Contents

Report: Annual Thermal Resilience Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Heat Index Hours

| Safe (≤ 80.1°F) [hr] | Caution (> 80.1°F, ≤ 90.0°F) [hr] | Extreme Caution (> 90.0°F, ≤ 102.9°F) [hr] | Danger (> 102.9, ≤ 125.1°F) [hr] | Extreme Danger (> 125.1°F) [hr]
LIVING_UNIT1 | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 7646.50 | 618.00 | 473.00 | 22.50 | 0.00
ATTIC_UNIT1 | 7471.33 | 485.50 | 478.33 | 324.83 | 0.00
CRAWLSPACE_UNIT1 | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 7471.33 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8760.00 | 618.00 | 478.33 | 324.83 | 0.00
Average | 8159.46 | 275.88 | 237.83 | 86.83 | 0.00
Sum | 32637.83 | 1103.50 | 951.33 | 347.33 | 0.00

Heat Index OccupantHours

| Safe (≤ 80.1°F) [hr] | Caution (> 80.1°F, ≤ 90.0°F) [hr] | Extreme Caution (> 90.0°F, ≤ 102.9°F) [hr] | Danger (> 102.9, ≤ 125.1°F) [hr] | Extreme Danger (> 125.1°F) [hr]
LIVING_UNIT1 | 18093.57 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 18093.57 | 0.00 | 0.00 | 0.00 | 0.00
Average | 4523.39 | 0.00 | 0.00 | 0.00 | 0.00
Sum | 18093.57 | 0.00 | 0.00 | 0.00 | 0.00

Heat Index OccupiedHours

| Safe (≤ 80.1°F) [hr] | Caution (> 80.1°F, ≤ 90.0°F) [hr] | Extreme Caution (> 90.0°F, ≤ 102.9°F) [hr] | Danger (> 102.9, ≤ 125.1°F) [hr] | Extreme Danger (> 125.1°F) [hr]
LIVING_UNIT1 | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
Average | 2190.00 | 0.00 | 0.00 | 0.00 | 0.00
Sum | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00

Humidex Hours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
LIVING_UNIT1 | 8749.00 | 11.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 8068.17 | 656.67 | 35.17 | 0.00 | 0.00
ATTIC_UNIT1 | 7818.50 | 580.83 | 178.17 | 137.17 | 45.33
CRAWLSPACE_UNIT1 | 8760.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 7818.50 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8760.00 | 656.67 | 178.17 | 137.17 | 45.33
Average | 8348.92 | 312.12 | 53.33 | 34.29 | 11.33
Sum | 33395.67 | 1248.50 | 213.33 | 137.17 | 45.33

Humidex OccupantHours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
LIVING_UNIT1 | 18067.94 | 25.63 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 18067.94 | 25.63 | 0.00 | 0.00 | 0.00
Average | 4516.98 | 6.41 | 0.00 | 0.00 | 0.00
Sum | 18067.94 | 25.63 | 0.00 | 0.00 | 0.00

Humidex OccupiedHours

| Little to no Discomfort (≤ 29) [hr] | Some Discomfort (> 29, ≤ 40) [hr] | Great Discomfort; Avoid Exertion (> 40, ≤ 45) [hr] | Dangerous (> 45, ≤ 50) [hr] | Heat Stroke Quite Possible (> 50) [hr]
LIVING_UNIT1 | 8749.00 | 11.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 8749.00 | 11.00 | 0.00 | 0.00 | 0.00
Average | 2187.25 | 2.75 | 0.00 | 0.00 | 0.00
Sum | 8749.00 | 11.00 | 0.00 | 0.00 | 0.00

Hours of Safety for Cold Events

| Hours of Safety [hr] | End Time of the Safety Duration | Safe Temperature Exceedance Hours [hr] | Safe Temperature Exceedance OccupantHours [hr] | Safe Temperature Exceedance OccupiedHours [hr]
LIVING_UNIT1 | 8760.00 | - | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | - | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | - | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | - | 0.00 | 0.00 | 0.00
Min | 0.00 | - | 0.00 | 0.00 | 0.00
Max | 8760.00 | - | 0.00 | 0.00 | 0.00
Average | 2190.00 | - | 0.00 | 0.00 | 0.00
Sum | 8760.00 | - | 0.00 | 0.00 | 0.00

Hours of Safety for Heat Events

| Hours of Safety [hr] | End Time of the Safety Duration | Safe Temperature Exceedance Hours [hr] | Safe Temperature Exceedance OccupantHours [hr] | Safe Temperature Exceedance OccupiedHours [hr]
LIVING_UNIT1 | 8760.00 | - | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | - | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | - | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | - | 0.00 | 0.00 | 0.00
Min | 0.00 | - | 0.00 | 0.00 | 0.00
Max | 8760.00 | - | 0.00 | 0.00 | 0.00
Average | 2190.00 | - | 0.00 | 0.00 | 0.00
Sum | 8760.00 | - | 0.00 | 0.00 | 0.00

Unmet Degree-Hours

| Cooling Setpoint Unmet Degree-Hours [°F·hr] | Cooling Setpoint Unmet Occupant-Weighted Degree-Hours [°F·hr] | Cooling Setpoint Unmet Occupied Degree-Hours [°F·hr] | Heating Setpoint Unmet Degree-Hours [°F·hr] | Heating Setpoint Unmet Occupant-Weighted Degree-Hours [°F·hr] | Heating Setpoint Unmet Occupied Degree-Hours [°C·hr]
LIVING_UNIT1 | 0.41 | 0.80 | 0.41 | 0.86 | 1.99 | 0.86
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.41 | 0.80 | 0.41 | 0.86 | 1.99 | 0.86
Average | 0.10 | 0.20 | 0.10 | 0.22 | 0.50 | 0.22
Sum | 0.41 | 0.80 | 0.41 | 0.86 | 1.99 | 0.86

Discomfort-weighted Exceedance OccupantHours

| Very-cold Exceedance OccupantHours [hr] | Cool Exceedance OccupantHours [hr] | Warm Exceedance OccupantHours [hr] | Very-hot Exceedance OccupantHours [hr]
LIVING_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.00 | 0.00 | 0.00 | 0.00
Average | 0.00 | 0.00 | 0.00 | 0.00
Sum | 0.00 | 0.00 | 0.00 | 0.00

Discomfort-weighted Exceedance OccupiedHours

| Very-cold Exceedance OccupantHours [hr] | Cool Exceedance OccupantHours [hr] | Warm Exceedance OccupantHours [hr] | Very-hot Exceedance OccupantHours [hr]
LIVING_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
Min | 0.00 | 0.00 | 0.00 | 0.00
Max | 0.00 | 0.00 | 0.00 | 0.00
Average | 0.00 | 0.00 | 0.00 | 0.00
Sum | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: Climatic Data Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

SizingPeriod:DesignDay

| Maximum Dry Bulb [F] | Daily Temperature Range [deltaF] | Humidity Value | Humidity Type | Wind Speed [ft/min] | Wind Direction
ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | -15.2 | 0.00 | -15.2 | Wetbulb [F] | 1122.10 | 310.00
ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 88.16 | 19.08 | 73.58 | Wetbulb [F] | 1318.96 | 200.00

Monthly Precipitation Summary

| Monthly Total Precipitation from .epw [in] | Monthly Total Hours of Rain from .epw | Monthly Total Precipitation in Site:Precipitation [in] | Monthly Total Roof Irrigation Depth [in] | Monthly Total Rain Collection Volume [ft3]
Jan | 1.02 | 35 |  |  |
Feb | 0.00 | 0 |  |  |
Mar | 0.00 | 0 |  |  |
Apr | 1.14 | 23 |  |  |
May | 0.00 | 0 |  |  |
Jun | 4.21 | 45 |  |  |
Jul | 2.83 | 29 |  |  |
Aug | 0.00 | 0 |  |  |
Sep | 0.79 | 11 |  |  |
Oct | 0.00 | 0 |  |  |
Nov | 0.00 | 0 |  |  |
Dec | 0.16 | 8 |  |  |

Weather Statistics File

| Value
Reference | USA_MN_Rochester.Intl.AP.726440_TMY3
Site:Location | Rochester International Arpt MN USA
Latitude | {N 43° 54'}
Longitude | {W 92° 30'}
Time Zone | {GMT -6.0 Hours}
Elevation (ft) above sea level | 1305.8
Standard Pressure at Elevation | 96634Pa
Data Source | TMY3
WMO Station | 726440
Weather File Design Conditions | Climate Design Data 2009 ASHRAE Handbook
Heating Design Temperature 99.6% (F) | -15.°
Heating Design Temperature 99% (F) | -9.°
Cooling Design Temperature 0.4% (F) | 88.2°
Cooling Design Temperature 1% (F) | 85.1°
Cooling Design Temperature 2% (F) | 82.4°
Maximum Dry Bulb Temperature (F) | 93.0°
Maximum Dry Bulb Occurs on | Aug 4
Minimum Dry Bulb Temperature (F) | -34.°
Minimum Dry Bulb Occurs on | Feb 2
Maximum Dew Point Temperature (F) | 78.1°
Maximum Dew Point Occurs on | Jul 26
Minimum Dew Point Temperature (F) | -41.°
Minimum Dew Point Occurs on | Feb 2
Annual Total Precipitation [mm] | 258
Max Hourly Precipitation [mm] | 16
Max Hourly Precipitation Occurs in | Jun
ASHRAE Handbook 2009 Cooling Degree-Days - base 50°(F) | 2412.0
Weather File Cooling Degree-Days - base 50°(F) | 2368.8
ASHRAE Handbook 2009 Heating Degree-Days - base 65°(F) | 7975.8
Weather File Heating Degree-Days - base 65°(F) | 8132.4
Köppen Classification | Dfb
Köppen Description | Moist continental (warm summer, cold winter, no dry season, lat. 30-60°N)
Köppen Recommendation |
ASHRAE Climate Zone | 6A
ASHRAE Description | Cold-Humid

Table of Contents

Report: Envelope Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Opaque Exterior

| Construction | Zone | Space | Reflectance | U-Factor with Film [Btu/h-ft2-F] | U-Factor no Film [Btu/h-ft2-F] | Gross Area [ft2] | Net Area [ft2] | Azimuth [deg] | Tilt [deg] | Cardinal Direction
WALL_LDF_1.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 168.42 | 123.99 | 180.00 | 90.00 | S
WALL_SDR_1.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 253.86 | 209.43 | 90.00 | 90.00 | E
WALL_LDB_1.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 338.48 | 254.03 | 0.00 | 90.00 | N
WALL_SDL_1.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 253.86 | 209.43 | 270.00 | 90.00 | W
WALL_LDF_2.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 338.48 | 294.05 | 180.00 | 90.00 | S
WALL_SDR_2.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 253.86 | 209.43 | 90.00 | 90.00 | E
WALL_LDB_2.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 338.48 | 294.05 | 0.00 | 90.00 | N
WALL_SDL_2.UNIT1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | 0.30 | 0.048 | 0.050 | 253.86 | 209.43 | 270.00 | 90.00 | W
WALL_LDF_1.GARAGE1 | GABLE_END | GARAGE1 | GARAGE1 | 0.30 | 0.314 | 0.428 | 170.06 | 58.02 | 180.00 | 90.00 | S
WALL_SDR_1.GARAGE1 | GABLE_END | GARAGE1 | GARAGE1 | 0.30 | 0.314 | 0.428 | 170.06 | 170.06 | 90.00 | 90.00 | E
WALL_SDL_1.GARAGE1 | GABLE_END | GARAGE1 | GARAGE1 | 0.30 | 0.314 | 0.428 | 170.06 | 170.06 | 270.00 | 90.00 | W
ROOF_RIGHT_GARAGE1 | GABLE_END | GARAGE1 | GARAGE1 | 0.30 | 0.314 | 0.428 | 28.33 | 28.33 | 90.00 | 90.00 | E
ROOF_LEFT_GARAGE1 | GABLE_END | GARAGE1 | GARAGE1 | 0.30 | 0.314 | 0.428 | 28.33 | 28.33 | 270.00 | 90.00 | W
ROOF_FRONT_GARAGE1 | EXTERIOR ROOF | GARAGE1 | GARAGE1 | 0.25 | 0.543 | 0.943 | 207.89 | 207.89 | 180.00 | 15.82 |
ROOF_BACK_GARAGE1 | EXTERIOR ROOF | GARAGE1 | GARAGE1 | 0.25 | 0.543 | 0.943 | 207.89 | 207.89 | 0.00 | 15.82 |
ROOF_RIGHT_UNIT1 | GABLE_END | ATTIC_UNIT1 | ATTIC_UNIT1 | 0.30 | 0.314 | 0.428 | 66.82 | 66.82 | 90.00 | 90.00 | E
ROOF_LEFT_UNIT1 | GABLE_END | ATTIC_UNIT1 | ATTIC_UNIT1 | 0.30 | 0.314 | 0.428 | 66.82 | 66.82 | 270.00 | 90.00 | W
ROOF_FRONT_UNIT1 | EXTERIOR ROOF | ATTIC_UNIT1 | ATTIC_UNIT1 | 0.25 | 0.543 | 0.943 | 620.41 | 620.41 | 180.00 | 16.69 |
ROOF_BACK_UNIT1 | EXTERIOR ROOF | ATTIC_UNIT1 | ATTIC_UNIT1 | 0.25 | 0.543 | 0.943 | 620.41 | 620.41 | 0.00 | 16.69 |
BGWALL_UPPER_LDF | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.776 | 2.276 | 19.91 | 19.91 | 180.00 | 90.00 | S
BGWALL_LOWER_LDF | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.893 | 2.276 | 59.73 | 59.73 | 180.00 | 90.00 | S
BGWALL_UPPER_SDR | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.776 | 2.276 | 14.93 | 14.93 | 90.00 | 90.00 | E
BGWALL_LOWER_SDR | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.893 | 2.276 | 44.80 | 44.80 | 90.00 | 90.00 | E
BGWALL_UPPER_LDB | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.776 | 2.276 | 19.91 | 19.91 | 0.00 | 90.00 | N
BGWALL_LOWER_LDB | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.893 | 2.276 | 59.73 | 59.73 | 0.00 | 90.00 | N
BGWALL_UPPER_SDL | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.776 | 2.276 | 14.93 | 14.93 | 270.00 | 90.00 | W
BGWALL_LOWER_SDL | CRAWL WALL | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.893 | 2.276 | 44.80 | 44.80 | 270.00 | 90.00 | W
EXTFLOOR_UNIT1 | INTERIOR FLOOR | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | 0.30 | 0.235 | 0.300 | 1188.55 | 1188.55 | 90.00 | 180.00 |

Opaque Interior

| Construction | Zone | Space | Adjacent Surface | Reflectance | U-Factor with Film [Btu/h-ft2-F] | U-Factor no Film [Btu/h-ft2-F] | Gross Area [ft2] | Net Area [ft2] | Azimuth [deg] | Tilt [deg] | Cardinal Direction
WALL_LDB_1.GARAGE1 | EXTERIOR WALL | LIVING_UNIT1 | LIVING_UNIT1 | iz-WALL_LDB_1.GARAGE1 | 0.30 | 0.047 | 0.050 | 170.06 | 149.05 | 180.00 | 90.00 | S
INTER ZONE FLOOR 1 | INTERIOR FLOOR | LIVING_UNIT1 | LIVING_UNIT1 | INTER ZONE FLOOR 1 | 0.30 | 0.193 | 0.300 | 1188.55 | 1188.55 | 90.00 | 180.00 |
FLOOR_UNIT1 | EXTERIOR FLOOR | LIVING_UNIT1 | LIVING_UNIT1 | iz-FLOOR_UNIT1 | 0.30 | 0.033 | 0.034 | 1188.55 | 1188.55 | 90.00 | 180.00 |
CEILING_UNIT1 | INTERIOR CEILING | LIVING_UNIT1 | LIVING_UNIT1 | iz-CEILING_UNIT1 | 0.30 | 0.026 | 0.027 | 1188.55 | 1188.55 | 180.00 | 0.00 |
iz-WALL_LDB_1.GARAGE1 | iz-EXTERIOR WALL | GARAGE1 | GARAGE1 | WALL_LDB_1.GARAGE1 | 0.30 | 0.047 | 0.050 | 170.06 | 149.05 | 0.00 | 90.00 | N
FLOOR_GARAGE1 | INTERIOR FLOOR | GARAGE1 | GARAGE1 | SURFPROPOTHSDCOEFSLABAVERAGE | 0.30 | 0.235 | 0.300 | 400.04 | 400.04 | 90.00 | 180.00 |
iz-CEILING_UNIT1 | ATTIC FLOOR | ATTIC_UNIT1 | ATTIC_UNIT1 | CEILING_UNIT1 | 0.30 | 0.026 | 0.027 | 1188.55 | 1188.55 | 0.00 | 180.00 |
iz-FLOOR_UNIT1 | iz-EXTERIOR FLOOR | CRAWLSPACE_UNIT1 | CRAWLSPACE_UNIT1 | FLOOR_UNIT1 | 0.30 | 0.033 | 0.034 | 1188.55 | 1188.55 | 270.00 | 0.00 |
INTERNALMASS_UNIT1 | INTERIORFURNISHINGS | LIVING_UNIT1 | LIVING_UNIT1 | INTERNALMASS_UNIT1 | 0.30 |  | 0.141 | 106.53 |  | 0.00 | 90.00 | N

Exterior Fenestration

| Construction | Zone | Space | Frame and Divider | Glass Area [ft2] | Frame Area [ft2] | Divider Area [ft2] | Area of One Opening [ft2] | Area of Multiplied Openings [ft2] | Glass U-Factor [Btu/h-ft2-F] | Glass SHGC | Glass Visible Transmittance | Frame Conductance [Btu/h-ft2-F] | Divider Conductance [Btu/h-ft2-F] | NFRC Product Type | Assembly U-Factor [Btu/h-ft2-F] | Assembly SHGC | Assembly Visible Transmittance | Shade Control | Parent Surface | Azimuth [deg] | Tilt [deg] | Cardinal Direction
WINDOW_LDF_1.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_LDF_1.UNIT1 | 180.00 | 90.00 | S
WINDOW_SDR_1.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_SDR_1.UNIT1 | 90.00 | 90.00 | E
WINDOW_LDB_1.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_LDB_1.UNIT1 | 0.00 | 90.00 | N
WINDOW_SDL_1.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_SDL_1.UNIT1 | 270.00 | 90.00 | W
WINDOW_LDF_2.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_LDF_2.UNIT1 | 180.00 | 90.00 | S
WINDOW_SDR_2.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_SDR_2.UNIT1 | 90.00 | 90.00 | E
WINDOW_LDB_2.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_LDB_2.UNIT1 | 0.00 | 90.00 | N
WINDOW_SDL_2.UNIT1 | EXTERIOR WINDOW | LIVING_UNIT1 | LIVING_UNIT1 |  | 44.43 | 0.00 | 0.00 | 44.43 | 44.43 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  | Yes | WALL_SDL_2.UNIT1 | 270.00 | 90.00 | W
Total or Average |  |  |  |  |  |  |  |  | 355.40 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  |  |  |  |  |
North Total or Average |  |  |  |  |  |  |  |  | 88.85 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  |  |  |  |  |
Non-North Total or Average |  |  |  |  |  |  |  |  | 266.55 | 0.280 | 0.335 | 0.882 |  |  |  |  |  |  |  |  |  |  |

Exterior Fenestration Shaded State

| Frame and Divider | Glass U-Factor [Btu/h-ft2-F] | Glass SHGC | Glass Visible Transmittance | NFRC Product Type | Assembly U-Factor [Btu/h-ft2-F] | Assembly SHGC | Assembly Visible Transmittance
None |  |  |  |  |  |  |  |

Interior Fenestration

| Construction | Zone | Space | Area of One Opening [ft2] | Area of Openings [ft2] | Glass U-Factor [Btu/h-ft2-F] | Glass SHGC | Glass Visible Transmittance | Parent Surface
Total or Average |  |  |  |  | 0.00 | - | - | - |

Exterior Door

| Construction | Zone | Space | U-Factor with Film [Btu/h-ft2-F] | U-Factor no Film [Btu/h-ft2-F] | Gross Area [ft2] | Parent Surface
DOOR_LDB_UNIT1 | EXTERIOR DOOR | LIVING_UNIT1 | LIVING_UNIT1 | 0.226 | 0.280 | 40.02 | WALL_LDB_1.UNIT1
DOOR_GARAGE1 | EXTERIOR DOOR | GARAGE1 | GARAGE1 | 0.226 | 0.280 | 112.04 | WALL_LDF_1.GARAGE1

Interior Door

| Construction | Zone | Space | U-Factor with Film [Btu/h-ft2-F] | U-Factor no Film [Btu/h-ft2-F] | Gross Area [ft2] | Parent Surface
INT_DOOR_GARAGE1 | EXTERIOR DOOR | LIVING_UNIT1 | LIVING_UNIT1 | 0.203 | 0.280 | 21.01 | WALL_LDB_1.GARAGE1
iz-INT_DOOR_GARAGE1 | EXTERIOR DOOR | GARAGE1 | GARAGE1 | 0.203 | 0.280 | 21.01 | iz-WALL_LDB_1.GARAGE1

Opaque Construction Layers

| Layer 1 | Layer 2 | Layer 3 | Layer 4 | Layer 5 | Layer 6 | Layer 7 | Layer 8 | Layer 9 | Layer 10
EXTERIOR WALL | syn_stucco | sheathing_consol_layer | OSB_7/16in | wall_consol_layer | Drywall_1/2in |  |  |  |  |
INTERIORFURNISHINGS | Std Wood 6inch |  |  |  |  |  |  |  |  |
EXTERIOR FLOOR | floor_consol_layer | Plywood_3/4in | Carpet_n_pad |  |  |  |  |  |  |
INTERIOR FLOOR | Plywood_3/4in | Carpet_n_pad |  |  |  |  |  |  |  |
INTERIOR CEILING | ceil_consol_layer | Drywall_1/2in |  |  |  |  |  |  |  |
ATTIC FLOOR | Drywall_1/2in | ceil_consol_layer |  |  |  |  |  |  |  |
EXTERIOR ROOF | Asphalt_shingle | OSB_1/2in |  |  |  |  |  |  |  |
EXTERIOR DOOR | door_const |  |  |  |  |  |  |  |  |
GABLE_END | cement_stucco | BLDG_PAPER_FELT | OSB_5/8in | AIR_4_IN_VERT | Drywall_1/2in |  |  |  |  |
CRAWL WALL | Concrete_4in |  |  |  |  |  |  |  |  |
iz-EXTERIOR WALL | Drywall_1/2in | wall_consol_layer | OSB_7/16in | sheathing_consol_layer | syn_stucco |  |  |  |  |
iz-EXTERIOR FLOOR | Carpet_n_pad | Plywood_3/4in | floor_consol_layer |  |  |  |  |  |  |

Table of Contents

Report: Shading Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Sunlit Fraction

| March 21 9am | March 21 noon | March 21 3pm | June 21 9am | June 21 noon | June 21 3pm | December 21 9am | December 21 noon | December 21 3pm
WINDOW_LDF_1.UNIT1 | 0.61 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00 | 0.06 | 1.00 | 1.00
WINDOW_SDR_1.UNIT1 | 1.00 | 0.96 | 0.00 | 0.99 | 0.93 | 0.00 | 1.00 | 0.96 | 0.00
WINDOW_LDB_1.UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
WINDOW_SDL_1.UNIT1 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00
WINDOW_LDF_2.UNIT1 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00 | 1.00
WINDOW_SDR_2.UNIT1 | 1.00 | 0.96 | 0.00 | 0.99 | 0.93 | 0.00 | 1.00 | 0.96 | 0.00
WINDOW_LDB_2.UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
WINDOW_SDL_2.UNIT1 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00 | 0.00 | 0.00 | 1.00

Window Control

| Name | Type | Shaded Construction | Control | Glare Control
WINDOW_LDF_1.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_SDR_1.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_LDB_1.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_SDL_1.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_LDF_2.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_SDR_2.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_LDB_2.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No
WINDOW_SDL_2.UNIT1 | SHADES-LIVING_UNIT1 | Interior Blind | WINDOW_W_BLINDS | AlwaysOff | No

Table of Contents

Report: Lighting Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Interior Lighting

| Zone Name | Space Name | Space Type | Lighting Power Density [Btu/h-ft2] | Space Area [ft2] | Total Power [Btu/h] | End Use Subcategory | Schedule Name | Scheduled Hours/Week [hr] | Hours/Week > 1% [hr] | Full Load Hours/Week [hr] | Return Air Fraction | Conditioned (Y/N) | Consumption [kWh]
LIVING HARDWIRED LIGHTING1 | LIVING_UNIT1 | LIVING_UNIT1 | GENERAL | 0.3335 | 2377.10 | 792.73 | General | INTERIORLIGHTINGHE | 58.88 | 168.00 | 58.88 | 0.0000 | Y | 713.27
LIVING PLUG-IN LIGHTING1 | LIVING_UNIT1 | LIVING_UNIT1 | GENERAL | 0.1517 | 2377.10 | 360.49 | General | INTERIORLIGHTINGHE | 58.88 | 168.00 | 58.88 | 0.0000 | Y | 324.36
Interior Lighting Total |  |  |  | 0.2426 | 4754.19 | 1153.22 |  |  |  |  |  |  |  | 1037.63

Daylighting

| Zone | Control Name | Daylighting Method | Control Type | Fraction Controlled | Lighting Installed in Zone [Btu/h] | Lighting Controlled [Btu/h]
None |  |  |  |  |  |  |

Exterior Lighting

| Total Watts | Astronomical Clock/Schedule | Schedule Name | Scheduled Hours/Week [hr] | Hours/Week > 1% [hr] | Full Load Hours/Week [hr] | Consumption [kWh]
EXTERIOR-LIGHTS_UNIT1 | 43.24 | Schedule | EXTERIORLIGHTING | 84.00 | 84.00 | 84.00 | 189.40
GARAGE-LIGHTS_UNIT1 | 7.16 | Schedule | INTERIORLIGHTINGHE | 58.88 | 168.00 | 58.88 | 21.99
Exterior Lighting Total | 50.41 |  |  |  |  |  | 211.39

Table of Contents

Report: Equipment Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Central Plant

| Type | Reference Capacity [Btu/h] | Reference Efficiency [Btuh/Btuh] | Rated Capacity [Btu/h] | Rated Efficiency [Btuh/Btuh] | IPLV in SI Units [W/W] | IPLV in IP Units [Btu/W-h]
GAHP | Boiler:HotWater | 44188.51 | 1.00 |  |  |  |

Cooling Coils

| Type | Design Coil Load [Btu/h] | Nominal Total Capacity [Btu/h] | Nominal Sensible Capacity [Btu/h] | Nominal Latent Capacity [Btu/h] | Nominal Sensible Heat Ratio | Nominal Efficiency [Btuh/Btuh] | Nominal Coil UA Value [Btu/h-F] | Nominal Coil Surface Area [ft2]
DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed |  | 23176.29 | 17656.79 | 5519.50 | 0.76 | 4.09 |  |

Nominal values are gross at rated conditions, i.e., the supply air fan heat and electric power NOT accounted for.
DX Cooling Coil Standard Ratings 2017

| Cooling Coil Type (1) | Standard Rating Net Cooling Capacity [ton][2] | Standard Rating Net COP [Btuh/Btuh][2] | EER [Btu/W-h][2] | SEER User [Btu/W-h][2,3] | SEER Standard [Btu/W-h][2,3] | IEER [Btu/W-h][2]
DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed | 1.9 | 3.42 | 11.67 | 12.37 | 11.89 | 12.1

ANSI/AHRI ratings account for supply air fan heat and electric power.

1. EnergyPlus object type.
2. Capacity less than 65K Btu/h (19050 W) - calculated as per AHRI Standard 210/240-2017.
   Capacity of 65K Btu/h (19050 W) to less than 135K Btu/h (39565 W) - calculated as per AHRI Standard 340/360-2007.
   Capacity from 135K (39565 W) to 250K Btu/hr (73268 W) - calculated as per AHRI Standard 365-2009 - Ratings not yet supported in EnergyPlus.
3. SEER (User) is calculated using user-input PLF curve and cooling coefficient of degradation.
   SEER (Standard) is calculated using the default PLF curve and cooling coefficient of degradation from the appropriate AHRI standard.

DX Cooling Coil Standard Ratings 2023

| Cooling Coil Type (1) | Standard Rating Net Cooling Capacity [ton][2] | Standard Rating Net COP2 [Btuh/Btuh][2,4] | EER2 [Btu/W-h][2,4] | SEER2 User [Btu/W-h][2,3] | SEER2 Standard [Btu/W-h][2,3] | IEER [Btu/W-h][2]
DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed | 1.8 | 3.30 | 11.26 | 11.93 | 11.79 | 11.5

ANSI/AHRI ratings account for supply air fan heat and electric power.

1. EnergyPlus object type.
2. Capacity less than 65K Btu/h (19050 W) - calculated as per AHRI Standard 210/240-2023.
   Capacity of 65K Btu/h (19050 W) to less than 135K Btu/h (39565 W) - calculated as per AHRI Standard 340/360-2022.
   Capacity from 135K (39565 W) to 250K Btu/hr (73268 W) - calculated as per AHRI Standard 365-2009 - Ratings not yet supported in EnergyPlus.
3. SEER2 (User) is calculated using user-input PLF curve and cooling coefficient of degradation.
   SEER2 (Standard) is calculated using the default PLF curve and cooling coefficient of degradation from the appropriate AHRI standard.
4. Value for the Full Speed of the coil.

DX Cooling Coil ASHRAE 127 Standard Ratings Report

| DX Cooling Coil Type | Rated Net Cooling Capacity Test A [ton] | Rated Electric Power Test A [W] | Rated Net Cooling Capacity Test B [ton] | Rated Electric Power Test B [W] | Rated Net Cooling Capacity Test C [ton] | Rated Electric Power Test C [W] | Rated Net Cooling Capacity Test D [ton] | Rated Electric Power Test D [W]
None |  |  |  |  |  |  |  |  |

Water-to-Air Heat Pumps at Rated Temperatures Report

| Coil Type | Rated Total Capacity [Btu/h] | Rated Sensible Capacity [Btu/h] | Rated Power[Btu/h] | Rated COP [Btuh/Btuh] | Rated Air Dry-bulb Temperature [F] | Rated Air Wet-bulb Temperature [F] | Rated Water Temperature [F] | Design Day used for Sizing
None |  |  |  |  |  |  |  |  |

DX Heating Coils

| DX Heating Coil Type | High Temperature Heating (net) Rating Capacity [Btu/h] | Low Temperature Heating (net) Rating Capacity [Btu/h] | HSPF [Btu/W-h] | Region Number | Minimum Outdoor Dry-Bulb Temperature for Compressor Operation [F] | Supplemental Heat High Shutoff Temperature [F] | Airloop Name
MAIN DX HEATING COIL_UNIT1 |  |  |  |  |  |  | 69.80 |

DX Heating Coils AHRI 2023

| DX Heating Coil Type | High Temperature Heating (net) Rating Capacity [Btu/h] | Low Temperature Heating (net) Rating Capacity [Btu/h] | HSPF2 [Btu/W-h] | Region Number | Minimum Outdoor Dry-Bulb Temperature for Compressor Operation [F] | Airloop Name
None |  |  |  |  |  |  |

Heating Coils

| Type | Design Coil Load [Btu/h] | Nominal Total Capacity [Btu/h] | Nominal Efficiency [Btuh/Btuh] | Used as Supplementary Heat | Airloop Name | Plantloop Name
MAIN DX HEATING COIL_UNIT1 | Coil:Heating:Water | 35350.81 | 69088.21 | - | No | CENTRAL SYSTEM_UNIT1 | GAHP_LOOP
SUPP HEATING COIL_UNIT1 | Coil:Heating:Fuel |  | 44188.51 | 0.80 | Yes | CENTRAL SYSTEM_UNIT1 | N/A

Nominal values are gross at rated conditions, i.e., the supply air fan heat and electric power NOT accounted for.
Fans

| Type | Total Efficiency [Btuh/Btuh] | Delta Pressure [psi] | Max Air Flow Rate [ft3/min] | Rated Electricity Rate [W] | Rated Power Per Max Air Flow Rate [W-min/ft3] | Motor Heat In Air Fraction | Fan Energy Index | End Use Subcategory | Design Day Name for Fan Sizing Peak | Date/Time for Fan Sizing Peak | Purpose | Is Autosized | Motor Efficiency | Motor Heat to Zone Fraction | Motor Loss Zone Name | Airloop Name
OASUPPLYFAN_UNIT1 | Fan:OnOff | 0.60 | 0.15 | 59.99 | 50.00 | 0.83 | 0.00 | 7.76 | Ventilation |  |  | N/A | Yes | 1.00 | 0.00 | N/A | N/A
OAEXHAUSTFAN_UNIT1 | Fan:OnOff | 0.60 | 0.15 | 59.99 | 50.00 | 0.83 | 0.00 | 7.76 | Ventilation |  |  | N/A | Yes | 1.00 | 0.00 | N/A | N/A
SUPPLY FAN_UNIT1 | Fan:SystemModel | 1260.73 | 147.23 | 692.47 | 263.17 | 0.38 | 1.00 | 2815.73 | General | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | N/A | Yes | 0.85 | 0.00 | N/A | CENTRAL SYSTEM_UNIT1

Pumps

| Type | Control | Head [psi] | Water Flow [gal/min] | Electricity Rate [W] | Power Per Water Flow Rate [W-min/gal] | Motor Efficiency [Btuh/Btuh] | End Use Subcategory | Is Autosized | Plantloop Name | Plantloop Branch Name
GAHP_PUMP | Pump:VariableSpeed | Intermittent | 26.01 | 2.558659 | 41.24 | 16.12 | 0.90 | General | Yes | GAHP_LOOP | GAHP_PUMP_BRANCH
MAINS PRESSURE_UNIT1 | Pump:VariableSpeed | Intermittent | 0.00 | 7.827838 | 0.00 | 0.00 | 1.00 | General | Yes | DHW LOOP_UNIT1 | MAINS INLET BRANCH_UNIT1

Service Water Heating

| Type | Storage Volume [ft3] | Input [Btu/h] | Thermal Efficiency [Btuh/Btuh] | Recovery Efficiency [Btuh/Btuh] | Energy Factor
WATER HEATER_UNIT1 | WaterHeater:Mixed | 6.95 | 38002.17 | 0.80 | 0.82 | 0.60

Chillers

| Type | Reference Capacity[Btu/h] | TypeReference Efficiency [Btuh/Btuh] | Rated Capacity [Btu/h] | Rated Efficiency [Btuh/Btuh] | IPLV in SI Units [W/W] | IPLV in IP Units [Btu/W-h] | Minimum Part Load Ratio | Fuel Type | Rated Entering Condenser Temperature [F] | Rated Leaving Evaporator Temperature [F] | Reference Entering Condenser Temperature [F] | Reference Leaving Evaporator Temperature [F] | Design Size Reference Chilled Water Flow Rate [lb/s] | Design Size Reference Condenser Fluid Flow Rate [lb/s] | Plantloop Name | Plantloop Branch Name | Condenser Loop Name | Condenser Loop Branch Name | Heat Recovery Plantloop Name | Heat Recovery Plantloop Branch Name | Recovery Relative Capacity Fraction
None |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Boilers

| Type | Reference Capacity [Btu/h] | Reference Efficiency[Btuh/Btuh] | Rated Capacity [Btu/h] | Rated Efficiency [Btuh/Btuh] | Minimum Part Load Ratio | Fuel Type | Parasitic Electric Load [W] | Plantloop Name | Plantloop Branch Name
GAHP | Boiler:HotWater | 44188.51 | 1.00 | 44188.51 | 1.00 | 0.00 | NaturalGas | 0.00 | GAHP_LOOP | GAHP_BRANCH

Cooling Towers and Fluid Coolers

| Type | Fluid Type | Range [F] | Approach [F] | Design Fan Power [Btu/h] | Design Inlet Air Wet-Bulb Temperature [F] | Design Water Flow Rate [gal/min] | Leaving Water Setpoint Temperature [F] | Condenser Loop Name | Condenser Loop Branch Name
None |  |  |  |  |  |  |  |  |  |

PlantLoop or CondenserLoop

| Type | Provides Heating | Provides Cooling | Maximum Loop Flow Rate [ft3/min] | Minimum Loop Flow Rate [ft3/min]
GAHP_LOOP | PlantLoop | Yes | Yes | 0.34 | 0.00
DHW LOOP_UNIT1 | PlantLoop | Yes | Yes | 1.05 | 0.00

Air Terminals

| Zone Name | Minimum Flow [ft3/min] | Minimum Outdoor Flow [ft3/min] | Supply Cooling Setpoint [F] | Supply Heating Setpoint [F] | Heating Capacity [Btu/h] | Cooling Capacity [ton] | Type of Input Object | Heat/Reheat Coil Object Type | Chilled Water Coil Object Type | Fan Object Type | Fan Name | Primary Air Flow Rate [ft3/min] | Secondary Air Flow Rate [ft3/min] | Minimum Flow Schedule Name | Maximum Flow During Reheat [ft3/min] | Minimum Outdoor Flow Schedule Name
ZONEDIRECTAIR_UNIT1 | LIVING_UNIT1 | 356.49 | 59.99 | 53.60 | 104.00 | 16579.66 | 1.29 | AirTerminal:SingleDuct:ConstantVolume:NoReheat |  | n/a | n/a |  | 692.47 | n/a | n/a | 0.00 | n/a

Air Heat Recovery

| Name | Input object type | Plate/Rotary | Sensible Effectiveness at 100% Heating Air Flow | Sensible Effectiveness at 100% Cooling Air Flow | Latent Effectiveness at 100% Heating Air Flow | Latent Effectiveness at 100% Cooling Air Flow | Exhaust Airflow [lb/s] | Outdoor Airflow [lb/s]
OA_HEAT_RECOVERY_UNIT1 | OA_HEAT_RECOVERY_UNIT1 | Generic | Rotary | 0.64 | 0.64 | 0.00 | 0.00 | 0.00 | 0.00

Table of Contents

Report: HVAC Sizing Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Space Sensible Cooling

| Calculated Design Load [Btu/h] | User Design Load [Btu/h] | User Design Load per Area [Btu/h-ft2] | Calculated Design Air Flow [ft3/min] | User Design Air Flow [ft3/min] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [F] | Indoor Temperature at Peak Load [F] | Indoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Outdoor Temperature at Peak Load [F] | Outdoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Minimum Outdoor Air Flow Rate [ft3/min] | Heat Gain Rate from DOAS [Btu/h]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the space sensible load only. It does not include any system effects or ventilation loads.
Zone Sensible Cooling

| Calculated Design Load [Btu/h] | User Design Load [Btu/h] | User Design Load per Area [Btu/h-ft2] | Calculated Design Air Flow [ft3/min] | User Design Air Flow [ft3/min] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [F] | Indoor Temperature at Peak Load [F] | Indoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Outdoor Temperature at Peak Load [F] | Outdoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Minimum Outdoor Air Flow Rate [ft3/min] | Heat Gain Rate from DOAS [Btu/h]
LIVING_UNIT1 | 15513.88 | 15513.88 | 6.53 | 692.472 | 692.472 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | 75.00 | 75.00 | 0.00771 | 83.58 | 0.01536 | 59.993 | 0.00

The Design Load is the zone sensible load only. It does not include any system effects or ventilation loads.
Space Sensible Heating

| Calculated Design Load [Btu/h] | User Design Load [Btu/h] | User Design Load per Area [Btu/h-ft2] | Calculated Design Air Flow [ft3/min] | User Design Air Flow [ft3/min] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [F] | Indoor Temperature at Peak Load [F] | Indoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Outdoor Temperature at Peak Load [F] | Outdoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Minimum Outdoor Air Flow Rate [ft3/min] | Heat Gain Rate from DOAS [Btu/h]
None |  |  |  |  |  |  |  |  |  |  |  |  |  |

The Design Load is the space sensible load only. It does not include any system effects or ventilation loads.
Zone Sensible Heating

| Calculated Design Load [Btu/h] | User Design Load [Btu/h] | User Design Load per Area [Btu/h-ft2] | Calculated Design Air Flow [ft3/min] | User Design Air Flow [ft3/min] | Design Day Name | Date/Time Of Peak {TIMESTAMP} | Thermostat Setpoint Temperature at Peak Load [F] | Indoor Temperature at Peak Load [F] | Indoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Outdoor Temperature at Peak Load [F] | Outdoor Humidity Ratio at Peak Load [lbWater/lbDryAir] | Minimum Outdoor Air Flow Rate [ft3/min] | Heat Gain Rate from DOAS [Btu/h]
LIVING_UNIT1 | 16579.66 | 16579.66 | 6.97 | 494.458 | 494.458 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | 72.00 | 72.00 | 0.00814 | -15.2 | 0.00036 | 59.993 | 0.00

The Design Load is the zone sensible load only. It does not include any system effects or ventilation loads.
System Design Air Flow Rates

| Calculated cooling [ft3/min] | User cooling [ft3/min] | Calculated heating [ft3/min] | User heating [ft3/min] | Adjusted cooling [ft3/min] | Adjusted heating [ft3/min] | Adjusted main [ft3/min] | Calculated Heating Air Flow Ratio [] | User Heating Air Flow Ratio []
CENTRAL SYSTEM_UNIT1 | 692.47 | 692.47 | 494.46 | 494.46 | 692.4717 | 692.4717 | 692.4717 | 1.0000 | 1.0000

Plant Loop Coincident Design Fluid Flow Rate Adjustments

| Previous Design Volume Flow Rate [ft3/min] | Algorithm Volume Flow Rate [ft3/min] | Coincident Design Volume Flow Rate [ft3/min] | Coincident Size Adjusted | Peak Sizing Period Name | Peak Day into Period {TIMESTAMP}[day] | Peak Hour Of Day {TIMESTAMP}[hr] | Peak Step Start Minute {TIMESTAMP}[min]
None |  |  |  |  |  |  |  |

Coil Sizing Summary

| Coil Type | HVAC Type | HVAC Name | Coil Final Gross Total Capacity [Btu/h] | Coil Final Gross Sensible Capacity [Btu/h] | Coil Final Reference Air Volume Flow Rate [ft3/min] | Coil Final Reference Plant Fluid Volume Flow Rate [ft3/min] | Coil U-value Times Area Value [Btu/h-F] | Design Day Name at Sensible Ideal Loads Peak | Date/Time at Sensible Ideal Loads Peak | Design Day Name at Air Flow Ideal Loads Peak | Date/Time at Air Flow Ideal Loads Peak | Coil Total Capacity at Ideal Loads Peak [Btu/h] | Coil Sensible Capacity at Ideal Loads Peak [Btu/h] | Coil Air Volume Flow Rate at Ideal Loads Peak [ft3/min] | Coil Entering Air Drybulb at Ideal Loads Peak [F] | Coil Entering Air Wetbulb at Ideal Loads Peak [F] | Coil Entering Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Coil Leaving Air Drybulb at Ideal Loads Peak [F] | Coil Leaving Air Wetbulb at Ideal Loads Peak [F] | Coil Leaving Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Outdoor Air Drybulb at Ideal Loads Peak [F] | Outdoor Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Outdoor Air Wetbulb at Ideal Loads Peak [F] | Outdoor Air Flow Percentage at Ideal Loads Peak [%] | Zone Air Drybulb at Ideal Loads Peak [F] | Zone Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Zone Air Relative Humidity at Ideal Loads Peak [%] | Zone Sensible Heat Gain at Ideal Loads Peak [Btu/h] | Zone Latent Heat Gain at Ideal Loads Peak [Btu/h] | Coil Total Capacity at Rating Conditions [Btu/h] | Coil Sensible Capacity at Rating Conditions [Btu/h]
MAIN DX HEATING COIL_UNIT1 | COIL:HEATING:WATER | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | 35350.807 | 35350.807 | 692.471728 | 0.34196867 | 2159.712 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | 35350.81 | 28698.67 | 692.471728 | 64.45 | 54.97 | 0.00746666 | 104.00 | 69.14 | 0.00800000 | -15.2 | 0.00036134 | -15.2 | 8.6636 | 72.00 | 0.00814063 | 46.5678 | 16579.66 | 0.00 | 69182.70 | 69182.70
DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | 23176.290 | 17656.793 | 692.471728 | -999. | -999.00 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | 22771.83 | 20026.86 | 692.471728 | 76.98 | 61.06 | 0.00837415 | 53.60 | 50.60 | 0.00750000 | 83.58 | 0.01536037 | 72.39 | 8.6636 | 75.00 | 0.00771148 | 39.9102 | 15513.88 | 0.00 | 23185.96 | 17248.60
SUPP HEATING COIL_UNIT1 | COIL:HEATING:FUEL | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | 44188.508 | 44188.508 | -999. | -999. | -999.00 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | 44188.51 | 28698.67 | 692.471728 | 64.45 | 54.97 | 0.00746666 | 104.00 | 69.14 | 0.00800000 | -15.2 | 0.00036134 | -15.2 | 8.6636 | 72.00 | 0.00814063 | 46.5678 | 16579.66 | 0.00 | -999.0 | -999.0

Table of Contents

Report: Coil Sizing Details

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Coils

| Coil Type | Coil Location | HVAC Type | HVAC Name | Zone Name(s) | System Sizing Method Concurrence | System Sizing Method Capacity | System Sizing Method Air Flow | Autosized Coil Capacity? | Autosized Coil Airflow? | Autosized Coil Water Flow? | OA Pretreated prior to coil inlet? | Coil Final Gross Total Capacity [Btu/h] | Coil Final Gross Sensible Capacity [Btu/h] | Coil Final Reference Air Volume Flow Rate [ft3/min] | Coil Final Reference Plant Fluid Volume Flow Rate [ft3/min] | Coil U-value Times Area Value [Btu/h-F] | Terminal Unit Reheat Coil Multiplier | DX Coil Capacity Increase Ratio from Too Low Flow/Capacity Ratio | DX Coil Capacity Decrease Ratio from Too High Flow/Capacity Ratio | Moist Air Heat Capacity [Btu/lbm-R] | Dry Air Heat Capacity [Btu/lbm-R] | Standard Air Density Adjusted for Elevation [lb/ft3] | Supply Fan Name for Coil | Supply Fan Type for Coil | Supply Fan Maximum Air Volume Flow Rate [ft3/min] | Supply Fan Maximum Air Mass Flow Rate [lb/s] | Plant Name for Coil | Plant Fluid Specific Heat Capacity [Btu/lbm-R] | Plant Fluid Density [lb/ft3] | Plant Maximum Fluid Mass Flow Rate [lb/s] | Plant Design Fluid Return Temperature [F] | Plant Design Fluid Supply Temperature [F] | Plant Design Fluid Temperature Difference [deltaF] | Plant Design Capacity [Btu/h] | Coil Capacity Percentage of Plant Design Capacity [%] | Coil Fluid Flow Rate Percentage of Plant Design Flow Rate [%] | Design Day Name at Sensible Ideal Loads Peak | Date/Time at Sensible Ideal Loads Peak | Design Day Name at Total Ideal Loads Peak | Date/Time at Total Ideal Loads Peak | Design Day Name at Air Flow Ideal Loads Peak | Date/Time at Air Flow Ideal Loads Peak | Peak Load Type to Size On | Coil Total Capacity at Ideal Loads Peak [Btu/h] | Coil Sensible Capacity at Ideal Loads Peak [Btu/h] | Coil Off-Rating Capacity Modifier at Ideal Loads Peak [] | Coil Air Mass Flow Rate at Ideal Loads Peak [lb/s] | Coil Air Volume Flow Rate at Ideal Loads Peak [ft3/min] | Coil Entering Air Drybulb at Ideal Loads Peak [F] | Coil Entering Air Wetbulb at Ideal Loads Peak [F] | Coil Entering Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Coil Entering Air Enthalpy at Ideal Loads Peak [Btu/lb] | Coil Leaving Air Drybulb at Ideal Loads Peak [F] | Coil Leaving Air Wetbulb at Ideal Loads Peak [F] | Coil Leaving Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Coil Leaving Air Enthalpy at Ideal Loads Peak [Btu/lb] | Coil Plant Fluid Mass Flow Rate at Ideal Loads Peak [lb/s] | Coil Entering Plant Fluid Temperature at Ideal Loads Peak [F] | Coil Leaving Plant Fluid Temperature at Ideal Loads Peak [F] | Coil Plant Fluid Temperature Difference at Ideal Loads Peak [deltaF] | Supply Fan Air Heat Gain at Ideal Loads Peak [Btu/h] | Coil and Fan Net Total Capacity at Ideal Loads Peak [Btu/h] | Outdoor Air Drybulb at Ideal Loads Peak [F] | Outdoor Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Outdoor Air Wetbulb at Ideal Loads Peak [F] | Outdoor Air Volume Flow Rate at Ideal Loads Peak [ft3/min] | Outdoor Air Flow Percentage at Ideal Loads Peak [%] | System Return Air Drybulb at Ideal Loads Peak [F] | System Return Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Zone Air Drybulb at Ideal Loads Peak [F] | Zone Air Humidity Ratio at Ideal Loads Peak [lbWater/lbDryAir] | Zone Air Relative Humidity at Ideal Loads Peak [%] | Zone Sensible Heat Gain at Ideal Loads Peak [Btu/h] | Zone Latent Heat Gain at Ideal Loads Peak [Btu/h] | Coil Total Capacity at Rating Conditions [Btu/h] | Coil Sensible Capacity at Rating Conditions [Btu/h] | Coil Air Mass Flow Rate at Rating Conditions [lb/s] | Coil Entering Air Drybulb at Rating Conditions [F] | Coil Entering Air Wetbulb at Rating Conditions [F] | Coil Entering Air Humidity Ratio at Rating Conditions [lbWater/lbDryAir] | Coil Entering Air Enthalpy at Rating Conditions [Btu/lb] | Coil Leaving Air Drybulb at Rating Conditions [F] | Coil Leaving Air Wetbulb at Rating Conditions [F] | Coil Leaving Air Humidity Ratio at Rating Conditions [lbWater/lbDryAir] | Coil Leaving Air Enthalpy at Rating Conditions [Btu/lb]
MAIN DX HEATING COIL_UNIT1 | COIL:HEATING:WATER | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | Non-Coincident | FractionOfAutosizedHeatingCapacity | N/A | Yes | Yes | Yes | No | 35350.807 | 35350.807 | 692.471728 | 0.34196867 | 2159.712 | -999.0000 | 1.00000 | 1.00000 | 0.2436 | 0.2400 | 0.0717 | SUPPLY FAN_UNIT1 | Fan:SystemModel | 692.471728 | 0.82761054 |  | 1.0027 | 62.4216 | 0.35580650 | 89.96 | 125.06 | 35.10 | 45077.82 | 78.4217 | 100.000000 | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | unknown | unknown | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | Sensible | 35350.81 | 28698.67 | 1.0000 | 0.82761054 | 692.471728 | 64.45 | 54.97 | 0.00746666 | 23.6 | 104.00 | 69.14 | 0.00800000 | 33.8 | 0.35580650 | 140.00 | 104.90 | 35.10 | 0.000 | 35350.81 | -15.2 | 0.00036134 | -15.2 | 59.99331233 | 8.6636 | 72.00 | 0.00814063 | 72.00 | 0.00814063 | 46.5678 | 16579.66 | 0.00 | 69182.70 | 69182.70 | 0.82761054 | 61.88 | 54.73 | 0.00746666 | 23.0 | 157.32 | 83.14 | 0.00746666 | 46.2
DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | Non-Coincident | FractionOfAutosizedCoolingCapacity | N/A | Yes | Yes | unknown | No | 23176.290 | 17656.793 | 692.471728 | -999. | -999.00 | -999.0000 | 1.00000 | 1.00000 | 0.2437 | 0.2400 | 0.0717 | SUPPLY FAN_UNIT1 | Fan:SystemModel | 692.471728 | 0.82761054 |  | -999.000 | -999.000 | -999. | -999.0 | -999.0 | -999.0 | -999.0 | -999.000 | -999. | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | ROCHESTER INTERNATIONAL ARPT ANN CLG .4% CONDNS DB=>MWB | 7/21 18:00:00 | Sensible | 22771.83 | 20026.86 | 0.9825 | 0.82761054 | 692.471728 | 76.98 | 61.06 | 0.00837415 | 27.6 | 53.60 | 50.60 | 0.00750000 | 21.0 | -999. | -999.0 | -999.0 | -999.0 | 897.931 | 21873.90 | 83.58 | 0.01536037 | 72.39 | 59.99331233 | 8.6636 | 75.00 | 0.00771148 | 75.00 | 0.00771148 | 39.9102 | 15513.88 | 0.00 | 23185.96 | 17248.60 | 0.79492618 | 80.00 | 67.00 | 0.01118466 | 31.4 | 55.31 | 55.29 | 0.00929249 | 23.3
SUPP HEATING COIL_UNIT1 | COIL:HEATING:FUEL | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | Non-Coincident | FractionOfAutosizedHeatingCapacity | N/A | Yes | Yes | unknown | No | 44188.508 | 44188.508 | -999. | -999. | -999.00 | -999.0000 | 1.00000 | 1.00000 | 0.2436 | 0.2400 | 0.0717 | SUPPLY FAN_UNIT1 | Fan:SystemModel | 692.471728 | 0.82761054 |  | -999.000 | -999.000 | -999. | -999.0 | -999.0 | -999.0 | -999.0 | -999.000 | -999. | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | unknown | unknown | ROCHESTER INTERNATIONAL ARPT ANN HTG 99.6% CONDNS DB | 1/21 14:00:00 | Sensible | 44188.51 | 28698.67 | 1.0000 | 0.82761054 | 692.471728 | 64.45 | 54.97 | 0.00746666 | 23.6 | 104.00 | 69.14 | 0.00800000 | 33.8 | -999. | -999.0 | -999.0 | -999.0 | 0.000 | 44188.51 | -15.2 | 0.00036134 | -15.2 | 59.99331233 | 8.6636 | 72.00 | 0.00814063 | 72.00 | 0.00814063 | 46.5678 | 16579.66 | 0.00 | -999.0 | -999.0 | -999. | -999.0 | -999.0 | -999. | -999. | -999.0 | -999.0 | -999. | -999.

Coil Connections

| Coil Name | Coil Type | Coil Location | HVAC Type | HVAC Name | Zone Name(s) | Supply Fan Name for HVAC | Supply Fan Type for HVAC | Airloop Name | Plant Name for Coil | Plant Loop Name
MAIN DX HEATING COIL_UNIT1 | MAIN DX HEATING COIL_UNIT1 | COIL:HEATING:WATER | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | SUPPLY FAN_UNIT1 | Fan:SystemModel | CENTRAL SYSTEM_UNIT1 | GAHP_LOOP | GAHP_LOOP
DX COOLING COIL_UNIT1 | DX COOLING COIL_UNIT1 | Coil:Cooling:DX:SingleSpeed | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | SUPPLY FAN_UNIT1 | Fan:SystemModel | CENTRAL SYSTEM_UNIT1 | unknown | unknown
SUPP HEATING COIL_UNIT1 | SUPP HEATING COIL_UNIT1 | COIL:HEATING:FUEL | AirLoop | AirLoopHVAC | CENTRAL SYSTEM_UNIT1 | LIVING_UNIT1 | SUPPLY FAN_UNIT1 | Fan:SystemModel | CENTRAL SYSTEM_UNIT1 | unknown | unknown

Table of Contents

Report: System Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Economizer

| High Limit Shutoff Control | Minimum Outdoor Air [ft3/min] | Maximum Outdoor Air [ft3/min] | Return Air Temp Limit | Return Air Enthalpy Limit | Outdoor Air Temperature Limit [F] | Outdoor Air Enthalpy Limit [F]
None |  |  |  |  |  |  |

Demand Controlled Ventilation using Controller:MechanicalVentilation

| Controller:MechanicalVentilation Name | Outdoor Air Per Person [ft3/min-person] | Outdoor Air Per Area [ft3/min-ft2] | Outdoor Air Per Zone [ft3/min] | Outdoor Air ACH [ACH] | Outdoor Air Method | Outdoor Air Schedule Name | Air Distribution Effectiveness in Cooling Mode | Air Distribution Effectiveness in Heating Mode | Air Distribution Effectiveness Schedule Name | Type
None |  |  |  |  |  |  |  |  |  |  |

Time Not Comfortable Based on Simple ASHRAE 55-2004

| Winter Clothes [hr] | Summer Clothes [hr] | Summer or Winter Clothes [hr]
LIVING_UNIT1 | 3245.00 | 5767.17 | 1416.17
GARAGE1 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00
Facility | 3245.00 | 5767.17 | 1416.17

Aggregated over the RunPeriods for Weather
Time Setpoint Not Met

| During Heating [hr] | During Cooling [hr] | During Occupied Heating [hr] | During Occupied Cooling [hr]
LIVING_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00
Facility | 0.00 | 0.00 | 0.00 | 0.00

Aggregated over the RunPeriods for Weather
Thermostat Schedules

| Thermostat Name 1 | Control Type Schedule | Control Type | Control Type Name | Heating Schedule | Cooling Schedule
LIVING_UNIT1 | ZONE THERMOSTAT_UNIT1 | ZONE_CONTROL_TYPE | DualSetPointWithDeadBand | THERMOSTAT_LIVING DUAL SP CONTROL | HEATING_SCH | COOLING_SCH

Table of Contents

Report: HVAC Topology

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Air Loop Supply Side Component Arrangement

| Airloop Name | Splitter Name | Supply Branch Name | Supply Branch Type | Component Type | Component Name | Sub-Component Type | Sub-Component Name | Sub-Sub-Component Type | Sub-Sub-Component Name | Mixer Name
1 | CENTRAL SYSTEM_UNIT1 |  |  |  |  |  |  |  |  |  |
2 | CENTRAL SYSTEM_UNIT1 |  | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:UNITARYSYSTEM | GAHP_AHU_UNIT1 |  |  |  |  |
3 | CENTRAL SYSTEM_UNIT1 |  | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:UNITARYSYSTEM | GAHP_AHU_UNIT1 | FAN:SYSTEMMODEL | SUPPLY FAN_UNIT1 |  |  |
4 | CENTRAL SYSTEM_UNIT1 |  | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:UNITARYSYSTEM | GAHP_AHU_UNIT1 | COIL:COOLING:DX:SINGLESPEED | DX COOLING COIL_UNIT1 |  |  |
5 | CENTRAL SYSTEM_UNIT1 |  | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:UNITARYSYSTEM | GAHP_AHU_UNIT1 | COIL:HEATING:WATER | MAIN DX HEATING COIL_UNIT1 |  |  |
6 | CENTRAL SYSTEM_UNIT1 |  | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:UNITARYSYSTEM | GAHP_AHU_UNIT1 | COIL:HEATING:FUEL | SUPP HEATING COIL_UNIT1 |  |  |

Air Loop Demand Side Component Arrangement

| Airloop Name | Supply Branch Name | Supply Branch Type | Supply Path Component Type | Supply Path Component Name | Terminal Unit Type | Terminal Unit Name | Zone Name | Return Path Component Type | Return Path Component Name
1 | CENTRAL SYSTEM_UNIT1 |  |  |  |  |  |  |  |  |
2 | CENTRAL SYSTEM_UNIT1 | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:ZONESPLITTER | ZONE SUPPLY AIR SPLITTER_UNIT1 |  |  |  |  |
3 | CENTRAL SYSTEM_UNIT1 | AIR LOOP MAIN BRANCH_UNIT1 | Main | AIRLOOPHVAC:ZONESPLITTER | ZONE SUPPLY AIR SPLITTER_UNIT1 | AIRTERMINAL:SINGLEDUCT:CONSTANTVOLUME:NOREHEAT | ZONEDIRECTAIR_UNIT1 | LIVING_UNIT1 | AIRLOOPHVAC:ZONEMIXER | ZONE RETURN AIR MIXER_UNIT1
4 | CENTRAL SYSTEM_UNIT1 | AIR LOOP MAIN BRANCH_UNIT1 | Main |  |  |  |  |  | AIRLOOPHVAC:ZONEMIXER | ZONE RETURN AIR MIXER_UNIT1

Zone Equipment Component Arrangement

| Zone Name | Component Type | Component Name | Sub-Component Type | Sub-Component Name | Sub-Sub-Component Type | Sub-Sub-Component Name
1 | LIVING_UNIT1 |  |  |  |  |  |
2 | LIVING_UNIT1 | ZONEHVAC:ENERGYRECOVERYVENTILATOR | ERV_UNIT1 |  |  |  |
3 | LIVING_UNIT1 | ZONEHVAC:ENERGYRECOVERYVENTILATOR | ERV_UNIT1 | HEATEXCHANGER:AIRTOAIR:SENSIBLEANDLATENT | OA_HEAT_RECOVERY_UNIT1 |  |
4 | LIVING_UNIT1 | ZONEHVAC:ENERGYRECOVERYVENTILATOR | ERV_UNIT1 | FAN:ONOFF | OASUPPLYFAN_UNIT1 |  |
5 | LIVING_UNIT1 | ZONEHVAC:ENERGYRECOVERYVENTILATOR | ERV_UNIT1 | FAN:ONOFF | OAEXHAUSTFAN_UNIT1 |  |
6 | LIVING_UNIT1 | ZONEHVAC:AIRDISTRIBUTIONUNIT | ZONEDIRECTAIR_UNIT1 |  |  |  |
7 | LIVING_UNIT1 | ZONEHVAC:AIRDISTRIBUTIONUNIT | ZONEDIRECTAIR_UNIT1 | AIRTERMINAL:SINGLEDUCT:CONSTANTVOLUME:NOREHEAT | ZONEDIRECTAIR_UNIT1 |  |
8 | GARAGE1 |  |  |  |  |  |
9 | ATTIC_UNIT1 |  |  |  |  |  |
10 | CRAWLSPACE_UNIT1 |  |  |  |  |  |

Plant Loop Component Arrangement

| Loop Type | Loop Name | Side | Splitter Name | Branch Name | Component Type | Component Name | Mixer Name
1 | PlantLoop | GAHP_LOOP | Supply |  |  |  |  |
2 | PlantLoop | GAHP_LOOP | Supply |  | GAHP_PUMP_BRANCH | PUMP:VARIABLESPEED | GAHP_PUMP |
3 | PlantLoop | GAHP_LOOP | Supply | GAHP_SUPPLY_SPLITTER | GAHP_BRANCH | BOILER:HOTWATER | GAHP | GAHP_SUPPLY_MIXER
4 | PlantLoop | GAHP_LOOP | Supply | GAHP_SUPPLY_SPLITTER | GAHP_BYPASS_BRANCH | PIPE:ADIABATIC | GAHP_BYPASS_PIPE | GAHP_SUPPLY_MIXER
5 | PlantLoop | GAHP_LOOP | Supply |  | GAHP_SUPPLY_OUTLET_PIPE_BRANCH | PIPE:ADIABATIC | GAHP_SUPPLY_OUTLET_PIPE |
6 | PlantLoop | GAHP_LOOP | Demand |  |  |  |  |
7 | PlantLoop | GAHP_LOOP | Demand |  | GAHP_DEMAND_INLET_PIPE_BRANCH | PIPE:ADIABATIC | GAHP_DEMAND_INLET_PIPE |
8 | PlantLoop | GAHP_LOOP | Demand | GAHP_DEMAND_SPLITTER | GAHP_HEATING_COIL_UNIT1 BRANCH | COIL:HEATING:WATER | MAIN DX HEATING COIL_UNIT1 | GAHP_DEMAND_MIXER
9 | PlantLoop | GAHP_LOOP | Demand |  | GAHP_DEMAND_OUTLET_PIPE_BRANCH | PIPE:ADIABATIC | GAHP_DEMAND_OUTLET_PIPE |
10 | PlantLoop | DHW LOOP_UNIT1 | Supply |  |  |  |  |
11 | PlantLoop | DHW LOOP_UNIT1 | Supply |  | MAINS INLET BRANCH_UNIT1 | PUMP:VARIABLESPEED | MAINS PRESSURE_UNIT1 |
12 | PlantLoop | DHW LOOP_UNIT1 | Supply | DHW SUPPLY SPLITTER_UNIT1 | WATER HEATER BRANCH_UNIT1 | WATERHEATER:MIXED | WATER HEATER_UNIT1 | DHW SUPPLY MIXER_UNIT1
13 | PlantLoop | DHW LOOP_UNIT1 | Supply |  | DHW SUPPLY OUTLET BRANCH_UNIT1 | PIPE:INDOOR | DHW SUPPLY OUTLET PIPE_UNIT1 |
14 | PlantLoop | DHW LOOP_UNIT1 | Demand |  |  |  |  |
15 | PlantLoop | DHW LOOP_UNIT1 | Demand |  | DHW DEMAND INLET BRANCH_UNIT1 | PIPE:INDOOR | DHW DEMAND INLET PIPE_UNIT1 |
16 | PlantLoop | DHW LOOP_UNIT1 | Demand | DHW DEMAND SPLITTER_UNIT1 | WATER SINK BRANCH_UNIT1 | WATERUSE:CONNECTIONS | DHW SINKS_UNIT1 | DHW DEMAND MIXER_UNIT1
17 | PlantLoop | DHW LOOP_UNIT1 | Demand | DHW DEMAND SPLITTER_UNIT1 | WATER SHOWER BRANCH_UNIT1 | WATERUSE:CONNECTIONS | DHW SHOWERS_UNIT1 | DHW DEMAND MIXER_UNIT1
18 | PlantLoop | DHW LOOP_UNIT1 | Demand | DHW DEMAND SPLITTER_UNIT1 | WATER CLOTHESWASHER BRANCH_UNIT1 | WATERUSE:CONNECTIONS | DHW CLOTHESWASHER_UNIT1 | DHW DEMAND MIXER_UNIT1
19 | PlantLoop | DHW LOOP_UNIT1 | Demand | DHW DEMAND SPLITTER_UNIT1 | WATER DISHWASHER BRANCH_UNIT1 | WATERUSE:CONNECTIONS | DHW DISHWASHER_UNIT1 | DHW DEMAND MIXER_UNIT1
20 | PlantLoop | DHW LOOP_UNIT1 | Demand | DHW DEMAND SPLITTER_UNIT1 | WATER BATH BRANCH_UNIT1 | WATERUSE:CONNECTIONS | DHW BATHS_UNIT1 | DHW DEMAND MIXER_UNIT1
21 | PlantLoop | DHW LOOP_UNIT1 | Demand |  | MAINS MAKEUP BRANCH_UNIT1 | PIPE:ADIABATIC | MAINS MAKEUP PIPE_UNIT1 |

Table of Contents

Report: Outdoor Air Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Average Outdoor Air During Occupied Hours

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume [ft3] | Mechanical Ventilation [ACH] | Infiltration [ACH] | AFN Infiltration [ACH] | Simple Ventilation [ACH]
LIVING_UNIT1 | 2.07 | 3.00 | 17050.56 | 0.204 | 0.000 | 0.000 | 0.000

Values shown for a single zone without multipliers
Minimum Outdoor Air During Occupied Hours

| Average Number of Occupants | Nominal Number of Occupants | Zone Volume [ft3] | Mechanical Ventilation [ACH] | Infiltration [ACH] | AFN Infiltration [ACH] | Simple Ventilation [ACH]
LIVING_UNIT1 | 2.07 | 3.00 | 17050.56 | 0.049 | 0.000 | 0.000 | 0.000

Values shown for a single zone without multipliers

Table of Contents

Report: Outdoor Air Details

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Mechanical Ventilation Parameters by Zone

| AirLoop Name | Average Number of Occupants | Nominal Number of Occupants | Zone Volume [ft3] | Zone Area [ft2] | Design Zone Outdoor Airflow - Voz [ft3/min] | Minimum Dynamic Target Ventilation - Voz-dyn-min [ft3/min]
LIVING_UNIT1 | CENTRAL SYSTEM_UNIT1 | 2.07 | 3.00 | 17050.56 | 2377.10 | 0.0000 | 0.000
Total Facility |  | 2.07 | 3.00 | 17050.56 | 2377.10 | 0.0000 | 0.000

Values shown for a single zone without multipliers. Total Facility includes multipliers.
Total Outdoor Air by Zone

| Mechanical Ventilation [ft3] | Natural Ventilation [ft3] | Total Ventilation [ft3] | Infiltration [ft3] | Total Ventilation and Infiltration [ft3] | Dynamic Target Ventilation - Voz-dyn [ft3] | Time Below Voz-dyn [hr] | Time At Voz-dyn [hr] | Time Above Voz-dyn [hr] | Time Above Zero When Unoccupied [hr]
LIVING_UNIT1 | 30039486.73 | 0.00 | 30039486.73 | 0.00 | 30039486.73 | 31713442.85 | 1701.17 | 7106.83 | 0.00 | 0.00
Total Facility | 30039486.73 | 0.00 | 30039486.73 | 0.00 | 30039486.73 | 31713442.85 | 1701.17 | 7106.83 | 0.00 | 0.00

Values shown for a single zone without multipliers. Total Facility includes multipliers.
Average Outdoor Air During Occupancy by Zone - Flow Rates

| Mechanical Ventilation [ft3/min] | Natural Ventilation [ft3/min] | Total Ventilation [ft3/min] | Infiltration [ft3/min] | Total Ventilation and Infiltration [ft3/min] | Dynamic Target Ventilation - Voz-dyn [ft3/min] | Time Below Voz-dyn [hr] | Time At Voz-dyn [hr] | Time Above Voz-dyn [hr]
LIVING_UNIT1 | 56.8266 | 0.0000 | 56.8266 | 0.0000 | 56.8266 | 59.9933 | 1701.17 | 7106.83 | 0.00
Total Facility | 56.8266 | 0.0000 | 56.8266 | 0.0000 | 56.8266 | 59.9933 | 1701.17 | 7106.83 | 0.00

Values shown for a single zone without multipliers. Total Facility includes multipliers.
Total Outdoor Air by AirLoop

| Mechanical Ventilation [ft3] | Natural Ventilation [ft3] | Total Ventilation [ft3] | Sum Zone Dynamic Target Ventilation - Voz-sum-dyn [ft3] | Time Below Voz-sum-dyn [hr] | Time At Voz-sum-dyn [hr] | Time Above Voz-sum-dyn [hr] | Time Above Zero When Unoccupied [hr]
CENTRAL SYSTEM_UNIT1 | 0.00 | 0.00 | 0.00 | 31713442.85 | 8808.00 | 0.00 | 0.00 | 0.00

Values shown include multipliers.
Average Outdoor Air During Occupancy by AirLoop

| Mechanical Ventilation [ft3/min] | Natural Ventilation [ft3/min] | Total Ventilation [ft3/min] | Sum Zone Dynamic Target Ventilation - Voz-sum-dyn [ft3/min] | Time Below Voz-sum-dyn [hr] | Time At Voz-sum-dyn [hr] | Time Above Voz-sum-dyn [hr]
CENTRAL SYSTEM_UNIT1 | 0.0000 | 0.0000 | 0.0000 | 59.9933 | 8808.00 | 0.00 | 0.00

Values shown include multipliers.
Outdoor Air Controller Limiting Factors by AirLoop

| No Limiting Factor [hr] | Limits and Scheduled Limits [hr] | Economizer [hr] | Exhaust Flow [hr] | Mixed Air Flow [hr] | High Humidity [hr] | Demand Controlled Ventilation [hr] | Night Ventilation [hr] | Demand Limiting [hr] | Energy Management System [hr]
CENTRAL SYSTEM_UNIT1 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Average Outdoor Air for Limiting Factors During Occupancy

| No Limiting Factor [ft3/min] | Limits and Scheduled Limits [ft3/min] | Economizer [ft3/min] | Exhaust Flow [ft3/min] | Mixed Air Flow [ft3/min] | High Humidity [ft3/min] | Demand Controlled Ventilation [ft3/min] | Night Ventilation [ft3/min] | Demand Limiting [ft3/min] | Energy Management System [ft3/min]
CENTRAL SYSTEM_UNIT1 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000

Values shown include multipliers.

Table of Contents

Report: Object Count Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Surfaces by Class

| Total | Outdoors
Wall | 25 | 23
Floor | 5 | 1
Roof | 6 | 4
Internal Mass | 1 | 0
Building Detached Shading | 0 | 0
Fixed Detached Shading | 0 | 0
Window | 8 | 8
Door | 4 | 2
Glass Door | 0 | 0
Shading | 4 | 4
Overhang | 2 | 2
Fin | 0 | 0
Tubular Daylighting Device Dome | 0 | 0
Tubular Daylighting Device Diffuser | 0 | 0

HVAC

| Count
HVAC Air Loops | 1
Conditioned Zones | 1
Unconditioned Zones | 3
Supply Plenums | 0
Return Plenums | 0

Input Fields

| Count
IDF Objects | 587
Defaulted Fields | 477
Fields with Defaults | 2274
Autosized Fields | 29
Autosizable Fields | 44
Autocalculated Fields | 39
Autocalculatable Fields | 81

Table of Contents

Report: Energy Meters

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Annual and Peak Values - Electricity

| Electricity Annual Value [kWh] | Electricity Minimum Value [W] | Timestamp of Minimum {TIMESTAMP} | Electricity Maximum Value [W] | Timestamp of Maximum {TIMESTAMP}
Electricity:Facility | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
Electricity:Building | 8878.99 | 598.96 | 02-JAN-03:10 | 1642.68 | 21-JAN-18:10
Electricity:Zone:LIVING_UNIT1 | 8878.99 | 598.96 | 02-JAN-03:10 | 1642.68 | 21-JAN-18:10
Electricity:SpaceType:GENERAL | 8878.99 | 598.96 | 02-JAN-03:10 | 1642.68 | 21-JAN-18:10
InteriorLights:Electricity | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
InteriorLights:Electricity:Zone:LIVING_UNIT1 | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
InteriorLights:Electricity:SpaceType:GENERAL | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
General:InteriorLights:Electricity | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
General:InteriorLights:Electricity:Zone:LIVING_UNIT1 | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
General:InteriorLights:Electricity:SpaceType:GENERAL | 1043.31 | 23.24 | 21-JAN-00:10 | 337.99 | 21-JAN-19:10
InteriorEquipment:Electricity | 7835.68 | 567.10 | 02-JAN-04:10 | 1337.70 | 21-JAN-18:10
InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 7835.68 | 567.10 | 02-JAN-04:10 | 1337.70 | 21-JAN-18:10
InteriorEquipment:Electricity:SpaceType:GENERAL | 7835.68 | 567.10 | 02-JAN-04:10 | 1337.70 | 21-JAN-18:10
dishwasher:InteriorEquipment:Electricity | 207.09 | 1.89 | 02-JAN-03:10 | 65.70 | 21-JAN-19:10
dishwasher:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 207.09 | 1.89 | 02-JAN-03:10 | 65.70 | 21-JAN-19:10
dishwasher:InteriorEquipment:Electricity:SpaceType:GENERAL | 207.09 | 1.89 | 02-JAN-03:10 | 65.70 | 21-JAN-19:10
refrigerator:InteriorEquipment:Electricity | 672.34 | 66.60 | 21-JAN-04:10 | 91.06 | 21-JAN-18:10
refrigerator:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 672.34 | 66.60 | 21-JAN-04:10 | 91.06 | 21-JAN-18:10
refrigerator:InteriorEquipment:Electricity:SpaceType:GENERAL | 672.34 | 66.60 | 21-JAN-04:10 | 91.06 | 21-JAN-18:10
clotheswasher:InteriorEquipment:Electricity | 105.82 | 1.01 | 02-JAN-02:10 | 28.48 | 21-JAN-09:10
clotheswasher:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 105.82 | 1.01 | 02-JAN-02:10 | 28.48 | 21-JAN-09:10
clotheswasher:InteriorEquipment:Electricity:SpaceType:GENERAL | 105.82 | 1.01 | 02-JAN-02:10 | 28.48 | 21-JAN-09:10
electric_dryer:InteriorEquipment:Electricity | 838.52 | 4.25 | 02-JAN-03:10 | 213.06 | 21-JAN-11:10
electric_dryer:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 838.52 | 4.25 | 02-JAN-03:10 | 213.06 | 21-JAN-11:10
electric_dryer:InteriorEquipment:Electricity:SpaceType:GENERAL | 838.52 | 4.25 | 02-JAN-03:10 | 213.06 | 21-JAN-11:10
electric_range:InteriorEquipment:Electricity | 607.40 | 5.84 | 21-JAN-02:10 | 248.15 | 21-JAN-17:10
electric_range:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 607.40 | 5.84 | 21-JAN-02:10 | 248.15 | 21-JAN-17:10
electric_range:InteriorEquipment:Electricity:SpaceType:GENERAL | 607.40 | 5.84 | 21-JAN-02:10 | 248.15 | 21-JAN-17:10
television:InteriorEquipment:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
television:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
television:InteriorEquipment:Electricity:SpaceType:GENERAL | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
electric_mels:InteriorEquipment:Electricity | 3376.45 | 293.39 | 21-JAN-09:10 | 567.46 | 21-JAN-20:10
electric_mels:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 3376.45 | 293.39 | 21-JAN-09:10 | 567.46 | 21-JAN-20:10
electric_mels:InteriorEquipment:Electricity:SpaceType:GENERAL | 3376.45 | 293.39 | 21-JAN-09:10 | 567.46 | 21-JAN-20:10
IECC_adj:InteriorEquipment:Electricity | 2028.06 | 176.23 | 21-JAN-09:10 | 340.85 | 21-JAN-20:10
IECC_adj:InteriorEquipment:Electricity:Zone:LIVING_UNIT1 | 2028.06 | 176.23 | 21-JAN-09:10 | 340.85 | 21-JAN-20:10
IECC_adj:InteriorEquipment:Electricity:SpaceType:GENERAL | 2028.06 | 176.23 | 21-JAN-09:10 | 340.85 | 21-JAN-20:10
Fans:Electricity | 1505.93 | 100.00 | 09-APR-09:10 | 339.45 | 04-AUG-15:30
Fans:Electricity:Zone:LIVING_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Ventilation (simple):Fans:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Ventilation (simple):Fans:Electricity:Zone:LIVING_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
ElectricityPurchased:Facility | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
ElectricityPurchased:Plant | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
Cogeneration:ElectricityPurchased | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
General:Cogeneration:ElectricityPurchased | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
ElectricitySurplusSold:Facility | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
ElectricitySurplusSold:Plant | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Cogeneration:ElectricitySurplusSold | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Cogeneration:ElectricitySurplusSold | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
ElectricityNet:Facility | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
ElectricityNet:Plant | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
Cogeneration:ElectricityNet | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
General:Cogeneration:ElectricityNet | 12224.77 | 742.69 | 20-MAR-03:10 | 3345.91 | 25-JUN-18:10
Electricity:HVAC | 3083.01 | 100.00 | 09-APR-09:10 | 1789.62 | 04-AUG-15:30
HeatRecovery:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:HeatRecovery:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Ventilation:Fans:Electricity | 880.80 | 100.00 | 09-APR-09:10 | 100.00 | 13-MAR-08:50
General:Fans:Electricity | 625.13 | 0.00 | 02-JAN-14:30 | 239.45 | 04-AUG-15:30
Cooling:Electricity | 1577.08 | 0.00 | 21-JAN-00:10 | 1450.17 | 04-AUG-15:30
General:Cooling:Electricity | 1577.08 | 0.00 | 21-JAN-00:10 | 1450.17 | 04-AUG-15:30
Heating:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Heating:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
ExteriorLights:Electricity | 212.55 | 0.92 | 21-JAN-09:10 | 50.41 | 21-JAN-19:10
Exterior-Lights:ExteriorLights:Electricity | 190.44 | 0.00 | 21-JAN-06:10 | 43.24 | 21-JAN-00:10
Garage-Lights:ExteriorLights:Electricity | 22.11 | 0.49 | 21-JAN-00:10 | 7.16 | 21-JAN-19:10
Electricity:Plant | 50.21 | 0.00 | 21-JUL-00:10 | 27.47 | 02-FEB-07:30
Boiler Parasitic:Heating:Electricity | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Pumps:Electricity | 50.21 | 0.00 | 21-JUL-00:10 | 27.47 | 02-FEB-07:30
General:Pumps:Electricity | 50.21 | 0.00 | 21-JUL-00:10 | 27.47 | 02-FEB-07:30

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Natural Gas

| Natural Gas Annual Value [therm] | Natural Gas Minimum Value [Btu/h] | Timestamp of Minimum {TIMESTAMP} | Natural Gas Maximum Value [Btu/h] | Timestamp of Maximum {TIMESTAMP}
NaturalGas:Facility | 234.33 | 0.00 | 21-JUL-00:10 | 18066.68 | 02-FEB-07:30
NaturalGas:HVAC | 0.06 | 0.00 | 21-JAN-00:10 | 14.55 | 19-JAN-10:10
Heating:NaturalGas | 234.33 | 0.00 | 21-JUL-00:10 | 18066.68 | 02-FEB-07:30
General:Heating:NaturalGas | 234.33 | 0.00 | 21-JUL-00:10 | 18066.68 | 02-FEB-07:30
NaturalGas:Plant | 234.27 | 0.00 | 21-JUL-00:10 | 18066.68 | 02-FEB-07:30
Boiler Parasitic:Heating:NaturalGas | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Cooling

| Cooling Annual Value [ton-hrs] | Cooling Minimum Value [ton] | Timestamp of Minimum {TIMESTAMP} | Cooling Maximum Value [ton] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Water

| Annual Value [ft3] | Minimum Value [ft3/min] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [ft3/min] | Timestamp of Maximum {TIMESTAMP}
Water:Facility | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
Water:Plant | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
WaterSystems:Water | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
Domestic Hot Water:WaterSystems:Water | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
MainsWater:Facility | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
MainsWater:Plant | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
WaterSystems:MainsWater | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
Domestic Hot Water:WaterSystems:MainsWater | 1998.36 | 0.00 | 02-JAN-02:20 | 0.01 | 21-JUL-08:20
Water Heater:WaterSystems:Water | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Water Heater:WaterSystems:MainsWater | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other by Weight/Mass

| Annual Value [lb] | Minimum Value [lb/s] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [lb/s] | Timestamp of Maximum {TIMESTAMP}
Carbon Equivalent:Facility | 0.00 | 0.000 | 21-JAN-00:10 | 0.000 | 21-JAN-00:10
CarbonEquivalentEmissions:Carbon Equivalent | 0.00 | 0.000 | 21-JAN-00:10 | 0.000 | 21-JAN-00:10

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other Volumetric

| Annual Value [ft3] | Minimum Value [ft3/min] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [ft3/min] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other Liquid/Gas

| Annual Value [gal] | Minimum Value [gal] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [gal] | Timestamp of Maximum {TIMESTAMP}
None |  |  |  |  |

Values shown are for all completed run periods - including any simulations run during sizing periods
Annual and Peak Values - Other

| Annual Value [kBtu] | Minimum Value [Btu/h] | Timestamp of Minimum {TIMESTAMP} | Maximum Value [Btu/h] | Timestamp of Maximum {TIMESTAMP}
EnergyTransfer:Facility | 133293.94 | 738.87 | 10-JUL-04:40 | 63499.09 | 02-FEB-07:30
EnergyTransfer:Building | 42508.81 | 0.64 | 05-JUN-07:50 | 18382.64 | 02-FEB-07:30
EnergyTransfer:Zone:LIVING_UNIT1 | 42508.81 | 0.64 | 05-JUN-07:50 | 18382.64 | 02-FEB-07:30
Heating:EnergyTransfer | 21784.59 | 0.00 | 21-JUL-00:10 | 18382.64 | 02-FEB-07:30
Heating:EnergyTransfer:Zone:LIVING_UNIT1 | 21784.59 | 0.00 | 21-JUL-00:10 | 18382.64 | 02-FEB-07:30
General:Heating:EnergyTransfer | 21784.59 | 0.00 | 21-JUL-00:10 | 18382.64 | 02-FEB-07:30
General:Heating:EnergyTransfer:Zone:LIVING_UNIT1 | 21784.59 | 0.00 | 21-JUL-00:10 | 18382.64 | 02-FEB-07:30
Cooling:EnergyTransfer | 20724.22 | 0.00 | 21-JAN-00:10 | 15913.28 | 07-SEP-15:30
Cooling:EnergyTransfer:Zone:LIVING_UNIT1 | 20724.22 | 0.00 | 21-JAN-00:10 | 15913.28 | 07-SEP-15:30
General:Cooling:EnergyTransfer | 20724.22 | 0.00 | 21-JAN-00:10 | 15913.28 | 07-SEP-15:30
General:Cooling:EnergyTransfer:Zone:LIVING_UNIT1 | 20724.22 | 0.00 | 21-JAN-00:10 | 15913.28 | 07-SEP-15:30
EnergyTransfer:Zone:GARAGE1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Heating:EnergyTransfer:Zone:GARAGE1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Heating:EnergyTransfer:Zone:GARAGE1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Cooling:EnergyTransfer:Zone:GARAGE1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Cooling:EnergyTransfer:Zone:GARAGE1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
EnergyTransfer:Zone:ATTIC_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Heating:EnergyTransfer:Zone:ATTIC_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Heating:EnergyTransfer:Zone:ATTIC_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Cooling:EnergyTransfer:Zone:ATTIC_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Cooling:EnergyTransfer:Zone:ATTIC_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
EnergyTransfer:Zone:CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Heating:EnergyTransfer:Zone:CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Heating:EnergyTransfer:Zone:CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
Cooling:EnergyTransfer:Zone:CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
General:Cooling:EnergyTransfer:Zone:CRAWLSPACE_UNIT1 | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
PlantLoopHeatingDemand:Facility | 30728.78 | 59.23 | 22-AUG-03:00 | 19854.26 | 02-FEB-07:30
PlantLoopHeatingDemand:Plant | 7102.26 | 59.23 | 22-AUG-03:00 | 1847.88 | 19-FEB-09:00
WaterSystems:PlantLoopHeatingDemand | 7102.26 | 59.23 | 22-AUG-03:00 | 1847.88 | 19-FEB-09:00
General:WaterSystems:PlantLoopHeatingDemand | 7102.26 | 59.23 | 22-AUG-03:00 | 1847.88 | 19-FEB-09:00
EnergyTransfer:HVAC | 60256.14 | 347.62 | 21-OCT-12:10 | 25354.75 | 02-FEB-07:30
HeatRecoveryForHeating:EnergyTransfer | 11846.17 | 0.00 | 21-JUL-08:20 | 7210.13 | 02-FEB-08:00
HeatRecoveryForCooling:EnergyTransfer | 147.31 | 0.00 | 21-JAN-00:10 | 729.78 | 04-AUG-15:00
HeatingCoils:EnergyTransfer | 23631.53 | 0.00 | 21-JUL-00:10 | 18159.23 | 02-FEB-07:30
PlantLoopHeatingDemand:HVAC | 23626.53 | 0.00 | 21-JUL-00:10 | 18159.23 | 02-FEB-07:30
HeatingCoils:PlantLoopHeatingDemand | 23626.53 | 0.00 | 21-JUL-00:10 | 18159.23 | 02-FEB-07:30
CoolingCoils:EnergyTransfer | 24631.13 | 0.00 | 21-JAN-00:10 | 19573.50 | 04-AUG-15:30
EnergyTransfer:Plant | 30528.99 | 59.23 | 22-AUG-03:00 | 19761.70 | 02-FEB-07:30
WaterSystems:EnergyTransfer | 7102.26 | 59.23 | 22-AUG-03:00 | 1847.88 | 19-FEB-09:00
Domestic Hot Water:WaterSystems:EnergyTransfer | 7102.26 | 59.23 | 22-AUG-03:00 | 1847.88 | 19-FEB-09:00
Boilers:EnergyTransfer | 23426.74 | 0.00 | 21-JUL-00:10 | 18066.68 | 02-FEB-07:30
Water Heater:WaterSystems:PlantLoopHeatingDemand | 0.00 | 0.00 | 21-JAN-00:10 | 0.00 | 21-JAN-00:10
FuelOilNo2:Facility | 14020.78 | 0.00 | 21-JAN-00:10 | 12362.66 | 26-FEB-08:10
FuelOilNo2:Plant | 14020.78 | 0.00 | 21-JAN-00:10 | 12362.66 | 26-FEB-08:10
WaterSystems:FuelOilNo2 | 14020.78 | 0.00 | 21-JAN-00:10 | 12362.66 | 26-FEB-08:10
Water Heater:WaterSystems:FuelOilNo2 | 14020.78 | 0.00 | 21-JAN-00:10 | 12362.66 | 26-FEB-08:10

Values shown are for all completed run periods - including any simulations run during sizing periods

Table of Contents

Report: Sensible Heat Gain Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Annual Building Sensible Heat Gain Components

| HVAC Zone Eq & Other Sensible Air Heating [kBtu] | HVAC Zone Eq & Other Sensible Air Cooling [ton-hrs] | HVAC Terminal Unit Sensible Air Heating [kBtu] | HVAC Terminal Unit Sensible Air Cooling [ton-hrs] | HVAC Input Heated Surface Heating [kBtu] | HVAC Input Cooled Surface Cooling [ton-hrs] | People Sensible Heat Addition [kBtu] | Lights Sensible Heat Addition [kBtu] | Equipment Sensible Heat Addition [kBtu] | Window Heat Addition [kBtu] | Interzone Air Transfer Heat Addition [kBtu] | Infiltration Heat Addition [kBtu] | Opaque Surface Conduction and Other Heat Addition [kBtu] | Equipment Sensible Heat Removal [kBtu] | Window Heat Removal [kBtu] | Interzone Air Transfer Heat Removal [kBtu] | Infiltration Heat Removal [kBtu] | Opaque Surface Conduction and Other Heat Removal [kBtu]
LIVING_UNIT1 | 262.124 | -323.53 | 24345.431 | -1651.11 | 0.000 | 0.000 | 4556.457 | 3542.897 | 16883.373 | 17747.196 | 0.000 | 0.000 | 0.000 | 0.000 | -16274.96 | 0.000 | 0.000 | -27351.00
GARAGE1 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000
ATTIC_UNIT1 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000
CRAWLSPACE_UNIT1 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000 | 0.000
Total Facility | 262.124 | -323.53 | 24345.431 | -1651.11 | 0.000 | 0.000 | 4556.457 | 3542.897 | 16883.373 | 17747.196 | 0.000 | 0.000 | 0.000 | 0.000 | -16274.96 | 0.000 | 0.000 | -27351.00

Peak Cooling Sensible Heat Gain Components

| Time of Peak {TIMESTAMP} | HVAC Zone Eq & Other Sensible Air Heating [Btu/h] | HVAC Zone Eq & Other Sensible Air Cooling [ton] | HVAC Terminal Unit Sensible Air Heating [Btu/h] | HVAC Terminal Unit Sensible Air Cooling [ton] | HVAC Input Heated Surface Heating [Btu/h] | HVAC Input Cooled Surface Cooling [ton] | People Sensible Heat Addition [Btu/h] | Lights Sensible Heat Addition [Btu/h] | Equipment Sensible Heat Addition [Btu/h] | Window Heat Addition [Btu/h] | Interzone Air Transfer Heat Addition [Btu/h] | Infiltration Heat Addition [Btu/h] | Opaque Surface Conduction and Other Heat Addition [Btu/h] | Equipment Sensible Heat Removal [Btu/h] | Window Heat Removal [Btu/h] | Interzone Air Transfer Heat Removal [Btu/h] | Infiltration Heat Removal [Btu/h] | Opaque Surface Conduction and Other Heat Removal [Btu/h]
LIVING_UNIT1 | 07-SEP-15:35 | 0.00 | 0.04 | 0.00 | -1.4 | 0.00 | 0.00 | 172.63 | 257.67 | 1809.61 | 11120.35 | 0.00 | 0.00 | 2553.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
GARAGE1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Facility | 07-SEP-15:35 | 0.00 | 0.04 | 0.00 | -1.4 | 0.00 | 0.00 | 172.63 | 257.67 | 1809.61 | 11120.35 | 0.00 | 0.00 | 2553.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

Peak Heating Sensible Heat Gain Components

| Time of Peak {TIMESTAMP} | HVAC Zone Eq & Other Sensible Air Heating [Btu/h] | HVAC Zone Eq & Other Sensible Air Cooling [ton] | HVAC Terminal Unit Sensible Air Heating [Btu/h] | HVAC Terminal Unit Sensible Air Cooling [ton] | HVAC Input Heated Surface Heating [Btu/h] | HVAC Input Cooled Surface Cooling [ton] | People Sensible Heat Addition [Btu/h] | Lights Sensible Heat Addition [Btu/h] | Equipment Sensible Heat Addition [Btu/h] | Window Heat Addition [Btu/h] | Interzone Air Transfer Heat Addition [Btu/h] | Infiltration Heat Addition [Btu/h] | Opaque Surface Conduction and Other Heat Addition [Btu/h] | Equipment Sensible Heat Removal [Btu/h] | Window Heat Removal [Btu/h] | Interzone Air Transfer Heat Removal [Btu/h] | Infiltration Heat Removal [Btu/h] | Opaque Surface Conduction and Other Heat Removal [Btu/h]
LIVING_UNIT1 | 02-FEB-07:30 | -380.3 | 0.00 | 18763.73 | 0.00 | 0.00 | 0.00 | 697.09 | 495.53 | 1983.50 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -9042.6 | 0.00 | 0.00 | -12516.9
GARAGE1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
ATTIC_UNIT1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
CRAWLSPACE_UNIT1 | - | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Total Facility | 02-FEB-07:30 | -380.3 | 0.00 | 18763.73 | 0.00 | 0.00 | 0.00 | 697.09 | 495.53 | 1983.50 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | -9042.6 | 0.00 | 0.00 | -12516.9

Table of Contents

Report: Standard 62.1 Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

System Ventilation Requirements for Cooling

| Sum of Zone Primary Air Flow - Vpz-sum [ft3/min] | System Population - Ps | Sum of Zone Population - Pz-sum | Occupant Diversity - D | Origin of D | Uncorrected Outdoor Air Intake Airflow - Vou [ft3/min] | System Primary Airflow - Vps [ft3/min] | Average Outdoor Air Fraction - Xs | System Ventilation Efficiency - Ev | Calculation Method for Ev | Outdoor Air Intake Flow - Vot [ft3/min] | Percent Outdoor Air - %OA | Environment Name of Peak System Population - Ps | Date and Time of Last Peak System Population - Ps
CENTRAL SYSTEM_UNIT1 | 692.4717 | 0.0000 | 3.0000 | 1.0000 | Calculated from schedules | 0.0000 | 692.4717 | 0.0000 | 1.0000 | Not calculated | 0.0000 | 0.0000 |  |

System Ventilation Requirements for Heating

| Sum of Zone Primary Air Flow - Vpz-sum [ft3/min] | System Population - Ps | Sum of Zone Population - Pz-sum | Occupant Diversity - D | Origin of D | Uncorrected Outdoor Air Intake Airflow - Vou [ft3/min] | System Primary Airflow - Vps [ft3/min] | Average Outdoor Air Fraction - Xs | System Ventilation Efficiency - Ev | Calculation Method for Ev | Outdoor Air Intake Flow Vot [ft3/min] | Percent Outdoor Air - %OA | Environment Name of Peak System Population - Ps | Date and Time of Last Peak System Population - Ps
CENTRAL SYSTEM_UNIT1 | 692.4717 | 0.0000 | 3.0000 | 1.0000 | Calculated from schedules | 0.0000 | 692.4717 | 0.0000 | 1.0000 | Not calculated | 0.0000 | 0.0000 |  |

Zone Ventilation Parameters

| AirLoop Name | People Outdoor Air Rate - Rp [ft3/min-person] | Zone Population - Pz | Area Outdoor Air Rate - Ra [ft3/min-ft2] | Zone Floor Area - Az [ft2] | Breathing Zone Outdoor Airflow - Vbz [ft3/min] | Cooling Zone Air Distribution Effectiveness - Ez-clg | Cooling Zone Outdoor Airflow - Voz-clg [ft3/min] | Heating Zone Air Distribution Effectiveness - Ez-htg | Heating Zone Outdoor Airflow - Voz-htg [ft3/min]
LIVING_UNIT1 | CENTRAL SYSTEM_UNIT1 | 0.000000 | 3.0000 | 0.000000 | 2377.10 | 0.0000 | 1.0000 | 0.0000 | 1.000 | 0.0000

System Ventilation Parameters

| People Outdoor Air Rate - Rp [ft3/min-person] | Sum of Zone Population - Pz-sum | Area Outdoor Air Rate - Ra [ft3/min-ft2] | Sum of Zone Floor Area - Az-sum [ft2] | Breathing Zone Outdoor Airflow - Vbz [ft3/min] | Cooling Zone Outdoor Airflow - Voz-clg [ft3/min] | Heating Zone Outdoor Airflow - Voz-htg [ft3/min]
CENTRAL SYSTEM_UNIT1 | 0.000000 | 3.00 | 0.000000 | 2377.0955 | 0.0000 | 0.0000 | 0.0000

Zone Ventilation Calculations for Cooling Design

| AirLoop Name | Box Type | Zone Primary Airflow - Vpz [ft3/min] | Zone Discharge Airflow - Vdz [ft3/min] | Minimum Zone Primary Airflow - Vpz-min [ft3/min] | Is Vpz-min calculated using the Standard 62.1 Simplified Procedure? | Zone Outdoor Airflow Cooling - Voz-clg [ft3/min] | Primary Outdoor Air Fraction - Zpz | Primary Air Fraction - Ep | Secondary Recirculation Fraction- Er | Supply Air Fraction- Fa | Mixed Air Fraction - Fb | Outdoor Air Fraction - Fc | Zone Ventilation Efficiency - Evz
LIVING_UNIT1 | CENTRAL SYSTEM_UNIT1 | AIRTERMINAL:SINGLEDUCT:CONSTANTVOLUME:NOREHEAT | 692.4717 | 692.4717 | 692.4717 | No | 0.0000 | 0.0000 | 1.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 1.0000

System Ventilation Calculations for Cooling Design

| Sum of Zone Primary Airflow - Vpz-sum [ft3/min] | System Primary Airflow - Vps [ft3/min] | Sum of Zone Discharge Airflow - Vdz-sum [ft3/min] | Sum of Min Zone Primary Airflow - Vpz-min [ft3/min] | Zone Outdoor Airflow Cooling - Voz-clg [ft3/min] | Zone Ventilation Efficiency - Evz-min
CENTRAL SYSTEM_UNIT1 | 692.4717 | 692.4717 | 692.4717 | 692.4717 | 0.0000 | 1.0000

Zone Ventilation Calculations for Heating Design

| AirLoop Name | Box Type | Zone Primary Airflow - Vpz [ft3/min] | Zone Discharge Airflow - Vdz [ft3/min] | Minimum Zone Primary Airflow - Vpz-min [ft3/min] | Is Vpz-min calculated using the Standard 62.1 Simplified Procedure? | Zone Outdoor Airflow Heating - Voz-htg [ft3/min] | Primary Outdoor Air Fraction - Zpz | Primary Air Fraction - Ep | Secondary Recirculation Fraction- Er | Supply Air Fraction- Fa | Mixed Air Fraction - Fb | Outdoor Air Fraction - Fc | Zone Ventilation Efficiency - Evz
LIVING_UNIT1 | CENTRAL SYSTEM_UNIT1 | AIRTERMINAL:SINGLEDUCT:CONSTANTVOLUME:NOREHEAT | 692.4717 | 692.4717 | 692.4717 | No | 0.0000 | 0.0000 | 1.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000 | 1.0000

System Ventilation Calculations for Heating Design

| Sum of Zone Primary Airflow - Vpz-sum [ft3/min] | System Primary Airflow - Vps [ft3/min] | Sum of Zone Discharge Airflow - Vdz-sum [ft3/min] | Sum of Min Zone Primary Airflow - Vpz-min [ft3/min] | Zone Outdoor Airflow Heating - Voz-htg [ft3/min] | Zone Ventilation Efficiency - Evz-min
CENTRAL SYSTEM_UNIT1 | 692.4717 | 692.4717 | 692.4717 | 692.4717 | 0.0000 | 1.0000

Table of Contents

Report: LEED Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Sec1.1A-General Information

| Data
Cooling Degree Days | 2368.8
Heating Degree Days | 8132.4
HDD and CDD data source | Weather File Stat
Climate Zone | 6A
Weather File | ANNUAL ** Rochester International Arpt MN USA TMY3 WMO#=726440
Total gross floor area [ft2] | 5154.23
Principal Heating Source | Natural Gas

EAp2-1. Space Usage Type

| Space Area [ft2] | Regularly Occupied Area [ft2] | Unconditioned Area [ft2] | Typical Hours/Week in Operation [hr/wk]
LIVING_UNIT1 | 2377.10 | 2377.10 | 0.00 | 168.00
GARAGE1 | 400.04 | 0.00 | 400.04 | 0.00
ATTIC_UNIT1 | 1188.55 | 0.00 | 1188.55 | 0.00
CRAWLSPACE_UNIT1 | 1188.55 | 0.00 | 1188.55 | 0.00
Totals | 5154.23 | 2377.10 | 2777.13 |

EAp2-2. Advisory Messages

| Data
Number of hours heating loads not met | 0.00
Number of hours cooling loads not met | 0.00
Number of hours not met | 0.00

EAp2-3. Energy Type Summary

| Utility Rate | Virtual Rate [$/unit energy] | Units of Energy | Units of Demand
None |  |  |  |

EAp2-4/5. Performance Rating Method Compliance

| Electricity Energy Use [kWh] | Electricity Demand [W] | Natural Gas Energy Use [therm] | Natural Gas Demand [Btu/h] | Gasoline Use [therm] | Gasoline Demand [Btu/h] | Diesel Use [kBtu] | Diesel Demand [Btu/h] | Coal Use [kBtu] | Coal Demand [Btu/h] | Fuel Oil No 1 Use [kBtu] | Fuel Oil No 1 Demand [Btu/h] | Fuel Oil No 2 Use [kBtu] | Fuel Oil No 2 Demand [Btu/h] | Propane Use [kBtu] | Propane Demand [Btu/h] | Other Fuel 1 Use [kBtu] | Other Fuel 1 Demand [Btu/h] | Other Fuel 2 Use [kBtu] | Other Fuel 2 Demand [Btu/h] | District Cooling Use [ton-hrs] | District Cooling Demand [ton] | District Heating Water Use [kBtu] | District Heating Water Demand [Btu/h] | District Heating Steam Use [kBtu] | District Heating Steam Demand [Btu/h]
Heating -- General | 0.00 | 0.00 | 230.52 | 18066.68 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heating -- Boiler Parasitic | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Cooling -- General | 1557.96 | 1450.17 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Lighting -- General | 1037.63 | 337.99 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting -- Exterior-Lights | 189.40 | 43.24 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Lighting -- Garage-Lights | 21.99 | 7.16 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- dishwasher | 205.90 | 65.70 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- refrigerator | 668.67 | 91.06 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- clotheswasher | 105.15 | 28.48 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- electric_dryer | 833.27 | 213.06 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- electric_range | 604.09 | 248.15 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- television | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- electric_mels | 3358.05 | 567.46 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Interior Equipment -- IECC_adj | 2017.01 | 340.85 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Exterior Equipment -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans -- Ventilation (simple) | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans -- Ventilation | 876.00 | 100.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Fans -- General | 617.87 | 239.45 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Pumps -- General | 49.62 | 27.47 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Rejection -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Humidification -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Heat Recovery -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems -- Domestic Hot Water | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Water Systems -- Water Heater | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 13944.29 | 12362.66 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Refrigeration -- Not Subdivided | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00
Generators -- General | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.00

EAp2-6. Energy Use Summary

| Process Subtotal [kBtu] | Total Energy Use [kBtu]
Electricity | 26605.68 | 41459.99
Natural Gas | 0.00 | 23051.97
Additional | 0.00 | 13225463.48
Total | 26605.68 | 78456.25

EAp2-7. Energy Cost Summary

| Process Subtotal [$] | Total Energy Cost [$]
Electricity | 0.00 |
Natural Gas | 0.00 |
Additional | 0.00 |
Total | 0.00 |

Process energy cost based on ratio of process to total energy.
L-1. Renewable Energy Source Summary

| Rated Capacity [kW] | Annual Energy Generated [kBtu]
Photovoltaic | 0.00 | 0.00
Wind | 0.00 | 0.00

EAp2-17a. Energy Use Intensity - Electricity

| Electricty [kWh/ft2]
Interior Lighting (All) | 0.20
Space Heating | 0.00
Space Cooling | 0.30
Fans (All) | 0.29
Service Water Heating | 0.00
Receptacle Equipment | 1.51
Miscellaneous (All) | 2.36
Subtotal | 2.36

EAp2-17b. Energy Use Intensity - Natural Gas

| Natural Gas [kBtu/ft2]
Space Heating | 4.47
Service Water Heating | 0.00
Miscellaneous (All) | 4.47
Subtotal | 4.47

EAp2-17c. Energy Use Intensity - Additional

| Additional [kBtu/ft2]
Subtotal | 2.70
Miscellaneous | 2.70

EAp2-18. End Use Percentage

| Percent [%]
Interior Lighting (All) | 4.52
Space Heating | 29.38
Space Cooling | 6.78
Fans (All) | 6.50
Service Water Heating | 17.77
Receptacle Equipment | 33.91
Miscellaneous | 1.14

Schedules-Equivalent Full Load Hours (Schedule Type=Fraction)

| Equivalent Full Load Hours of Operation Per Year [hr] | Hours > 1% [hr]
OCCUPANCY | 6031. | 8760.
INTERIORLIGHTING | 2852. | 8760.
INTERIORLIGHTINGHE | 3070. | 8760.
INTERIORLIGHTINGHE_OS | 2910. | 8760.
INTERIORLIGHTINGHE_VS | 2149. | 8760.
EXTERIORLIGHTING | 4380. | 4380.
REFRIGERATOR | 7343. | 8760.
MISCPLUGLOAD | 5918. | 8760.
COOKINGRANGE | 2434. | 8760.
DISHWASHER_FLOW_SCH | 1777. | 8760.
CLOTHESWASHER_FLOW_SCH | 2094. | 8760.
DISHWASHER_EQUIP_SCH | 3134. | 8760.
CLOTHESWASHER_EQUIP_SCH | 3692. | 8760.
CLOTHESDRYER | 3911. | 8760.
SHADING_2012IECC | 0. | 0.
SHADING_2012IECC_HERS | 7007. | 8760.
SINKSENSSCHEDULE | 6025. | 8760.
SINKLATSCHEDULE | 2735. | 8760.
SHOWERSENSSCHEDULE | 4492. | 8760.
SHOWERLATSCHEDULE | 4268. | 8760.
BATHSENSSCHEDULE | 8760. | 8760.
BATHLATSCHEDULE | 0. | 0.

Schedules-SetPoints (Schedule Type=Temperature)

| First Object Used | Month Assumed | 11am First Wednesday [F] | Days with Same 11am Value | 11pm First Wednesday [F] | Days with Same 11pm Value
HEATING_SCH | THERMOSTAT_LIVING DUAL SP CONTROL | January | 72.00 | 365 | 72.00 | 365
COOLING_SCH | THERMOSTAT_LIVING DUAL SP CONTROL | July | 75.00 | 365 | 75.00 | 365

Table of Contents

Report: Annual CO2 Resilience Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

CO2 Level Hours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

CO2 Level OccupantHours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

CO2 Level OccupiedHours

| Safe (<= 1000 ppm) [hr] | Caution (> 1000, <= 5000 ppm) [hr] | Hazard (> 5000 ppm) [hr]
None |  |  |

Table of Contents

Report: Annual Visual Resilience Summary

For: Entire Facility

Timestamp: 2025-05-15 15:06:31

Illuminance Level Hours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Illuminance Level OccupantHours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Illuminance Level OccupiedHours

| A Bit Dark (<= 100 lux) [hr] | Dim (> 100, <= 300 lux) [hr] | Adequate (> 300, <= 500 lux) [hr] | Bright (>500 lux) [hr]
None |  |  |  |

Table of Contents

Report: FANSPLIT

For: CENTRAL SYSTEM_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| AIR SYSTEM COOLING COIL TOTAL COOLING ENERGY {HOURS NON-ZERO} [HOURS] | AIR SYSTEM FAN ELECTRICITY ENERGY {FOR HOURS SHOWN} [kWh] | AIR SYSTEM HEATING COIL TOTAL HEATING ENERGY {HOURS NON-ZERO} [HOURS] | AIR SYSTEM FAN ELECTRICITY ENERGY {FOR HOURS SHOWN} [kWh] | AIR SYSTEM FAN ELECTRICITY ENERGY [kWh]
January | 0.083 | 0.000 | 730.222 | 75.545 | 75.545
February | 19.917 | 0.607 | 603.194 | 54.151 | 54.758
March | 99.458 | 2.970 | 524.000 | 36.434 | 39.404
April | 266.835 | 17.592 | 319.667 | 18.910 | 36.502
May | 528.616 | 34.716 | 44.667 | 1.621 | 36.338
June | 624.208 | 60.201 | 29.306 | 0.699 | 60.900
July | 722.375 | 72.174 | 0.000 | 0.000 | 72.174
August | 696.933 | 62.632 | 1.000 | 0.011 | 62.643
September | 476.425 | 37.066 | 108.917 | 4.319 | 41.385
October | 185.664 | 7.482 | 331.750 | 16.720 | 24.202
November | 32.919 | 1.193 | 570.958 | 43.486 | 44.678
December | 1.000 | 0.006 | 720.611 | 69.336 | 69.343
Annual Sum or Average | 3654.434 | 296.639 | 3984.292 | 321.233 | 617.872
Minimum of Months | 0.083 | 0.000 | 0.000 | 0.000 | 24.202
Maximum of Months | 722.375 | 72.174 | 730.222 | 75.545 | 75.545

Table of Contents

Report: COILLOADS

For: MAIN DX HEATING COIL_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| HEATING COIL HEATING RATE [Btu/h] | HEATING COIL AIR HEATING RATE [] | COOLING COIL TOTAL COOLING RATE []
January | 8304.58 | 0.00 | 0.00
February | 6108.19 | 0.00 | 0.00
March | 3188.71 | 0.00 | 0.00
April | 1523.22 | 0.00 | 0.00
May | 96.17 | 0.00 | 0.00
June | 31.55 | 0.00 | 0.00
July | 0.00 | 0.00 | 0.00
August | 0.28 | 0.00 | 0.00
September | 281.42 | 0.00 | 0.00
October | 1185.77 | 0.00 | 0.00
November | 4154.70 | 0.00 | 0.00
December | 7128.97 | 0.00 | 0.00
Annual Sum or Average | 2651.49 | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00 | 0.00
Maximum of Months | 8304.58 | 0.00 | 0.00

Table of Contents

Report: COILLOADS

For: SUPP HEATING COIL_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| HEATING COIL HEATING RATE [Btu/h] | HEATING COIL AIR HEATING RATE [] | COOLING COIL TOTAL COOLING RATE []
January | 2.26 | 0.00 | 0.00
February | 1.24 | 0.00 | 0.00
March | 0.50 | 0.00 | 0.00
April | 0.24 | 0.00 | 0.00
May | 0.00 | 0.00 | 0.00
June | 0.00 | 0.00 | 0.00
July | 0.00 | 0.00 | 0.00
August | 0.00 | 0.00 | 0.00
September | 0.03 | 0.00 | 0.00
October | 0.19 | 0.00 | 0.00
November | 0.81 | 0.00 | 0.00
December | 1.57 | 0.00 | 0.00
Annual Sum or Average | 0.57 | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00 | 0.00
Maximum of Months | 2.26 | 0.00 | 0.00

Table of Contents

Report: COILLOADS

For: DX COOLING COIL_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| HEATING COIL HEATING RATE [] | HEATING COIL AIR HEATING RATE [] | COOLING COIL TOTAL COOLING RATE [ton]
January | 0.00 | 0.00 | 0.00
February | 0.00 | 0.00 | 0.01
March | 0.00 | 0.00 | 0.03
April | 0.00 | 0.00 | 0.17
May | 0.00 | 0.00 | 0.32
June | 0.00 | 0.00 | 0.57
July | 0.00 | 0.00 | 0.67
August | 0.00 | 0.00 | 0.58
September | 0.00 | 0.00 | 0.35
October | 0.00 | 0.00 | 0.07
November | 0.00 | 0.00 | 0.01
December | 0.00 | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00 | 0.23
Minimum of Months | 0.00 | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00 | 0.67

Table of Contents

Report: HEATING AND COOLING LOADS

For: LIVING_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| ZONE AIR SYSTEM SENSIBLE COOLING ENERGY [ton-hrs] | ZONE AIR SYSTEM SENSIBLE HEATING ENERGY [kBtu]
January | 0.87 | 5838.18
February | 8.08 | 3831.66
March | 27.70 | 2107.51
April | 115.37 | 954.20
May | 209.34 | 53.57
June | 332.44 | 14.74
July | 387.95 | 0.00
August | 336.13 | 0.02
September | 218.40 | 169.34
October | 58.25 | 757.61
November | 11.84 | 2734.90
December | 1.65 | 4944.10
Annual Sum or Average | 1708.01 | 21405.83
Minimum of Months | 0.87 | 0.00
Maximum of Months | 387.95 | 5838.18

Table of Contents

Report: HEATING AND COOLING LOADS

For: GARAGE1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| ZONE AIR SYSTEM SENSIBLE COOLING ENERGY [ton-hrs] | ZONE AIR SYSTEM SENSIBLE HEATING ENERGY [kBtu]
January | 0.00 | 0.00
February | 0.00 | 0.00
March | 0.00 | 0.00
April | 0.00 | 0.00
May | 0.00 | 0.00
June | 0.00 | 0.00
July | 0.00 | 0.00
August | 0.00 | 0.00
September | 0.00 | 0.00
October | 0.00 | 0.00
November | 0.00 | 0.00
December | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00

Table of Contents

Report: HEATING AND COOLING LOADS

For: ATTIC_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| ZONE AIR SYSTEM SENSIBLE COOLING ENERGY [ton-hrs] | ZONE AIR SYSTEM SENSIBLE HEATING ENERGY [kBtu]
January | 0.00 | 0.00
February | 0.00 | 0.00
March | 0.00 | 0.00
April | 0.00 | 0.00
May | 0.00 | 0.00
June | 0.00 | 0.00
July | 0.00 | 0.00
August | 0.00 | 0.00
September | 0.00 | 0.00
October | 0.00 | 0.00
November | 0.00 | 0.00
December | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00

Table of Contents

Report: HEATING AND COOLING LOADS

For: CRAWLSPACE_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| ZONE AIR SYSTEM SENSIBLE COOLING ENERGY [ton-hrs] | ZONE AIR SYSTEM SENSIBLE HEATING ENERGY [kBtu]
January | 0.00 | 0.00
February | 0.00 | 0.00
March | 0.00 | 0.00
April | 0.00 | 0.00
May | 0.00 | 0.00
June | 0.00 | 0.00
July | 0.00 | 0.00
August | 0.00 | 0.00
September | 0.00 | 0.00
October | 0.00 | 0.00
November | 0.00 | 0.00
December | 0.00 | 0.00
Annual Sum or Average | 0.00 | 0.00
Minimum of Months | 0.00 | 0.00
Maximum of Months | 0.00 | 0.00

Table of Contents

Report: WATER HEATER: LOADS

For: WATER HEATER_UNIT1

Timestamp: 2025-05-15 15:06:31

Custom Monthly Report

| WATER HEATER TOTAL DEMAND RATE [] | WATER HEATER TOTAL DEMAND ENERGY [] | WATER HEATER HEATING RATE [Btu/h] | WATER HEATER HEATING ENERGY [kBtu]
January | 0.00 | 0.00 | 1424.55 | 1060.61
February | 0.00 | 0.00 | 1451.30 | 975.97
March | 0.00 | 0.00 | 1433.54 | 1067.31
April | 0.00 | 0.00 | 1373.39 | 989.54
May | 0.00 | 0.00 | 1277.44 | 951.09
June | 0.00 | 0.00 | 1189.25 | 856.87
July | 0.00 | 0.00 | 1122.57 | 835.78
August | 0.00 | 0.00 | 1091.20 | 812.43
September | 0.00 | 0.00 | 1113.11 | 802.00
October | 0.00 | 0.00 | 1178.27 | 877.25
November | 0.00 | 0.00 | 1270.00 | 915.05
December | 0.00 | 0.00 | 1358.62 | 1011.53
Annual Sum or Average | 0.00 | 0.00 | 1272.55 | 11155.43
Minimum of Months | 0.00 | 0.00 | 1091.20 | 802.00
Maximum of Months | 0.00 | 0.00 | 1451.30 | 1067.31